<?xml version="1.0" encoding="UTF-8"?>

<!DOCTYPE MgmtTree PUBLIC "-//OMA//DTD-DM-DDF 1.2//EN"
	"http://www.openmobilealliance.org/tech/DTD/DM_DDF-V1_2.dtd"
	[<?oma-dm-ddf-ver supported-versions="1.2"?>]>

<!--

	FILE INFORMATION

	Description
		BCAST enabler - OMA BCAST Management Object according to the
		OMA DM Description Framework

	Version: 1.1
	Date:    10 Nov 2009

	OMA Permanent Document
		File: OMA-SUP-MO_oma_bcast-V1_1-20091110-D.ddf
		Type: Text - XML

	Public Reachable Information
		Path: http://www.openmobilealliance.org/tech/omna/dm-mo/
		Name: oma_bcast-v1_1.ddf

	NORMATIVE INFORMATION

	Information about this file can be found in the latest revision of
	the specification OMA-TS-BCAST_Services-V1_1 available at
		http://www.openmobilealliance.org/

	Send comments to technical-comments@mail.openmobilealliance.org

	LEGAL DISCLAIMER

	Use of this document is subject to all of the terms and conditions
	of the Use Agreement located at
		http://www.openmobilealliance.org/UseAgreement.html

	You may use this document or any part of the document for internal
	or educational purposes only, provided you do not modify, edit or
	take out of context the information in this document in any manner.
	Information contained in this document may be used, at your sole
	risk, for any purposes.

	You may not use this document in any other manner without the prior
	written permission of the Open Mobile Alliance.  The Open Mobile
	Alliance authorizes you to copy this document, provided that you
	retain all copyright and other proprietary notices contained in the
	original materials on any copies of the materials and that you
	comply strictly with these terms.  This copyright permission does
	not constitute an endorsement of the products or services.  The
	Open Mobile Alliance assumes no responsibility for errors or
	omissions in this document.

	Each Open Mobile Alliance member has agreed to use reasonable
	endeavors to inform the Open Mobile Alliance in a timely manner of
	Essential IPR as it becomes aware that the Essential IPR is related
	to the prepared or published specification.  However, the members
	do not have an obligation to conduct IPR searches.  The declared
	Essential IPR is publicly available to members and non-members of
	the Open Mobile Alliance and may be found on the "OMA IPR
	Declarations" list at http://www.openmobilealliance.org/ipr.html.
	The Open Mobile Alliance has not conducted an independent IPR review
	of this document and the information contained herein, and makes no
	representations or warranties regarding third party IPR, including
	without limitation patents, copyrights or trade secret rights.  This
	document may contain inventions for which you must obtain licenses
	from third parties before making, using or selling the inventions.
	Defined terms above are set forth in the schedule to the Open Mobile
	Alliance Application Form.

	NO REPRESENTATIONS OR WARRANTIES (WHETHER EXPRESS OR IMPLIED) ARE
	MADE BY THE OPEN MOBILE ALLIANCE OR ANY OPEN MOBILE ALLIANCE MEMBER
	OR ITS AFFILIATES REGARDING ANY OF THE IPR'S REPRESENTED ON THE "OMA
	IPR DECLARATIONS" LIST, INCLUDING, BUT NOT LIMITED TO THE ACCURACY,
	COMPLETENESS, VALIDITY OR RELEVANCE OF THE INFORMATION OR WHETHER OR
	NOT SUCH RIGHTS ARE ESSENTIAL OR NON-ESSENTIAL.

	THE OPEN MOBILE ALLIANCE IS NOT LIABLE FOR AND HEREBY DISCLAIMS ANY
	DIRECT, INDIRECT, PUNITIVE, SPECIAL, INCIDENTAL, CONSEQUENTIAL, OR
	EXEMPLARY DAMAGES ARISING OUT OF OR IN CONNECTION WITH THE USE OF
	DOCUMENTS AND THE INFORMATION CONTAINED IN THE DOCUMENTS.

	Copyright 2009 Open Mobile Alliance Ltd.  All Rights Reserved.
	Used with the permission of the Open Mobile Alliance Ltd. under the
	terms set forth above.
-->
<!--
	CHANGE HISTORY

	20090701	* File created from OMA-SUP-MO_oma_bcast-V1_0-20090212-A.ddf:
				  - embedded file information header aligned with
					 http://member.openmobilealliance.org/ftp/rel/gen_info/Procs/SupportFiles_XSD-v1_0.shtml
				* Leading spaces converted to TABs
				* Name of nodes (comments) moved up one line to ease DDF readibility in "block-folding" capable XML editors
				* Alignment with OMA-TS-BCAST_Services-V1_1-20090416-D,
				  following CRs implemented:
				  - OMA-BCAST-v1_1-2008-0029R06-CR_Service_provider_roaming_enabling
				  - OMA-BCAST-v1_1-2009-0020-CR_Services_DVBSH_BDS_and_BCASTMO_BDSEntryPoint

	20091001	* Alignment with OMA-TS-BCAST_Services-V1_1-20090914-D,
				  following CRs implemented:
				  - OMA-BCAST-v1_1-2009-0182-CR_Services_Correction_on_BCAST_MO

	20091027	* Alignment with OMA-TS-BCAST_Services-V1_1-20091015-D,
				  following CRs implemented:
				  - OMA-BCAST-v1_1-2009-0184R06-CR_Smartcard_Broadcast_Provisioning_Services
				* Alignment with OMA-TS-BCAST_Services-V1_1-20091027-D,
				  following CRs implemented:
				  - OMA-BCAST-v1_1-2009-0195-CR_FLO_Management_Objects

	20091110	* Update of BCAST MO URN minor version (from 1.0 to 1.1)

-->

<MgmtTree>
	<VerDTD>1.2</VerDTD>
	<Node> <!-- X -->
		<NodeName/>
		<!-- Status: Required -->
		<DFProperties>
			<AccessType>
				<Get/>
			</AccessType>
			<DFFormat>
				<node/>
			</DFFormat>
			<Occurrence>
				<ZeroOrMore/>
			</Occurrence>
			<DFTitle>This interior node acts as a placeholder for one or more BCAST Management Object
				root nodes. It is MANDATORY if the UE supports OMA BCAST.</DFTitle>
			<DFType>
				<DDFName>urn:oma:mo:oma_bcast:1.1</DDFName>
			</DFType>
		</DFProperties>
		<Node> <!-- X / BCASTRelease -->
			<NodeName>BCASTRelease</NodeName>
			<!-- Status: Required -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<chr/>
				</DFFormat>
				<Occurrence>
					<One/>
				</Occurrence>
				<DFTitle>This leaf node specifies the BCAST release of the client. It is MANDATORY and
					MUST have the value "1.0" for this release.</DFTitle>
				<DFType>
					<MIME>text/plain</MIME>
				</DFType>
			</DFProperties>
		</Node>
		<Node> <!-- X / BCASTClientID -->
			<NodeName>BCASTClientID</NodeName>
			<!-- Status: Optional -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<chr/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This leaf node contains the BCAST_Client_ID used by the Smartcard Profile as
					per OMA-TS-BCAST-SvcCntProtection-V1_0</DFTitle>
				<DFType>
					<MIME>text/plain</MIME>
				</DFType>
			</DFProperties>
		</Node>
		<Node> <!-- X / HomeBDSEntryPoint -->
			<NodeName>HomeBDSEntryPoint</NodeName>
			<!-- Status: Optional -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<chr/>
				</DFFormat>
				<DFTitle>This leaf node contains the URL referencing the BDSEntryPoint/[X] node that is
					associated to the Home Mobile Broadcast Service Provider.</DFTitle>
				<DFType>
					<MIME>text/plain</MIME>
				</DFType>
			</DFProperties>
		</Node>
		<Node> <!-- X / ServiceProviders -->
			<NodeName>ServiceProviders</NodeName>
			<!-- Status: Required -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node acts as a container for a list of Service Provider identifiers.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!--  X / ServiceProviders / X -->
				<NodeName/>
				<!-- Status: Required -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrMore/>
					</Occurrence>
					<DFTitle>This interior node acts as a placeholder for a list of Service Provider identifiers.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!--  X / ServiceProviders / X / ID -->
					<NodeName>ID</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<chr/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies the Service Provider identifier for the BCAST Service
							(URI).</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / SGServerAddress -->
			<NodeName>SGServerAddress</NodeName>
			<!-- Status: Required -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node contains information about BCAST Service Guide Servers for
					the interactive mode.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!--  X / SGServerAddress / X -->
				<NodeName/>
				<!-- Status: Required -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrMore/>
					</Occurrence>
					<DFTitle>This interior node serves as a placeholder for a list of addresses of BCAST
						Service Guide Servers for the interactive mode.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!-- X / SGServerAddress / X / URL -->
					<NodeName>URL</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<chr/>
						</DFFormat>
						<Occurrence>
							<One/>
						</Occurrence>
						<DFTitle>This leaf node specifies the BCAST Service Guide server URL for the
							interactive mode.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / BDSEntryPoint -->
			<NodeName>BDSEntryPoint</NodeName>
			<!-- Status: Optional -->
			<!--
				It is RECOMMENDED to also include Add, Delete and Replace access types on the implementations,
				in order to support write access on the sub-nodes to provision the necessary sets of information.
			-->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node contains information about the service entry points in the
					different BDSs.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!-- X / BDSEntryPoint / X -->
				<NodeName/>
				<!-- Status: Optional -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrMore/>
					</Occurrence>
					<DFTitle>This interior node acts as a placeholder for sets of BDS-specific
						information.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!-- X / BDSEntryPoint / X / IPDC -->
					<NodeName>IPDC</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This node acts as a container for all the BDS-specific information
							regarding IPDC over DVB-H.</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BDSEntryPoint / X / IPDC / X -->
						<NodeName/>
						<!-- Status: Optional -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node serves as a placeholder for a list of IPDC network tuning parameters.</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BDSEntryPoint / X / IPDC / X / Tuning -->
							<NodeName>Tuning</NodeName>
							<!-- Status: Optional -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains tuning parameters for the DVB-H receiver</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / IPDC / X / Tuning / X -->
								<NodeName/>
								<!-- Status: Optional -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<node/>
									</DFFormat>
									<Occurrence>
										<ZeroOrMore/>
									</Occurrence>
									<DFTitle>This interior node serves as a placeholder for a list of tuning frequencies for the IPDC network.</DFTitle>
									<DFType>
										<DDFName/>
									</DFType>
								</DFProperties>
								<Node> <!-- X / BDSEntryPoint / X / IPDC / X / Tuning / X / Frequency -->
									<NodeName>Frequency</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<int/>
										</DFFormat>
										<Occurrence>
											<One/>
										</Occurrence>
										<DFTitle>This leaf node carries the center frequency of the DVB-H channel
											to tune to, represented in kHz by a decimal number.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / IPDC / X / Tuning / X / UseLPChannel -->
									<NodeName>UseLPChannel </NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<bool/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node provides the information which is needed to tune to
											a hierarchically modulated DVB-H channel.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC / X / IPPlatformID -->
							<NodeName>IPPlatformID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node provides the DVB IP Platform ID according to [ETSI TS
									102 470]. Contains a decimal number representing a 24 bit unsigned integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC / X / DVBNetworkID -->
							<NodeName>DVBNetworkID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This leaf node provides the network ID to scope the IP platform ID
									when not globally unique. Contains a decimal number representing a 16 bit
									unsigned integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC / X / ESGProviderID -->
							<NodeName>ESGProviderID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node provides the Service Guide Provider ID for SG
									bootstrapping. Contains a decimal number representing a 16 bit unsigned
									integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / BDSEntryPoint / X / MBMS -->
					<NodeName>MBMS</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This interior node acts as a container for all the BDS-specific
							information regarding MBMS.</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BDSEntryPoint / X / MBMS / X -->
						<NodeName/>
						<!-- Status: Optional -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node serves as a placeholder for a list of MBMS Bearer Services</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG -->
							<NodeName>SG</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains bootstrap parameters for SG reception
									over MBMS broadcast bearer or SG retrieval over MBMS unicast bearer.</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X -->
								<NodeName/>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<node/>
									</DFFormat>
									<Occurrence>
										<ZeroOrMore/>
									</Occurrence>
									<DFTitle>This interior node acts as a placeholder a set of bootstrap
										parameters for SG reception over MBMS broadcast bearer or SG retrieval
										over MBMS unicast bearer.</DFTitle>
									<DFType>
										<DDFName/>
									</DFType>
								</DFProperties>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / IPSourceAddress -->
									<NodeName>IPSourceAddress</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node contains the IP Source Address of the SG
											delivery session for a broadcasted SG.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / IPMulticastAddress -->
									<NodeName>IPMulticastAddress</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node contains the IP Multicast Address of the SG
											delivery session for a broadcasted SG.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / Port -->
									<NodeName>Port</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<int/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node contains the port number for a broadcasted SG,
											as a decimal number representing a 16 bit unsigned integer.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / BCBearer -->
									<NodeName>BCBearer</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<node/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This interior node acts as a placeholder for sets of MBMS bearer parameter used for reception of a broadcasted SG.</DFTitle>
										<DFType>
											<DDFName/>
										</DFType>
									</DFProperties>
									<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / BCBearer / TMGI -->
										<NodeName>TMGI</NodeName>
										<!-- Status: Required -->
										<DFProperties>
											<AccessType>
												<Get/>
											</AccessType>
											<DFFormat>
												<chr/>
											</DFFormat>
											<Occurrence>
												<ZeroOrOne/>
											</Occurrence>
											<DFTitle>This leaf node contains the Temporary Mobile Group Identity
												(TMGI) for a broadcasted SG as defined in [3GPP TS 24.008]. </DFTitle>
											<DFType>
												<MIME>text/plain</MIME>
											</DFType>
										</DFProperties>
									</Node>
									<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / BCBearer / IsCounting -->
										<NodeName>IsCounting</NodeName>
										<!-- Status: Required -->
										<DFProperties>
											<AccessType>
												<Get/>
											</AccessType>
											<DFFormat>
												<bool/>
											</DFFormat>
											<Occurrence>
												<One/>
											</Occurrence>
											<DFTitle>This leaf node contains the information element MBMS Counting Information as defined in [3GPP TS 25.413].
												It indicates whether the RAN level counting procedures is applicable or not for the MBMS broadcast mode.</DFTitle>
											<DFType>
												<MIME>text/plain</MIME>
											</DFType>
										</DFProperties>
									</Node>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / URLs -->
									<NodeName>URLs</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<node/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This intermediate node contains a list of URLs where an SDP describing the
											delivery session of a broadcasted SG can be fetched.</DFTitle>
										<DFType>
											<DDFName/>
										</DFType>
									</DFProperties>
									<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / URLs / X -->
										<NodeName/>
										<!-- Status: Required -->
										<DFProperties>
											<AccessType>
												<Get/>
											</AccessType>
											<DFFormat>
												<node/>
											</DFFormat>
											<Occurrence>
												<ZeroOrMore/>
											</Occurrence>
											<DFTitle>This intermediate node acts as a placeholder for a list of URLs where an SDP describing the
												delivery session of a broadcasted SG can be fetched.</DFTitle>
											<DFType>
												<DDFName/>
											</DFType>
										</DFProperties>
										<Node> <!-- X / BDSEntryPoint / X / MBMS / X / SG / X / URLs / X / URL -->
											<NodeName>URL</NodeName>
											<!-- Status: Required -->
											<DFProperties>
												<AccessType>
													<Get/>
												</AccessType>
												<DFFormat>
													<chr/>
												</DFFormat>
												<Occurrence>
													<One/>
												</Occurrence>
												<DFTitle>This leaf node contains the URL where an SDP describing the
													delivery session of a broadcasted SG can be fetched.</DFTitle>
												<DFType>
													<MIME>text/plain</MIME>
												</DFType>
											</DFProperties>
										</Node>
									</Node>
								</Node>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / MBMS / X / APNs -->
							<NodeName>APNs</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains a list of URIs of usable MBMS Access Point Names
									(APN).</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / MBMS / X / APNs / X -->
								<NodeName/>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<node/>
									</DFFormat>
									<Occurrence>
										<ZeroOrMore/>
									</Occurrence>
									<DFTitle>This interior node acts as a placeholder for a list of URIs of usable MBMS Access Point Names
										(APN).</DFTitle>
									<DFType>
										<DDFName/>
									</DFType>
								</DFProperties>
								<Node> <!-- X / BDSEntryPoint / X / MBMS / X / APNs / X / APN -->
									<NodeName>APN</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<Occurrence>
											<One/>
										</Occurrence>
										<DFTitle>This leaf node contains the URI of a usable MBMS Access Point Name
											(APN).</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / MBMS / X / NotificationBCBearer -->
							<NodeName>NotificationBCBearer</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node acts as a placeholder for sets of MBMS bearer parameter used for reception of a broadcasted SG.</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / MBMS / X / NotificationBCBearer / TMGI -->
								<NodeName>TMGI</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<chr/>
									</DFFormat>
									<Occurrence>
										<ZeroOrOne/>
									</Occurrence>
									<DFTitle>This leaf node contains the Temporary Mobile Group Identity
										(TMGI) for a broadcasted SG as defined in [3GPP TS 24.008]. </DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / MBMS / X / NotificationBCBearer / IsCounting -->
								<NodeName>IsCounting</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<bool/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the information element MBMS Counting Information as defined in [3GPP TS 25.413].
										It indicates whether the RAN level counting procedures is applicable or not for the MBMS broadcast mode.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / BDSEntryPoint / X / BCMCS  -->
					<NodeName>BCMCS</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This interior node acts as a placeholder for all the BDS-specific information regarding BCMCS.</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BDSEntryPoint / X / BCMCS / X -->
						<NodeName/>
						<!-- Status: Required -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node acts as a placeholder for a list of Networks recognized by the terminal. </DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / NetworkID  -->
							<NodeName>NetworkID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<chr/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node contains network region identification information for BCMCS.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ControllerIPAddress -->
							<NodeName>ControllerIPAddress</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<chr/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node contains the IP address of the BCMCS Controller, saving DHCP bootstrap time.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / SGMulticastAddress -->
							<NodeName>SGMulticastAddress</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<chr/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node contains a string in the form of  "Hostname/Address:Port>".</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ROHCU -->
							<NodeName>ROHCU</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains ROHC Unidirectional (ROHC-U) parameters for BCMCS IP multicast communication.
									If the node is not present, compression is not enabled.</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ROHCU / MaxCID -->
								<NodeName>MaxCID</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node indicates the maximum number of CIDs used by ROHC-U</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ROHCU / LargeCIDs -->
								<NodeName>LargeCIDs</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<bool/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node is true when large CIDs (1 or 2 bytes) are used, otherwise it is false and small CIDs (0 or 1) are used</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ROHCU / MaxHeaderSize -->
								<NodeName>MaxHeaderSize</NodeName>
								<!-- Status: Required Optional -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the maximum header size, in octets, that can be compressed</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / BCMCS / X / ROHCU / MRRU -->
								<NodeName>MRRU</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the size of the Maximum Reconstructed Reception Unit,
										in octets, that the decompressor is expected to reassemble from segments. </DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / BDSEntryPoint / X / IPDC-SH -->
					<NodeName>IPDC-SH</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This node acts as a container for all the BDS-specific information regarding IPDC over DVB-SH</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X -->
						<NodeName/>
						<!-- Status: Required -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node serves as a placeholder for a list of DVB-SH IPDC network tuning parameters.</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning -->
							<NodeName>Tuning</NodeName>
							<!-- Status: Optional -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains tuning parameters for the DVB-SH receiver</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning / Frequency -->
								<NodeName>Frequency</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node carries the center frequency of the primary DVB-SH signal to tune to,
										represented in kHz by a decimal number.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning / UseLPChannel -->
								<NodeName>UseLPChannel </NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<bool/>
									</DFFormat>
									<Occurrence>
										<ZeroOrOne/>
									</Occurrence>
									<DFTitle>This leaf node provides the information which is needed to tune to
										a hierarchically modulated DVB-SH primary channel.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning / Complementary -->
								<NodeName>Complementary</NodeName>
								<!-- Status: Optional -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<node/>
									</DFFormat>
									<Occurrence>
										<ZeroOrOne/>
									</Occurrence>
									<DFTitle>This interior node contains parameters for the DVB-SH receiver
										to tune to the complementary terrestrial DVB-SH signal</DFTitle>
									<DFType>
										<DDFName/>
									</DFType>
								</DFProperties>
								<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning / Complementary / HybridFrequency -->
									<NodeName>HybridFrequency</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<int/>
										</DFFormat>
										<Occurrence>
											<One/>
										</Occurrence>
										<DFTitle>This leaf node carries the center frequency of the complementary
											terrestrial DVB-SH signal to tune to (hybrid frequency)</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / Tuning / Complementary / UseLPChannel -->
									<NodeName>UseLPChannel </NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<bool/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node provides the information which is needed to tune to
											a hierarchically modulated DVB-SH channel.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / IPPlatformID -->
							<NodeName>IPPlatformID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node provides the DVB IP Platform ID according to [ETSI TS
									102 470]. Contains a decimal number representing a 24 bit unsigned integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / DVBNetworkID -->
							<NodeName>DVBNetworkID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This leaf node provides the network ID to scope the IP platform ID
									when not globally unique. Contains a decimal number representing a 16 bit
									unsigned integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / IPDC-SH / X / ESGProviderID -->
							<NodeName>ESGProviderID</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This leaf node provides the Service Guide Provider ID for SG
									bootstrapping. Contains a decimal number representing a 16 bit unsigned
									integer.</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / BDSEntryPoint / X / FLO -->
					<NodeName>FLO</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This interior node acts as a placeholder for all the BDS-specific
							information regarding Forward Link Only.</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BDSEntryPoint / X / FLO / X -->
						<NodeName/>
						<!-- Status: Optional -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node acts as a placeholder for a list of Networks
								recognized by the terminal.</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BDSEntryPoint / X / FLO / X / Tuning -->
							<NodeName>Tuning</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This interior node contains information needed to tune the Forward Link Only
									receiver to the right frequency to receive Forward Link Only broadcasts.</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / Tuning / Priority -->
								<NodeName>Priority</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains a priority (lower values signal
										higher priority) that is used to select the proper frequency for tuning,
										when two or more frequencies are available.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / Tuning / Frequency -->
								<NodeName>Frequency</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node carries the bandwidth of the Forward Link Only transmission system.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / Tuning / Bandwidth -->
								<NodeName>Bandwidth </NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node carries the bandwidth of the Forward Link Only
										transmission system.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / FLO / X / ROHCU -->
							<NodeName>ROHCU</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node contains ROHC Unidirectional (ROHC-U) parameters
									for Forward Link Only IP multicast communication.</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / ROHCU / MaxCID -->
								<NodeName>MaxCID</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node indicates the maximum number of CIDs used by ROHC-U</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / ROHCU / LargeCIDs -->
								<NodeName>/LargeCIDs</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<bool/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node is true when large CIDs (1 or 2 bytes) are used.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / ROHCU / MaxHeaderSize -->
								<NodeName>MaxHeaderSize</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the maximum header size, in octets, that can be compressed.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / ROHCU / MRRU -->
								<NodeName>MRRU</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<int/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the size of the Maximum Reconstructed Reception Unit
										 that the decompressor is expected to reassemble from segments</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
						</Node>
						<Node> <!-- X / BDSEntryPoint / X / FLO / X / SG -->
							<NodeName>SG</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<One/>
								</Occurrence>
								<DFTitle>This interior node contains information that allows the Terminal
									to tune to the proper IP address and port to receive the broadcasted service guide</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / BDSEntryPoint / X / FLO / X / SG / IPSourceAddress -->
								<NodeName>IPSourceAddress</NodeName>
								<!-- Status: Required -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<chr/>
									</DFFormat>
									<Occurrence>
										<One/>
									</Occurrence>
									<DFTitle>This leaf node contains the IP address of the BSD/A that broadcasts
										the service guide.</DFTitle>
									<DFType>
										<MIME>text/plain</MIME>
									</DFType>
								</DFProperties>
							</Node>
								<Node> <!-- X / BDSEntryPoint / X / FLO / X / SG / IPMulticastAddress -->
									<NodeName>IPMulticastAddress</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<Occurrence>
											<One/>
										</Occurrence>
										<DFTitle>This leaf node contains the IP address used for multicast
											delivery of the service guide.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / BDSEntryPoint / X / FLO / X / SG / IPMulticastPort -->
									<NodeName>IPMulticastPort</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<int/>
										</DFFormat>
										<Occurrence>
											<One/>
										</Occurrence>
										<DFTitle>This leaf node contains the IP port used for multicast
											delivery of the service guide.</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
						</Node>
					</Node>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / BSMSelector -->
			<NodeName>BSMSelector </NodeName>
			<!-- Status: Required -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node contains information about the BSMSelector structures
					associated with the BSM of the Home or Roaming Broadcast Service Provider.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!-- X / BSMSelector / X -->
				<NodeName/>
				<!-- Status: Required -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrMore/>
					</Occurrence>
					<DFTitle>This interior node acts as a placeholder for a set of BSMSelector
						information.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!-- X / BSMSelector / X / Name -->
					<NodeName>Name</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<chr/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies a user readable name of the BSMFilterCode.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / BSMSelector / X / BSMFilterCode -->
					<NodeName>BSMFilterCode</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<xml/>
						</DFFormat>
						<Occurrence>
							<One/>
						</Occurrence>
						<DFTitle>This leaf node specifies the value of the BSMFilterCode associated with
							the BSM. The value is a BSMFilterCode XML structure as defined in
							OMA-TS-BCAST_ServiceGuide-V1_0 section 5.4.1.5.2.</DFTitle>
						<DFType>
							<MIME>text/xml</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / BSMSelector / X / IsHomeBSM -->
					<NodeName>IsHomeBSM</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DefaultValue>false</DefaultValue>
						<DFFormat>
							<bool/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies whether the BSM that is associated with the
							BSMSelector belongs to the Home Broadcast Service Provider of the user.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / BSMSelector / X / HomeServiceProvisioningRequestAddress -->
					<NodeName>HomeServiceProvisioningRequestAddress</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<chr/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies the address (URL) of the BSM the terminal can use to issue Service Provisioning requests.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / BSMSelector / X / RoamingRules -->
					<NodeName>RoamingRules</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This interior node contains a list of RoamingRule structures associated with the BSMSelector.</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / BSMSelector / X / RoamingRules / X -->
						<NodeName/>
						<!-- Status: Required -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node cts as a placeholder for a list of RoamingRule structures associated with the BSMSelector.</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / BSMSelector / X / RoamingRules / X / Rule -->
							<NodeName>Rule</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<xml/>
								</DFFormat>
								<Occurrence>
									<ZeroOrMore/>
								</Occurrence>
								<DFTitle>This leaf node contains the RoamingRule given as a RoamingRule XML structure as defined in
									section 5.4.1.5.2 of OMA-TS-BCAST_ServiceGuide-V1_0.</DFTitle>
								<DFType>
									<MIME>text/xml</MIME>
								</DFType>
							</DFProperties>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / BSMSelector / X / RoamingPriority -->
					<NodeName>RoamingPriority</NodeName>
					<!-- Status: Optional -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<int/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies the priority of the BSM in case of roaming the BCAST service.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / Roaming -->
			<NodeName>Roaming</NodeName>
			<!-- Status: Optional-->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node is a container for Roaming structures.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!-- >X / Roaming / X -->
				<NodeName/>
				<!-- Status: Optional -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrMore/>
					</Occurrence>
					<DFTitle>This interior node is a placeholder for a list of Roaming structures.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders -->
					<NodeName>VisitedMobileBroadcastServiceProviders</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<node/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This interior node is a container for providing information about the preferred
							Visited Mobile Broadcast Service Provider for the BCAST service in a roaming scenario</DFTitle>
						<DFType>
							<DDFName/>
						</DFType>
					</DFProperties>
					<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X -->
						<NodeName/>
						<!-- Status: Required -->
						<DFProperties>
							<AccessType>
								<Get/>
							</AccessType>
							<DFFormat>
								<node/>
							</DFFormat>
							<Occurrence>
								<ZeroOrMore/>
							</Occurrence>
							<DFTitle>This interior node contains the references to the network entry points of the Visited
								Mobile Broadcast Service Provider and the priority of this Visited Mobile Broadcast Service Provider.</DFTitle>
							<DFType>
								<DDFName/>
							</DFType>
						</DFProperties>
						<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / Priority -->
							<NodeName>Priority</NodeName>
							<!-- Status: Required -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<int/>
								</DFFormat>
								<DFTitle>This leaf node specifies the priority of this Visited Mobile Broadcast Service Provider
									for consuming the BCAST service in a roaming situation</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / BDSEntryPoint -->
							<NodeName>BDSEntryPoint</NodeName>
							<!-- Status: Optional -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<chr/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This leaf node contains the reference to the BDSEntryPoint/[X] node under the BCAST MO
									of the Visited Mobile Broadcast Service Provider</DFTitle>
								<DFType>
									<MIME>text/plain</MIME>
								</DFType>
							</DFProperties>
						</Node>
						<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / NetworkAccessPoints -->
							<NodeName>NetworkAccessPoints</NodeName>
							<!-- Status: Optional -->
							<DFProperties>
								<AccessType>
									<Get/>
								</AccessType>
								<DFFormat>
									<node/>
								</DFFormat>
								<Occurrence>
									<ZeroOrOne/>
								</Occurrence>
								<DFTitle>This interior node is a container for the unicast Network Access Points
									for roaming the BCAST service</DFTitle>
								<DFType>
									<DDFName/>
								</DFType>
							</DFProperties>
							<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / NetworkAccessPoints / X -->
								<NodeName/>
								<!-- Status: Optional -->
								<DFProperties>
									<AccessType>
										<Get/>
									</AccessType>
									<DFFormat>
										<node/>
									</DFFormat>
									<Occurrence>
										<ZeroOrMore/>
									</Occurrence>
									<DFTitle>This interior node is a placeholder for a list of references to unicast
										Network Access Points and Proxies for roaming the BCAST service.</DFTitle>
									<DFType>
										<DDFName/>
									</DFType>
								</DFProperties>
								<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / NetworkAccessPoints / X / NAP -->
									<NodeName>NAP</NodeName>
									<!-- Status: Required -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<DFTitle>This leaf node references the id of a Network Access Points MO as defined in [CONNMO].</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
								<Node> <!-- X / Roaming / X / VisitedMobileBroadcastServiceProviders / X / NetworkAccessPoints / X / Proxy -->
									<NodeName>Proxy</NodeName>
									<!-- Status: Optional -->
									<DFProperties>
										<AccessType>
											<Get/>
										</AccessType>
										<DFFormat>
											<chr/>
										</DFFormat>
										<Occurrence>
											<ZeroOrOne/>
										</Occurrence>
										<DFTitle>This leaf node references the id of a Proxy MO as defined in [CONNMO].</DFTitle>
										<DFType>
											<MIME>text/plain</MIME>
										</DFType>
									</DFProperties>
								</Node>
							</Node>
						</Node>
					</Node>
				</Node>
				<Node> <!-- X / Roaming / X / HomeRoamingRuleRequestAddress -->
					<NodeName>HomeRoamingRuleRequestAddress</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<chr/>
						</DFFormat>
						<Occurrence>
							<One/>
						</Occurrence>
						<DFTitle>This leaf node specifies the URL of the default Server to which the
							terminal can send RoamingRule Requests related to the BSMSelector in case no
							other contact points are signalled.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / Roaming / X / ForceHomeRoamingRuleRequestAddress -->
					<NodeName>ForceHomeRoamingRuleRequestAddress</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DefaultValue>true</DefaultValue>
						<DFFormat>
							<bool/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies whether the Terminal SHALL override any other
							RoamingRuleRequestAddresses and always contact the address represented by
							HomeRoamingRuleRequestAddress.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / Roaming / X / IgnoreUnIdentifiedBSM -->
					<NodeName>IgnoreUnIdentifiedBSM</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<bool/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies whether Terminal SHALL ignore fragments that
							are not associated with BSMSelector(s).</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
				<Node> <!-- X / Roaming / X / UseVisitedServiceProvisioningMode -->
					<NodeName>UseVisitedServiceProvisioningMode</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DefaultValue>true</DefaultValue>
						<DFFormat>
							<bool/>
						</DFFormat>
						<Occurrence>
							<ZeroOrOne/>
						</Occurrence>
						<DFTitle>This leaf node specifies whether Terminal SHALL initiate the service
							provisioning requests through Visited BSM or Home BSM.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / SmartcardProvisioning -->
			<NodeName>SmartcardProvisioning</NodeName>
			<!-- Status: Required -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>This interior node contains information about the SmartcardProvisioningReception structures.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
			<Node> <!-- X / SmartcardProvisioning / FixedAddressingMode -->
				<NodeName/>
				<!-- Status: Required -->
				<DFProperties>
					<AccessType>
						<Get/>
					</AccessType>
					<DFFormat>
						<node/>
					</DFFormat>
					<Occurrence>
						<ZeroOrOne/>
					</Occurrence>
					<DFTitle>This interior node acts as a placeholder for sets of FixedAdressingMode information.</DFTitle>
					<DFType>
						<DDFName/>
					</DFType>
				</DFProperties>
				<Node> <!-- X / SmartcardProvisioning / FixedAddressingMode / USF -->
					<NodeName>USF</NodeName>
					<!-- Status: Required -->
					<DFProperties>
						<AccessType>
							<Get/>
						</AccessType>
						<DFFormat>
							<b64/>
						</DFFormat>
						<Occurrence>
							<One/>
						</Occurrence>
						<DFTitle>This leaf node specifies the value of the USF (Unique Smartcard Filter) associated to the device.</DFTitle>
						<DFType>
							<MIME>text/plain</MIME>
						</DFType>
					</DFProperties>
				</Node>
			</Node>
		</Node>
		<Node> <!-- X / Ext -->
			<NodeName>Ext</NodeName>
			<!-- Status: Optional -->
			<DFProperties>
				<AccessType>
					<Get/>
				</AccessType>
				<DFFormat>
					<node/>
				</DFFormat>
				<Occurrence>
					<ZeroOrOne/>
				</Occurrence>
				<DFTitle>Inside this interior node, vendor specific information related to BCAST can be
					placed.</DFTitle>
				<DFType>
					<DDFName/>
				</DFType>
			</DFProperties>
		</Node>
	</Node>
</MgmtTree>
