OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module RRLPV5Types

Import Declarations:

- ASNAUX
  all

Data Types Summary
PrivateExtensionList |
ExtensionSet |
Ext_GeographicalInformation |
VelocityEstimate |
_0RRLP_PDU |
Accuracy |
MeasureResponseTime |
BTSPosition |
BCCHCarrier |
BSIC |
ModuloTimeSlot |
SeqOfMsrAssistBTS |
MultiFrameOffset |
RoughRTD |
SeqOfSystemInfoAssistBTS |
FineRTD |
RelDistance |
RelativeAlt |
_0MultipleSets0 |
_0MultipleSets |
SeqOfReferenceIdentityType |
RequestIndex |
SystemInfoIndex |
CellID |
LAC |
SeqOfOTD_MsrElementRest |
_0OTD_MsrElementFirst0 |
_0OTD_MsrElementFirst |
SeqOfOTD_FirstSetMsrs |
_0OTD_MsrElementRest0 |
_0OTD_MsrElementRest |
SeqOfOTD_MsrsOfOtherSets |
RefQuality |
NumOfMeasurements |
StdResolution |
OTD_FirstSetMsrs |
_0EOTDQuality |
_0EOTDQuality0 |
OTDValue |
_0LocationInfo |
_0LocationInfo0 |
FixType |
SeqOfGPS_MsrSetElement |
_0GPS_MsrSetElement |
GPSTOW24b |
SeqOfGPS_MsrElement |
_0GPS_MsrElement0 |
_0GPS_MsrElement1 |
_0GPS_MsrElement2 |
_0GPS_MsrElement3 |
_0GPS_MsrElement |
GPSAssistanceData |
GPSTOW23b |
GPSWeek |
GPSTOWAssist |
TLMWord |
AntiSpoofFlag |
AlertFlag |
TLMReservedBits |
FrameNumber |
TimeSlot |
BitNumber |
_0DGPSCorrections |
_0DGPSCorrections0 |
SeqOfSatElement |
_0SatElement0 |
_0SatElement1 |
_0SatElement2 |
_0SatElement3 |
_0SatElement4 |
_0SatElement5 |
_0SatElement6 |
_0SatElement |
SatelliteID |
SeqOfNavModelElement |
_0UncompressedEphemeris0 |
_0UncompressedEphemeris17 |
_0UncompressedEphemeris16 |
_0UncompressedEphemeris15 |
_0UncompressedEphemeris14 |
_0UncompressedEphemeris13 |
_0UncompressedEphemeris12 |
_0UncompressedEphemeris11 |
_0UncompressedEphemeris10 |
_0UncompressedEphemeris |
_0UncompressedEphemeris19 |
_0UncompressedEphemeris18 |
_0UncompressedEphemeris20 |
_0UncompressedEphemeris26 |
_0UncompressedEphemeris9 |
_0UncompressedEphemeris25 |
_0UncompressedEphemeris22 |
_0UncompressedEphemeris21 |
_0UncompressedEphemeris24 |
_0UncompressedEphemeris23 |
_0UncompressedEphemeris1 |
_0UncompressedEphemeris2 |
_0UncompressedEphemeris3 |
_0UncompressedEphemeris4 |
_0UncompressedEphemeris5 |
_0UncompressedEphemeris6 |
_0UncompressedEphemeris7 |
_0UncompressedEphemeris8 |
_0EphemerisSubframe1Reserved |
_0EphemerisSubframe1Reserved0 |
_0EphemerisSubframe1Reserved1 |
_0EphemerisSubframe1Reserved2 |
_0IonosphericModel4 |
_0IonosphericModel3 |
_0IonosphericModel6 |
_0IonosphericModel5 |
_0IonosphericModel0 |
_0IonosphericModel2 |
_0IonosphericModel1 |
_0IonosphericModel |
_0UTCModel6 |
_0UTCModel0 |
_0UTCModel1 |
_0UTCModel2 |
_0UTCModel |
_0UTCModel3 |
_0UTCModel4 |
_0UTCModel5 |
_0Almanac |
SeqOfAlmanacElement |
_0AlmanacElement8 |
_0AlmanacElement9 |
_0AlmanacElement |
_0AlmanacElement6 |
_0AlmanacElement7 |
_0AlmanacElement4 |
_0AlmanacElement5 |
_0AlmanacElement2 |
_0AlmanacElement3 |
_0AlmanacElement0 |
_0AlmanacElement1 |
SeqOfAcquisElement |
_0AcquisElement3 |
_0AcquisElement0 |
_0AcquisElement1 |
_0AcquisElement2 |
_0AcquisElement |
_0AddionalDopplerFields0 |
_0AddionalDopplerFields |
_0AddionalAngleFields0 |
_0AddionalAngleFields |
SeqOf_BadSatelliteSet |
SeqOfMsrAssistBTS_R98_ExpOTD |
SeqOfSystemInfoAssistBTS_R98_ExpOTD |
ExpectedOTD |
ExpOTDUncertainty |
GPSReferenceTimeUncertainty |
_0GPSTimeAssistanceMeasurements |
_0GPSTimeAssistanceMeasurements1 |
_0GPSTimeAssistanceMeasurements0 |
SeqOfOTD_FirstSetMsrs_R98_Ext |
_0Extended_reference0 |
_0Extended_reference |
OTD_MeasureInfo_5_Ext |
PositionMethod |
UseMultipleSets |
EnvironmentCharacter |
TimeSlotScheme |
ReferenceRelation |
MpathIndic |
LocErrorReason |
ErrorCodes |
MoreAssDataToBeSent |
UlPseudoSegInd |
ExtensionContainer |
PrivateExtension |
PCS_Extensions |
MAP_EXTENSION |
RRLP_PDU |
MsrPosition_Req |
MsrPosition_Rsp |
AssistanceData |
ProtocolError |
PositionInstruct |
AccuracyOpt |
ReferenceAssistData |
MsrAssistData |
MsrAssistBTS |
SystemInfoAssistData |
AssistBTSData |
CalcAssistanceBTS |
ReferenceWGS84 |
MultipleSets |
ReferenceIdentity |
BSICAndCarrier |
CellIDAndLAC |
OTD_MeasureInfo |
OTD_MsrElementFirst |
OTD_MsrElementRest |
TOA_MeasurementsOfRef |
OTD_Measurement |
OTD_MeasurementWithID |
EOTDQuality |
MultiFrameCarrier |
LocationInfo |
GPS_MeasureInfo |
GPS_MsrSetElement |
GPS_MsrElement |
LocationError |
AdditionalAssistanceData |
GPS_AssistData |
ControlHeader |
ReferenceTime |
GPSTime |
GPSTOWAssistElement |
GSMTime |
RefLocation |
DGPSCorrections |
SatElement |
NavigationModel |
NavModelElement |
UncompressedEphemeris |
EphemerisSubframe1Reserved |
IonosphericModel |
UTCModel |
Almanac |
AlmanacElement |
AcquisAssist |
TimeRelation |
AcquisElement |
AddionalDopplerFields |
AddionalAngleFields |
Rel98_MsrPosition_Req_Extension |
Rel98_AssistanceData_Extension |
Rel98_Ext_ExpOTD |
MsrAssistData_R98_ExpOTD |
MsrAssistBTS_R98_ExpOTD |
SystemInfoAssistData_R98_ExpOTD |
AssistBTSData_R98_ExpOTD |
GPSTimeAssistanceMeasurements |
Rel_98_MsrPosition_Rsp_Extension |
_0Rel_98_MsrPosition_Rsp_Extension |
OTD_MeasureInfo_R98_Ext |
OTD_MsrElementFirst_R98_Ext |
Rel_5_MsrPosition_Rsp_Extension |
Extended_reference |
Rel5_MsrPosition_Req_Extension |
Rel5_AssistanceData_Extension |
Rel_5_ProtocolError_Extension |
RRLP_Component |
MethodType |
SystemInfoAssistBTS |
ReferenceIdentityType |
OTD_MsrsOfOtherSets |
NeighborIdentity |
SatStatus |
SystemInfoAssistBTS_R98_ExpOTD |

Constants Summary
maxNumOfPrivateExtensions |
maxExt_GeographicalInformation |
FixType_twoDFix_ |
FixType_threeDFix_ |
maxGPSAssistanceData |

## Details

PrivateExtensionList

    PrivateExtensionList ::= SEQUENCE SIZE (1..maxNumOfPrivateExtensions) OF
                    PrivateExtension
    PrivateExtension

ExtensionSet

    ExtensionSet        MAP-EXTENSION ::=
            {...
             -- ExtensionSet is the set of all defined private extensions
        }
        -- Unsupported private extensions shall be discarded if received.
    PCS-Extensions

Ext_GeographicalInformation

    Ext-GeographicalInformation ::= OCTET STRING (SIZE (1..maxExt-GeographicalInformation))
    -- Refers to geographical Information defined in GSM 03.32.
    -- This is composed of 1 or more octets with an internal structure according to GSM 03.32
    -- Octet 1: Type of shape, only the following shapes in GSM 03.32 are allowed:
    --        (a) Ellipsoid point with uncertainty circle
    --        (b) Ellipsoid point with uncertainty ellipse
    -- Any other value in octet 1 shall be treated as invalid
    -- Octets 2 to 8 for case (a) – Ellipsoid point with uncertainty circle
    --        Degrees of Latitude                3 octets
    --        Degrees of Longitude                3 octets
    --        Uncertainty code                1 octet
    -- Octets 2 to 10 for case (b) – Ellipsoid point with uncertainty ellipse:
    --        Degrees of Latitude                3 octets
    --        Degrees of Longitude                3 octets
    --        Uncertainty semi-major axis                1 octet
    --        Uncertainty semi-minor axis                1 octet
    --        Angle of major axis                1 octet
    --
    -- An Ext-GeogrpahicalInformation parameter containing any other shape or an incorrect number
    -- of octets or coding according to GSM 03.32 shall be treated as invalid data by a receiver
    maxExt-GeographicalInformation

VelocityEstimate

    VelocityEstimate ::= OCTET STRING (SIZE (4..7))
        -- Refers to Velocity description defined in 3GPP TS 23.032.
        -- This is composed of 4 or more octets with an internal structure according to
        -- 3GPP TS 23.032
        -- Octet 1: Type of velocity, only the following types in 3GPP TS 23.032 are allowed:
        --        (a) Horizontal Velocity
        --        (b) Horizontal with Vertical Velocity
        --        (c) Horizontal Velocity with Uncertainty
        --        (d) Horizontal with Vertical Velocity and Uncertainty
        -- For types Horizontal with Vertical Velocity and Horizontal with Vertical Velocity
        -- and Uncertainty, the direction of the Vertical Speed is also included in Octet 1
        -- Any other value in octet 1 shall be treated as invalid
        -- Octets 2 to 4 for case (a) Horizontal velocity:
        --        Bearing                1 octet
        --        Horizontal Speed                2 octets
        -- Octets 2 to 5 for case (b) – Horizontal with Vertical Velocity:
        --        Bearing                1 octet
        --        Horizontal Speed                2 octets
        --        Vertical Speed                1 octet
        -- Octets 2 to 5 for case (c) – Horizontal velocity with Uncertainty:
        --        Bearing                1 octet
        --        Horizontal Speed                2 octets
        --        Uncertainty Speed                1 octet
        -- Octets 2 to 7 for case (d) – Horizontal with Vertical Velocity and Uncertainty:
        --        Bearing                1 octet
        --        Horizontal Speed                2 octets
        --        Vertical Speed                1 octet
        --        Horizontal Uncertainty Speed            1 octet
        --        Vertical Uncertainty Speed                1 octet
    -- Information Elements copied from TS 44.031 v5.c.0
    RRLP-PDU

_0RRLP_PDU

    INTEGER (0..7)

Accuracy

    Accuracy ::= INTEGER (0..127)
    -- Position Method
    PositionMethod

MeasureResponseTime

    MeasureResponseTime ::= INTEGER (0..7)
    -- useMultiple Sets, FFS!
    UseMultipleSets

BTSPosition

    Ext-GeographicalInformation
    -- RF channel number of BCCH
    BCCHCarrier

BCCHCarrier

    BCCHCarrier ::= INTEGER (0..1023)
    -- Base station Identity Code
    BSIC

BSIC

    BSIC ::= INTEGER (0..63)
    -- Timeslot scheme
    TimeSlotScheme

ModuloTimeSlot

    ModuloTimeSlot ::= INTEGER (0..3)
    -- E-OTD measurement assistance data IE
    -- The total number of neighbors in this element (MsrAssistData)
    -- and in SystemInfoAssistData element (presented neighbors
    -- can be at a maximum 15!)
    MsrAssistData

SeqOfMsrAssistBTS

    SeqOfMsrAssistBTS ::= SEQUENCE (SIZE(1..15)) OF MsrAssistBTS
    MsrAssistBTS

MultiFrameOffset

    MultiFrameOffset ::= INTEGER (0..51)
    -- The Multiframe Offset value 51 shall not be encoded by the transmitting entity and
    -- shall be treated by the receiving entity as 0.
    -- Rough RTD value between one base station and reference BTS
    RoughRTD

RoughRTD

    RoughRTD ::= INTEGER (0..1250)
    -- The RoughRTD value 1250 shall not be encoded by the transmitting entity and shall
    -- be treated by the receiving entity as 0.
    -- E-OTD Measurement assistance data for system information List IE
    -- The total number of base stations in this element (SystemInfoAssistData
    -- presented neighbors) and in MsrAssistData element can be at a maximum 15.
    SystemInfoAssistData

SeqOfSystemInfoAssistBTS

    SeqOfSystemInfoAssistBTS::= SEQUENCE (SIZE(1..32)) OF SystemInfoAssistBTS
    -- whether n.th is present or not ?
    SystemInfoAssistBTS

FineRTD

    FineRTD ::= INTEGER (0..255)
    -- Relative north/east distance
    RelDistance

RelDistance

    RelDistance ::= INTEGER (-200000..200000)
    -- Relative altitude
    RelativeAlt

RelativeAlt

    RelativeAlt ::= INTEGER (-4000..4000)
    -- Measure position response IEs
    -- Reference Identity
    -- Multiple sets
    MultipleSets

_0MultipleSets0

    INTEGER (1..3)

_0MultipleSets

    INTEGER (2..3)

SeqOfReferenceIdentityType

    SeqOfReferenceIdentityType ::= SEQUENCE (SIZE(1..3)) OF ReferenceIdentityType
    -- Cell identity
    ReferenceIdentityType

RequestIndex

    RequestIndex ::= INTEGER (1..16)
    SystemInfoIndex

SystemInfoIndex

    SystemInfoIndex ::= INTEGER (1..32)
    CellIDAndLAC

CellID

    CellID ::= INTEGER (0..65535)
    LAC

LAC

    LAC ::= INTEGER (0..65535)
    -- OTD-MeasureInfo
    OTD-MeasureInfo

SeqOfOTD_MsrElementRest

    SeqOfOTD-MsrElementRest ::= SEQUENCE (SIZE(1..2)) OF OTD-MsrElementRest
    -- OTD measurent information for 1 set
    OTD-MsrElementFirst

_0OTD_MsrElementFirst0

    INTEGER (0..960)        OPTIONAL

_0OTD_MsrElementFirst

    INTEGER (0..42431)

SeqOfOTD_FirstSetMsrs

    SeqOfOTD-FirstSetMsrs ::= SEQUENCE (SIZE(1..10)) OF OTD-FirstSetMsrs
    -- OTD measurent information 2 and 3 sets if exist
    OTD-MsrElementRest

_0OTD_MsrElementRest0

    INTEGER (0..960)            OPTIONAL

_0OTD_MsrElementRest

    INTEGER (0..42431)

SeqOfOTD_MsrsOfOtherSets

    SeqOfOTD-MsrsOfOtherSets ::= SEQUENCE (SIZE(1..10)) OF OTD-MsrsOfOtherSets
    -- Standard deviation of the TOA measurements from the reference BTS
    TOA-MeasurementsOfRef

RefQuality

    RefQuality ::= INTEGER (0..31)            -- St Dev of TOA of reference as defined in annex
    NumOfMeasurements

NumOfMeasurements

    NumOfMeasurements ::= INTEGER (0..7)    -- No. of measurements for RefQuality as defined in annex
    StdResolution

StdResolution

    StdResolution ::= INTEGER (0..3)        -- Values of resolution are defined in annex
    OTD-FirstSetMsrs

OTD_FirstSetMsrs

    OTD-MeasurementWithID
    -- Neighbour info in OTD measurements 0-10 times in TD measurement info
    OTD-MsrsOfOtherSets

_0EOTDQuality

    INTEGER    (0..7)

_0EOTDQuality0

    INTEGER (0..31)

OTDValue

    OTDValue ::= INTEGER (0..39999)
    -- Location information IE
    LocationInfo

_0LocationInfo

    INTEGER (0..65535)

_0LocationInfo0

    INTEGER (0..14399999)    OPTIONAL

FixType

    FixType ::= INTEGER {
        twoDFix (0),
        threeDFix (1)
    } (0..1)
    -- GPS-Measurement information
    GPS-MeasureInfo

SeqOfGPS_MsrSetElement

    SeqOfGPS-MsrSetElement ::= SEQUENCE (SIZE(1..3)) OF GPS-MsrSetElement
    -- OTD measurent information 1-3 times in message
    GPS-MsrSetElement

_0GPS_MsrSetElement

    INTEGER (0..65535)    OPTIONAL

GPSTOW24b

    GPSTOW24b ::= INTEGER (0..14399999)
    -- measured elements in measurement parameters field
    SeqOfGPS-MsrElement

SeqOfGPS_MsrElement

    SeqOfGPS-MsrElement ::= SEQUENCE (SIZE(1..16)) OF GPS-MsrElement
    GPS-MsrElement

_0GPS_MsrElement0

    INTEGER (-32768..32767)

_0GPS_MsrElement1

    INTEGER (0..1022)

_0GPS_MsrElement2

    INTEGER (0..1024)

_0GPS_MsrElement3

    INTEGER (0..63)

_0GPS_MsrElement

    INTEGER (0..63)

GPSAssistanceData

    GPSAssistanceData ::= OCTET STRING (SIZE (1..maxGPSAssistanceData))
    -- GPSAssistanceData has identical structure and encoding to octets 3 to n of the
    -- GPS Assistance Data IE in 3GPP TS 49.031
    maxGPSAssistanceData

GPSTOW23b

    GPSTOW23b ::= INTEGER (0..7559999)
    -- GPS week number
    GPSWeek

GPSWeek

    GPSWeek ::= INTEGER (0..1023)
    -- GPSTOWAssist consists of TLM message, Anti-spoof flag, Alert flag, and 2 reserved bits in TLM Word
    -- for each visible satellite.
    -- N_SAT can be read from number of elements in GPSTOWAssist
    GPSTOWAssist

GPSTOWAssist

    GPSTOWAssist ::= SEQUENCE (SIZE(1..12)) OF GPSTOWAssistElement
    GPSTOWAssistElement

TLMWord

    TLMWord ::= INTEGER (0..16383)
    -- Anti-Spoof flag
    AntiSpoofFlag

AntiSpoofFlag

    AntiSpoofFlag ::= INTEGER (0..1)
    -- Alert flag
    AlertFlag

AlertFlag

    AlertFlag ::= INTEGER (0..1)
    -- Reserved bits in TLM word, MSB occurs earlier in TLM Word transmitted by satellite
    TLMReservedBits

TLMReservedBits

    TLMReservedBits ::= INTEGER (0..3)
    GSMTime

FrameNumber

    FrameNumber ::= INTEGER (0..2097151)
    -- Time slot number
    TimeSlot

TimeSlot

    TimeSlot ::= INTEGER (0..7)
    -- Bit number
    BitNumber

BitNumber

    BitNumber ::= INTEGER (0..156)
    -- Reference Location IE
    RefLocation

_0DGPSCorrections

    INTEGER (0..604799)

_0DGPSCorrections0

    INTEGER (0..7)

SeqOfSatElement

    SeqOfSatElement ::= SEQUENCE (SIZE (1..16)) OF SatElement
    -- number of correction for satellites
    SatElement

_0SatElement0

    INTEGER (0..3)

_0SatElement1

    INTEGER (-2047..2047)

_0SatElement2

    INTEGER (-127..127)

_0SatElement3

    INTEGER (-127..127)

_0SatElement4

    INTEGER (-7..7)

_0SatElement5

    INTEGER (-127..127)

_0SatElement6

    INTEGER (-7..7)

_0SatElement

    INTEGER (0..239)

SatelliteID

    SatelliteID ::= INTEGER (0..63)    -- identifies satellite
    -- Navigation Model IE
    NavigationModel

SeqOfNavModelElement

    SeqOfNavModelElement ::= SEQUENCE (SIZE(1..16)) OF NavModelElement
    NavModelElement

_0UncompressedEphemeris0

    INTEGER (0..15)

_0UncompressedEphemeris17

    INTEGER (0..1)

_0UncompressedEphemeris16

    INTEGER (0..37799)

_0UncompressedEphemeris15

    INTEGER (0..4294967295)

_0UncompressedEphemeris14

    INTEGER (-32768..32767)

_0UncompressedEphemeris13

    INTEGER (0..4294967295)

_0UncompressedEphemeris12

    INTEGER (-32768..32767)

_0UncompressedEphemeris11

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris10

    INTEGER (-32768..32767)

_0UncompressedEphemeris

    INTEGER (0..3)

_0UncompressedEphemeris19

    INTEGER (-32768..32767)

_0UncompressedEphemeris18

    INTEGER (0..31)

_0UncompressedEphemeris20

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris26

    INTEGER (-8192..8191)

_0UncompressedEphemeris9

    INTEGER (-32768..32767)

_0UncompressedEphemeris25

    INTEGER (-8388608..8388607)

_0UncompressedEphemeris22

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris21

    INTEGER (-32768..32767)

_0UncompressedEphemeris24

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris23

    INTEGER (-32768..32767)

_0UncompressedEphemeris1

    INTEGER (0..63)

_0UncompressedEphemeris2

    INTEGER    (0..1023)

_0UncompressedEphemeris3

    INTEGER (0..1)

_0UncompressedEphemeris4

    INTEGER (-128..127)

_0UncompressedEphemeris5

    INTEGER (0..37799)

_0UncompressedEphemeris6

    INTEGER (-128..127)

_0UncompressedEphemeris7

    INTEGER (-32768..32767)

_0UncompressedEphemeris8

    INTEGER (-2097152..2097151)

_0EphemerisSubframe1Reserved

    INTEGER (0..8388607)

_0EphemerisSubframe1Reserved0

    INTEGER (0..16777215)

_0EphemerisSubframe1Reserved1

    INTEGER (0..16777215)

_0EphemerisSubframe1Reserved2

    INTEGER (0..65535)

_0IonosphericModel4

    INTEGER (-128..127)

_0IonosphericModel3

    INTEGER (-128..127)

_0IonosphericModel6

    INTEGER (-128..127)

_0IonosphericModel5

    INTEGER (-128..127)

_0IonosphericModel0

    INTEGER (-128..127)

_0IonosphericModel2

    INTEGER (-128..127)

_0IonosphericModel1

    INTEGER (-128..127)

_0IonosphericModel

    INTEGER (-128..127)

_0UTCModel6

    INTEGER (-128..127)

_0UTCModel0

    INTEGER (-2147483648..2147483647)

_0UTCModel1

    INTEGER (0..255)

_0UTCModel2

    INTEGER (0..255)

_0UTCModel

    INTEGER (-8388608..8388607)

_0UTCModel3

    INTEGER (-128..127)

_0UTCModel4

    INTEGER (0..255)

_0UTCModel5

    INTEGER (-128..127)

_0Almanac

    INTEGER (0..255)

SeqOfAlmanacElement

    SeqOfAlmanacElement ::= SEQUENCE (SIZE(1..64)) OF AlmanacElement
    -- Almanac info once per satellite
    AlmanacElement

_0AlmanacElement8

    INTEGER (-1024..1023)

_0AlmanacElement9

    INTEGER (-1024..1023)

_0AlmanacElement

    INTEGER (0..65535)

_0AlmanacElement6

    INTEGER (-8388608..8388607)

_0AlmanacElement7

    INTEGER (-8388608..8388607)

_0AlmanacElement4

    INTEGER (0..16777215)

_0AlmanacElement5

    INTEGER (-8388608..8388607)

_0AlmanacElement2

    INTEGER (-32768..32767)

_0AlmanacElement3

    INTEGER (0..255)

_0AlmanacElement0

    INTEGER (0..255)

_0AlmanacElement1

    INTEGER (-32768..32767)

SeqOfAcquisElement

    SeqOfAcquisElement ::= SEQUENCE (SIZE(1..16)) OF AcquisElement
    -- the relationship between GPS time and air-interface timing
    TimeRelation

_0AcquisElement3

    INTEGER (0..15)

_0AcquisElement0

    INTEGER (0..1022)

_0AcquisElement1

    INTEGER (0..19)

_0AcquisElement2

    INTEGER (0..3)

_0AcquisElement

    INTEGER (-2048..2047)

_0AddionalDopplerFields0

    INTEGER (0..7)

_0AddionalDopplerFields

    INTEGER (0..63)

_0AddionalAngleFields0

    INTEGER (0..7)

_0AddionalAngleFields

    INTEGER (0..31)

SeqOf_BadSatelliteSet

    SeqOf-BadSatelliteSet ::= SEQUENCE (SIZE(1..16)) OF SatelliteID
    -- Extension Elements
    -- Release 98 Extensions here
    Rel98-MsrPosition-Req-Extension

SeqOfMsrAssistBTS_R98_ExpOTD

    SeqOfMsrAssistBTS-R98-ExpOTD ::= SEQUENCE (SIZE(1..15)) OF MsrAssistBTS-R98-ExpOTD
    -- This element completes MsrAssistBTS IE
    MsrAssistBTS-R98-ExpOTD

SeqOfSystemInfoAssistBTS_R98_ExpOTD

    SeqOfSystemInfoAssistBTS-R98-ExpOTD ::= SEQUENCE (SIZE(1..32)) OF SystemInfoAssistBTS-R98-ExpOTD
    -- whether n.th is present or not ?
    SystemInfoAssistBTS-R98-ExpOTD

ExpectedOTD

    ExpectedOTD ::= INTEGER (0..1250)
    -- The ExpectedOTD value 1250 shall not be encoded by the transmitting entity and
    -- shall be treated by the receiving entity as 0.
    -- Uncertainty of Exptected OTD in bits
    ExpOTDUncertainty

ExpOTDUncertainty

    ExpOTDUncertainty ::= INTEGER(0..7)
    -- Release 98 extensions
    GPSReferenceTimeUncertainty

GPSReferenceTimeUncertainty

    GPSReferenceTimeUncertainty ::= INTEGER (0 .. 127)   -- Coding according to Annex
    GPSTimeAssistanceMeasurements

_0GPSTimeAssistanceMeasurements

    INTEGER (0 .. 63)

_0GPSTimeAssistanceMeasurements1

    INTEGER (0 .. 127)   OPTIONAL

_0GPSTimeAssistanceMeasurements0

    INTEGER (0 .. 9999)   OPTIONAL

SeqOfOTD_FirstSetMsrs_R98_Ext

    SeqOfOTD-FirstSetMsrs-R98-Ext ::= SEQUENCE (SIZE(1..5)) OF OTD-FirstSetMsrs
    Rel-5-MsrPosition-Rsp-Extension

_0Extended_reference0

    INTEGER (0..262143)

_0Extended_reference

    INTEGER (0..63)

OTD_MeasureInfo_5_Ext

    SeqOfOTD-MsrElementRest
    -- if more than one measurement sets are present this element is repeated
    -- NumberOfSets - 1 (-1 = first set) combined in OTD-MeasureInfo-5-Ext and
    -- OTD-MeasureInfo (e.g. if NumberOfSets is 3, then one otdMsrRestSets may
    -- be sent in OTD-MeasureInfo-5-Ext and one in OTD-MeasureInfo)
    -- First part of Uplink RRLP Pseudo-segmentation indication, possibly more may be defined
    -- in the future for segmentation with more than two segments.
    UlPseudoSegInd

PositionMethod

    ENUMERATED {
    eotd (0),
    gps (1),
    gpsOrEOTD (2)
    }
    -- Measurement request response time
    MeasureResponseTime

UseMultipleSets

    ENUMERATED {
    multipleSets (0),        -- multiple sets are allowed
    oneSet (1)                -- sending of multiple is not allowed
    }
    -- Environment characterization
    EnvironmentCharacter

EnvironmentCharacter

    ENUMERATED {
    badArea (0),        -- bad urban or suburban, heavy multipath and NLOS
    notBadArea (1),        -- light multipath and NLOS
    mixedArea (2),        -- not defined or mixed environment
    ...
    }
    -- E-OTD reference BTS for Assitance data IE
    ReferenceAssistData

TimeSlotScheme

    ENUMERATED {
    equalLength (0),
    variousLength (1)
    }
    -- Time slot (modulo)
    ModuloTimeSlot

ReferenceRelation

    ENUMERATED {
    secondBTSThirdSet (0),    -- 1st BTS related to 1st and 2nd sets
    secondBTSSecondSet (1),    -- 1st BTS related to 1st and 3rd sets
    firstBTSFirstSet (2)    -- 1st BTS related to 1st set
    }
    -- Reference BTS Identity, this element contains number of
    -- BTSs told nbrOfReferenceBTSs field in Multiple sets element)
    ReferenceIdentity

MpathIndic

    ENUMERATED {
    notMeasured (0),
    low (1),
    medium (2),
    high (3)
    }
    -- Location error IE
    LocationError

LocErrorReason

    ENUMERATED {
    unDefined (0),
    notEnoughBTSs (1),
    notEnoughSats (2),
    eotdLocCalAssDataMissing (3),
    eotdAssDataMissing (4),
    gpsLocCalAssDataMissing (5),
    gpsAssDataMissing (6),
    methodNotSupported (7),
    notProcessed (8),
    refBTSForGPSNotServingBTS (9),
    refBTSForEOTDNotServingBTS (10),
    ...
    }
    -- exception handling:
    -- an unrecognized value shall be treated the same as value 0
    -- defines additional assistance data needed for any new location attempt
    -- MS shall retain any assistance data already received
    AdditionalAssistanceData

ErrorCodes

    ENUMERATED {
    unDefined (0),
    missingComponet (1),
    incorrectData (2),
    missingIEorComponentElement (3),
    messageTooShort (4),
    unknowReferenceNumber (5),
    ...
    }
    -- exception handling:
    -- an unrecognized value shall be treated the same as value 0
    -- GPS assistance data IE
    GPS-AssistData

MoreAssDataToBeSent

    ENUMERATED {
    noMoreMessages (0),            -- This is the only or last Assistance Data message used to deliver
    -- the entire set of assistance data.
    moreMessagesOnTheWay (1)    -- The SMLC will send more Assistance Data messages or a final RRLP
    -- Measure Position Request message to deliver the
    -- the entire set of assistance data.
    }
    -- Control header of the GPS assistance data
    ControlHeader

UlPseudoSegInd

    ENUMERATED {
    firstOfMany (0),
    secondOfMany(1)
    }
    Rel5-MsrPosition-Req-Extension

ExtensionContainer

    ExtensionContainer ::= SEQUENCE {
        privateExtensionList    [0]PrivateExtensionList    OPTIONAL,
        pcs-Extensions    [1]PCS-Extensions    OPTIONAL,
        ...}
    PrivateExtensionList

PrivateExtension

    PrivateExtension ::= SEQUENCE {
        extId        MAP-EXTENSION.&extensionId
                    ({ExtensionSet}),
        extType        MAP-EXTENSION.&ExtensionType
                    ({ExtensionSet}{@extId})    OPTIONAL}
    maxNumOfPrivateExtensions

PCS_Extensions

    PCS-Extensions ::= SEQUENCE {
        ...}
    MAP-EXTENSION

MAP_EXTENSION

    MAP-EXTENSION  ::= CLASS {
    &ExtensionType                OPTIONAL,
    &extensionId     OBJECT IDENTIFIER }
    -- The length of the Object Identifier shall not exceed 16 octets and the
    -- number of components of the Object Identifier shall not exceed 16
    -- Information Elements copied from TS 29002-310 and TS 29002-750
    -- Note: Ext-GeographicalInformation is defined in TS 29002-310 MAP-LCS-DataTypes version5
    -- VelocityEstimate is defined in TS 29002-750 MAP-LCS-DataTypes version10
    Ext-GeographicalInformation

RRLP_PDU

    RRLP-PDU ::= SEQUENCE {
        referenceNumber            INTEGER (0..7),
        component                RRLP-Component
    }
    RRLP-Component

MsrPosition_Req

    MsrPosition-Req ::= SEQUENCE {
        positionInstruct        PositionInstruct,
        referenceAssistData        ReferenceAssistData        OPTIONAL,
        msrAssistData            MsrAssistData            OPTIONAL,
        systemInfoAssistData    SystemInfoAssistData    OPTIONAL,
        gps-AssistData            GPS-AssistData            OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release 98 extension element
    rel98-MsrPosition-Req-extension            Rel98-MsrPosition-Req-Extension            OPTIONAL,
        -- Release 5 extension element
    rel5-MsrPosition-Req-extension            Rel5-MsrPosition-Req-Extension            OPTIONAL
    }
    -- add this defintion to RRLP-Components module
    -- Measurement Position response component
    MsrPosition-Rsp

MsrPosition_Rsp

    MsrPosition-Rsp ::= SEQUENCE {
        multipleSets            MultipleSets            OPTIONAL,
        referenceIdentity        ReferenceIdentity        OPTIONAL,
        otd-MeasureInfo            OTD-MeasureInfo            OPTIONAL,
        locationInfo            LocationInfo            OPTIONAL,
        gps-MeasureInfo            GPS-MeasureInfo            OPTIONAL,
        locationError            LocationError            OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extension here
        rel-98-MsrPosition-Rsp-Extension
                                Rel-98-MsrPosition-Rsp-Extension        OPTIONAL,
        rel-5-MsrPosition-Rsp-Extension
                                Rel-5-MsrPosition-Rsp-Extension        OPTIONAL
        -- rel-5-MsrPosition-Rsp-Extension and other possible future extensions
        -- are the only information elements that may be included in the 2nd
        -- MsrPosition-Rsp component when RRLP pseudo-segmentation is used
    }
    -- add this defintion to RRLP-Components module
    -- Assistance Data component
    AssistanceData

AssistanceData

    AssistanceData ::= SEQUENCE {
        referenceAssistData    ReferenceAssistData            OPTIONAL,
        msrAssistData            MsrAssistData            OPTIONAL,
        systemInfoAssistData    SystemInfoAssistData    OPTIONAL,
        gps-AssistData            GPS-AssistData            OPTIONAL,
        moreAssDataToBeSent        MoreAssDataToBeSent        OPTIONAL,    -- If not present, interpret as only
                                                                    -- Assistance Data component used to
                                                                    -- deliver entire set of assistance
                                                                    -- data.
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extension here
        rel98-AssistanceData-Extension    Rel98-AssistanceData-Extension    OPTIONAL,
        rel5-AssistanceData-Extension    Rel5-AssistanceData-Extension    OPTIONAL
    }
    -- add this defintion to RRLP-Components module
    -- Protocol Error component
    ProtocolError

ProtocolError

    ProtocolError ::= SEQUENCE {
        errorCause                ErrorCodes,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extensions here
        rel-5-ProtocolError-Extension Rel-5-ProtocolError-Extension        OPTIONAL
    }
    -- add these defintions to RRLP-Components module
    -- Position instructions
    PositionInstruct

PositionInstruct

    PositionInstruct ::= SEQUENCE {
        -- Method type
        methodType                MethodType,
        positionMethod            PositionMethod,
        measureResponseTime        MeasureResponseTime,
        useMultipleSets            UseMultipleSets,
        environmentCharacter    EnvironmentCharacter    OPTIONAL
    }
    --
    MethodType

AccuracyOpt

    AccuracyOpt ::= SEQUENCE {
        accuracy        Accuracy    OPTIONAL
    }
    -- The values of this field are defined in 3GPP TS 23.032 (Uncertainty code)
    Accuracy

ReferenceAssistData

    ReferenceAssistData ::= SEQUENCE {
        bcchCarrier        BCCHCarrier,                        -- BCCH carrier
        bsic            BSIC,                                -- BSIC
        timeSlotScheme    TimeSlotScheme,                     -- Timeslot scheme
        btsPosition        BTSPosition            OPTIONAL
    }
    -- ellipsoid point and
    -- ellipsoid point with altitude and uncertainty ellipsoid shapes are supported
    BTSPosition

MsrAssistData

    MsrAssistData ::= SEQUENCE {
         msrAssistList SeqOfMsrAssistBTS
    }
    SeqOfMsrAssistBTS

MsrAssistBTS

    MsrAssistBTS ::= SEQUENCE {
        bcchCarrier            BCCHCarrier,        -- BCCH carrier
        bsic                BSIC,                -- BSIC
        multiFrameOffset    MultiFrameOffset,     -- multiframe offset
        timeSlotScheme        TimeSlotScheme,        -- Timeslot scheme
        roughRTD            RoughRTD,            -- rough RTD value
        -- Location Calculation Assistance data is moved here
        calcAssistanceBTS    CalcAssistanceBTS    OPTIONAL
    }
    -- Multiframe offset
    MultiFrameOffset

SystemInfoAssistData

    SystemInfoAssistData ::= SEQUENCE {
        systemInfoAssistList     SeqOfSystemInfoAssistBTS
    }
    SeqOfSystemInfoAssistBTS

AssistBTSData

    AssistBTSData ::= SEQUENCE {
        bsic                BSIC,                -- BSIC
        multiFrameOffset    MultiFrameOffset,    -- multiframe offset
        timeSlotScheme        TimeSlotScheme,        -- Timeslot scheme
        roughRTD            RoughRTD,            -- rough RTD value
        -- Location Calculation Assistance data
        calcAssistanceBTS    CalcAssistanceBTS    OPTIONAL
    }
    -- E-OTD Location calculation assistance data,
    -- CalcAssistanceBTS element is optional not subfields
    CalcAssistanceBTS

CalcAssistanceBTS

    CalcAssistanceBTS ::= SEQUENCE {
        fineRTD                FineRTD,        -- fine RTD value between base stations
        referenceWGS84        ReferenceWGS84    -- reference coordinates
    }
    -- Coordinates of neighbour BTS, WGS-84 ellipsoid
    ReferenceWGS84

ReferenceWGS84

    ReferenceWGS84 ::= SEQUENCE {
        relativeNorth    RelDistance,                -- relative distance (south negative)
        relativeEast    RelDistance,                -- relative distance (west negative)
        -- Relative Altitude is not always known
        relativeAlt        RelativeAlt        OPTIONAL    -- relative altitude
    }
    -- Fine RTD value between this BTS and the reference BTS
    FineRTD

MultipleSets

    MultipleSets ::= SEQUENCE {
        -- number of reference sets
        nbrOfSets            INTEGER (2..3),
        -- This field actually tells the number of reference BTSs
        nbrOfReferenceBTSs    INTEGER (1..3),
        -- This field is conditional and included optionally only if
        -- nbrOfSets is 3 and number of reference BTSs is 2.
        referenceRelation        ReferenceRelation        OPTIONAL
    }
    -- Relation between refence BTSs and sets
    ReferenceRelation

ReferenceIdentity

    ReferenceIdentity ::= SEQUENCE {
        -- Reference BTS list
        refBTSList        SeqOfReferenceIdentityType
    }
    SeqOfReferenceIdentityType

BSICAndCarrier

    BSICAndCarrier ::= SEQUENCE {
        carrier    BCCHCarrier,
        bsic        BSIC
    }
    RequestIndex

CellIDAndLAC

    CellIDAndLAC ::= SEQUENCE {
        referenceLAC    LAC,                -- Location area code
        referenceCI        CellID                -- Cell identity
    }
    CellID

OTD_MeasureInfo

    OTD-MeasureInfo ::= SEQUENCE {
        -- Measurement info elements, OTD-MsrElement is repeated number of times
        -- told in nbrOfReferenceBTSs in MultipleSets, default value is 1
        otdMsrFirstSets        OTD-MsrElementFirst,
        -- if more than one sets are present this element is repeated
        -- NumberOfSets - 1 (-1 = first set)
        otdMsrRestSets        SeqOfOTD-MsrElementRest        OPTIONAL
    }
    SeqOfOTD-MsrElementRest

OTD_MsrElementFirst

    OTD-MsrElementFirst ::= SEQUENCE {
        refFrameNumber            INTEGER (0..42431),                 -- Frame number modulo 42432
        referenceTimeSlot        ModuloTimeSlot,
        toaMeasurementsOfRef    TOA-MeasurementsOfRef    OPTIONAL,
        stdResolution            StdResolution,
        taCorrection            INTEGER (0..960)        OPTIONAL,    -- TA correction
        -- measured neighbors in OTD measurements
        otd-FirstSetMsrs         SeqOfOTD-FirstSetMsrs     OPTIONAL
    }
    SeqOfOTD-FirstSetMsrs

OTD_MsrElementRest

    OTD-MsrElementRest ::= SEQUENCE {
        refFrameNumber            INTEGER (0..42431),                     -- Frame number modulo 42432
        referenceTimeSlot        ModuloTimeSlot,
        toaMeasurementsOfRef    TOA-MeasurementsOfRef        OPTIONAL,
        stdResolution            StdResolution,
        taCorrection            INTEGER (0..960)            OPTIONAL,    -- TA correction
        -- measured neighbors in OTD measurements
        otd-MsrsOfOtherSets     SeqOfOTD-MsrsOfOtherSets    OPTIONAL
    }
    SeqOfOTD-MsrsOfOtherSets

TOA_MeasurementsOfRef

    TOA-MeasurementsOfRef ::= SEQUENCE {
        refQuality            RefQuality,
        numOfMeasurements    NumOfMeasurements
    }
    RefQuality

OTD_Measurement

    OTD-Measurement ::= SEQUENCE {
        nborTimeSlot    ModuloTimeSlot,
        eotdQuality        EOTDQuality,
        otdValue        OTDValue
    }
    -- This measurement contains the BTS identity and measurement
    OTD-MeasurementWithID

OTD_MeasurementWithID

    OTD-MeasurementWithID ::=SEQUENCE {
        neighborIdentity    NeighborIdentity,
        nborTimeSlot        ModuloTimeSlot,
        eotdQuality            EOTDQuality,
        otdValue            OTDValue
    }
    EOTDQuality

EOTDQuality

    EOTDQuality ::= SEQUENCE {
        nbrOfMeasurements    INTEGER    (0..7),
        stdOfEOTD            INTEGER (0..31)
    }
    NeighborIdentity

MultiFrameCarrier

    MultiFrameCarrier ::= SEQUENCE {
        bcchCarrier            BCCHCarrier,
        multiFrameOffset    MultiFrameOffset
    }
    -- OTD measurement value for neighbour
    OTDValue

LocationInfo

    LocationInfo ::= SEQUENCE {
        refFrame        INTEGER (0..65535),            -- Reference Frame number
        -- If refFrame is within (42432..65535), it shall be ignored by the receiver
        -- in that case the MS should provide GPS TOW if available
        gpsTOW            INTEGER (0..14399999)    OPTIONAL,    -- GPS TOW
        fixType            FixType,
        -- Note that applicable range for refFrame is 0 - 42431
        -- Possible shapes carried in posEstimate are
        -- ellipsoid point,
        -- ellipsoid point with uncertainty circle
        -- ellipsoid point with uncertainty ellipse
        -- ellipsoid point with altitude and uncertainty ellipsoid
        posEstimate        Ext-GeographicalInformation
    }
    FixType

GPS_MeasureInfo

    GPS-MeasureInfo ::= SEQUENCE {
        -- Measurement info elements
        -- user has to make sure that in this element is number of elements
        -- defined in reference BTS identity
        gpsMsrSetList    SeqOfGPS-MsrSetElement
    }
    SeqOfGPS-MsrSetElement

GPS_MsrSetElement

    GPS-MsrSetElement ::= SEQUENCE {
        refFrame        INTEGER (0..65535)    OPTIONAL,     -- Reference Frame number
        gpsTOW            GPSTOW24b,                        -- GPS TOW
        -- Note that applicable range for refFrame is 0 - 42431
    --N_SAT can be read from number of elements of gps-msrList
        gps-msrList        SeqOfGPS-MsrElement
    }
    -- 24 bit presentation for GPSTOW
    GPSTOW24b

GPS_MsrElement

    GPS-MsrElement ::= SEQUENCE {
        satelliteID        SatelliteID,                -- Satellite identifier
        cNo                INTEGER (0..63),            -- carrier noise ratio
        doppler            INTEGER (-32768..32767),     -- doppler, mulltiply by 0.2
        wholeChips        INTEGER (0..1022),            -- whole value of the code phase measurement
        fracChips        INTEGER (0..1024),            -- fractional value of the code phase measurement
                                                -- a value of 1024 shall not be encoded by the sender
                                                -- the receiver shall consider a value of 1024 to be
                                                -- invalid data
        mpathIndic        MpathIndic,                    -- multipath indicator
        pseuRangeRMSErr    INTEGER (0..63)                -- index
    }
    -- Multipath indicator
    MpathIndic

LocationError

    LocationError ::= SEQUENCE {
        locErrorReason                LocErrorReason,
        additionalAssistanceData    AdditionalAssistanceData    OPTIONAL,
        ...
    }
    LocErrorReason

AdditionalAssistanceData

    AdditionalAssistanceData ::= SEQUENCE {
        gpsAssistanceData        GPSAssistanceData        OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...
    }
    GPSAssistanceData

GPS_AssistData

    GPS-AssistData ::= SEQUENCE {
        controlHeader        ControlHeader
    }
    -- More Assistance Data To Be Sent IE
    -- More Assistance Data Components On the Way indication for delivery of an entire set of assistance
    -- data in multiple Assistance Data components.
    MoreAssDataToBeSent

ControlHeader

    ControlHeader ::= SEQUENCE {
        -- Field type Present information
        referenceTime        ReferenceTime        OPTIONAL,
        refLocation            RefLocation            OPTIONAL,
        dgpsCorrections        DGPSCorrections        OPTIONAL,
        navigationModel        NavigationModel        OPTIONAL,
        ionosphericModel        IonosphericModel        OPTIONAL,
        utcModel            UTCModel            OPTIONAL,
        almanac            Almanac            OPTIONAL,
        acquisAssist        AcquisAssist        OPTIONAL,
        realTimeIntegrity SeqOf-BadSatelliteSet OPTIONAL
    }
    ReferenceTime

ReferenceTime

    ReferenceTime ::= SEQUENCE {
        gpsTime                GPSTime,
        gsmTime                GSMTime                OPTIONAL,
        gpsTowAssist        GPSTOWAssist        OPTIONAL
    }
    -- GPS Time includes week number and time-of-week (TOW)
    GPSTime

GPSTime

    GPSTime ::= SEQUENCE {
        gpsTOW23b            GPSTOW23b,
        gpsWeek                GPSWeek
    }
    -- GPSTOW, range 0-604799.92, resolution 0.08 sec, 23-bit presentation
    GPSTOW23b

GPSTOWAssistElement

    GPSTOWAssistElement ::= SEQUENCE {
        satelliteID            SatelliteID,
        tlmWord                TLMWord,
        antiSpoof            AntiSpoofFlag,
        alert                AlertFlag,
        tlmRsvdBits            TLMReservedBits
    }
    -- TLM Word, 14 bits
    TLMWord

GSMTime

    GSMTime ::= SEQUENCE {
        bcchCarrier        BCCHCarrier,    -- BCCH carrier
        bsic            BSIC,            -- BSIC
        frameNumber        FrameNumber,
        timeSlot        TimeSlot,
        bitNumber        BitNumber
    }
    -- Frame number
    FrameNumber

RefLocation

    RefLocation ::= SEQUENCE {
        threeDLocation            Ext-GeographicalInformation
    }
    -- DGPS Corrections IE
    DGPSCorrections

DGPSCorrections

    DGPSCorrections ::= SEQUENCE {
        gpsTOW        INTEGER (0..604799),    -- DGPS reference time
        status        INTEGER (0..7),
        -- N_SAT can be read from number of elements of satList
        satList        SeqOfSatElement
    }
    SeqOfSatElement

SatElement

    SatElement ::= SEQUENCE {
        satelliteID        SatelliteID,
    --- Sequence number for ephemeris
        iode             INTEGER (0..239),
        -- User Differential Range Error
        udre            INTEGER (0..3),
        -- Pseudo Range Correction, range is
        -- -655.04 - +655.04,
        pseudoRangeCor    INTEGER (-2047..2047),
        -- Pseudo Range Rate Correction, range is
        -- -4.064 - +4.064,
        rangeRateCor    INTEGER (-127..127),
    -- Delta Pseudo Range Correction 2
        deltaPseudoRangeCor2     INTEGER (-127..127),    -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 2
        deltaRangeRateCor2        INTEGER (-7..7),        -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 3
        deltaPseudoRangeCor3     INTEGER (-127..127),    -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 3
        deltaRangeRateCor3        INTEGER (-7..7)            -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
    }
    SatelliteID

NavigationModel

    NavigationModel ::= SEQUENCE {
        navModelList    SeqOfNavModelElement
    }
    -- navigation model satellite list
    SeqOfNavModelElement

NavModelElement

    NavModelElement ::= SEQUENCE {
        satelliteID        SatelliteID,
        satStatus        SatStatus        -- satellite status
    }
    -- the Status of the navigation model
    SatStatus

UncompressedEphemeris

    UncompressedEphemeris ::= SEQUENCE {
        ephemCodeOnL2    INTEGER (0..3),
        ephemURA        INTEGER (0..15),
        ephemSVhealth    INTEGER (0..63),
        ephemIODC        INTEGER    (0..1023),
        ephemL2Pflag    INTEGER (0..1),
        ephemSF1Rsvd    EphemerisSubframe1Reserved,
        ephemTgd        INTEGER (-128..127),
        ephemToc        INTEGER (0..37799),
        ephemAF2        INTEGER (-128..127),
        ephemAF1        INTEGER (-32768..32767),
        ephemAF0        INTEGER (-2097152..2097151),
        ephemCrs        INTEGER (-32768..32767),
        ephemDeltaN        INTEGER (-32768..32767),
        ephemM0            INTEGER (-2147483648..2147483647),
        ephemCuc        INTEGER (-32768..32767),
        ephemE            INTEGER (0..4294967295),
        ephemCus        INTEGER (-32768..32767),
        ephemAPowerHalf    INTEGER (0..4294967295),
        ephemToe        INTEGER (0..37799),
        ephemFitFlag    INTEGER (0..1),
        ephemAODA        INTEGER (0..31),
        ephemCic        INTEGER (-32768..32767),
        ephemOmegaA0    INTEGER (-2147483648..2147483647),
        ephemCis        INTEGER (-32768..32767),
        ephemI0            INTEGER (-2147483648..2147483647),
        ephemCrc        INTEGER (-32768..32767),
        ephemW            INTEGER (-2147483648..2147483647),
        ephemOmegaADot    INTEGER (-8388608..8388607),
        ephemIDot        INTEGER (-8192..8191)
    }
    -- Reserved bits in subframe 1 of navigation message
    EphemerisSubframe1Reserved

EphemerisSubframe1Reserved

    EphemerisSubframe1Reserved ::= SEQUENCE {
        reserved1        INTEGER (0..8388607),    -- 23-bit field
        reserved2        INTEGER (0..16777215),    -- 24-bit field
        reserved3        INTEGER (0..16777215),    -- 24-bit field
        reserved4        INTEGER (0..65535)        -- 16-bit field
    }
    -- Ionospheric Model IE
    IonosphericModel

IonosphericModel

    IonosphericModel ::= SEQUENCE {
        alfa0            INTEGER (-128..127),
        alfa1            INTEGER (-128..127),
        alfa2            INTEGER (-128..127),
        alfa3            INTEGER (-128..127),
        beta0            INTEGER (-128..127),
        beta1            INTEGER (-128..127),
        beta2            INTEGER (-128..127),
        beta3            INTEGER (-128..127)
    }
    -- Universal Time Coordinate Model
    UTCModel

UTCModel

    UTCModel ::= SEQUENCE {
        utcA1            INTEGER (-8388608..8388607),
        utcA0            INTEGER (-2147483648..2147483647),
        utcTot            INTEGER (0..255),
        utcWNt            INTEGER (0..255),
        utcDeltaTls        INTEGER (-128..127),
        utcWNlsf        INTEGER (0..255),
        utcDN            INTEGER (-128..127),
        utcDeltaTlsf    INTEGER (-128..127)
    }
    -- Almanac, Long term model
    -- NOTE: These are parameters are subset of the ephemeris
    -- NOTE: But with reduced resolution and accuracy
    Almanac

Almanac

    Almanac ::= SEQUENCE {
        alamanacWNa        INTEGER (0..255),    -- Once per message
        -- navigation model satellite list.
        -- The size of almanacList is actually Nums_Sats_Total field
        almanacList        SeqOfAlmanacElement
    }
    SeqOfAlmanacElement

AlmanacElement

    AlmanacElement ::= SEQUENCE {
        satelliteID            SatelliteID,
        almanacE            INTEGER (0..65535),
        alamanacToa            INTEGER (0..255),
        almanacKsii            INTEGER (-32768..32767),
        almanacOmegaDot        INTEGER (-32768..32767),
        almanacSVhealth        INTEGER (0..255),
        almanacAPowerHalf    INTEGER (0..16777215),
        almanacOmega0        INTEGER (-8388608..8388607),
        almanacW            INTEGER (-8388608..8388607),
        almanacM0            INTEGER (-8388608..8388607),
        almanacAF0            INTEGER (-1024..1023),
        almanacAF1            INTEGER (-1024..1023)
    }
    -- Acquisition Assistance
    AcquisAssist

AcquisAssist

    AcquisAssist ::= SEQUENCE {
        -- Number of Satellites can be read from acquistList
        timeRelation    TimeRelation,
        -- Acquisition assistance list
        -- The size of Number of Satellites is actually Number of Satellites field
        acquisList        SeqOfAcquisElement
    }
    SeqOfAcquisElement

TimeRelation

    TimeRelation ::= SEQUENCE {
        --
        gpsTOW        GPSTOW23b,        -- 23b presentation
        gsmTime        GSMTime        OPTIONAL
    }
    -- data occuring per number of satellites
    AcquisElement

AcquisElement

    AcquisElement ::= SEQUENCE {
        svid                    SatelliteID,
        -- Doppler 0th order term,
        -- -5120.0 - 5117.5 Hz (= -2048 - 2047 with 2.5 Hz resolution)
        doppler0                INTEGER (-2048..2047),
        addionalDoppler            AddionalDopplerFields    OPTIONAL,
        codePhase                INTEGER (0..1022),    -- Code Phase
        intCodePhase            INTEGER (0..19),    -- Integer Code Phase
        gpsBitNumber            INTEGER (0..3),     -- GPS bit number
        codePhaseSearchWindow    INTEGER (0..15),    -- Code Phase Search Window
        addionalAngle            AddionalAngleFields        OPTIONAL
    }
    AddionalDopplerFields

AddionalDopplerFields

    AddionalDopplerFields ::= SEQUENCE {
        -- Doppler 1st order term, -1.0 - +0.5 Hz/sec
        -- (= -42 + (0 to 63) with 1/42 Hz/sec. resolution)
        doppler1                INTEGER (0..63),
        dopplerUncertainty        INTEGER (0..7)
    }
    AddionalAngleFields

AddionalAngleFields

    AddionalAngleFields    ::= SEQUENCE {
        -- azimuth angle, 0 - 348.75 deg (= 0 - 31 with 11.25 deg resolution)
        azimuth                    INTEGER (0..31),
        -- elevation angle, 0 - 78.75 deg (= 0 - 7 with 11.25 deg resolution)
        elevation                INTEGER (0..7)
    }
    -- Real-Time Integrity
    -- number of bad satellites can be read from this element
    SeqOf-BadSatelliteSet

Rel98_MsrPosition_Req_Extension

    Rel98-MsrPosition-Req-Extension ::= SEQUENCE {
        rel98-Ext-ExpOTD            Rel98-Ext-ExpOTD        OPTIONAL,    -- ExpectedOTD extension
        ...,
        gpsTimeAssistanceMeasurementRequest   NULL   OPTIONAL,
        gpsReferenceTimeUncertainty        GPSReferenceTimeUncertainty   OPTIONAL
    -- Further R98 extensions here
    }
    Rel98-AssistanceData-Extension

Rel98_AssistanceData_Extension

    Rel98-AssistanceData-Extension ::= SEQUENCE {
        rel98-Ext-ExpOTD            Rel98-Ext-ExpOTD        OPTIONAL,    -- ExpectedOTD extension
        ...,
        gpsTimeAssistanceMeasurementRequest   NULL   OPTIONAL,
        gpsReferenceTimeUncertainty    GPSReferenceTimeUncertainty       OPTIONAL
    -- Further R98 extensions here
    }
    -- Release 98 ExpOTD extension
    Rel98-Ext-ExpOTD

Rel98_Ext_ExpOTD

    Rel98-Ext-ExpOTD ::= SEQUENCE {
    -- If MsrAssistBTS is included in message, msrAssistData-R98-ExpOTD shall be included.
        msrAssistData-R98-ExpOTD            MsrAssistData-R98-ExpOTD            OPTIONAL,
    -- If SystemInfoAssistaData is included in message, systemInfoAssistData-R98-ExpOTD shall be
    -- included.
        systemInfoAssistData-R98-ExpOTD    SystemInfoAssistData-R98-ExpOTD    OPTIONAL
    }
    -- MsrAssistData R98 extension
    MsrAssistData-R98-ExpOTD

MsrAssistData_R98_ExpOTD

    MsrAssistData-R98-ExpOTD ::= SEQUENCE {
         msrAssistList-R98-ExpOTD             SeqOfMsrAssistBTS-R98-ExpOTD
    }
    -- Indexes in SeqOfMsrAssistBTS-R98-ExpOTD refer to SeqOfMsrAssistBTS
    -- If the index exceeds the SegOfMsrAssistBTS range or if there is other
    -- inconsistencies between the BTS indices, the MS shall apply protocol
    -- error cause incorrectData
    SeqOfMsrAssistBTS-R98-ExpOTD

MsrAssistBTS_R98_ExpOTD

    MsrAssistBTS-R98-ExpOTD ::= SEQUENCE {
        expectedOTD                ExpectedOTD,
        expOTDUncertainty        ExpOTDUncertainty
    }
    -- SystemInfoAssistData R98 extension
    SystemInfoAssistData-R98-ExpOTD

SystemInfoAssistData_R98_ExpOTD

    SystemInfoAssistData-R98-ExpOTD ::= SEQUENCE {
        systemInfoAssistListR98-ExpOTD     SeqOfSystemInfoAssistBTS-R98-ExpOTD
    }
    -- SeqOfSystemInfoAssistBTS-R98-ExpOTD index refer to SeqOfSystemInfoAssistBTS
    -- If the index exceeds the SegOfSystemInfoAssistBTS range or if there is other
    -- inconsistencies between the BTS indices, the MS shall apply protocol
    -- error cause incorrectData
    SeqOfSystemInfoAssistBTS-R98-ExpOTD

AssistBTSData_R98_ExpOTD

    AssistBTSData-R98-ExpOTD ::= SEQUENCE {
        expectedOTD                ExpectedOTD,
        expOTDuncertainty        ExpOTDUncertainty    -- Uncertainty of expected OTD
    }
    -- Expected OTD value between nbor base station and reference BTS
    -- at MS's current estimated location.
    ExpectedOTD

GPSTimeAssistanceMeasurements

    GPSTimeAssistanceMeasurements ::= SEQUENCE {
        referenceFrameMSB  INTEGER (0 .. 63),                 -- MSB of frame number
        gpsTowSubms        INTEGER (0 .. 9999)   OPTIONAL,     -- in units of 100ns, for MS based AGPS
        deltaTow           INTEGER (0 .. 127)   OPTIONAL,      -- for MS assisted AGPS
        gpsReferenceTimeUncertainty        GPSReferenceTimeUncertainty   OPTIONAL
    }
    Rel-98-MsrPosition-Rsp-Extension

Rel_98_MsrPosition_Rsp_Extension

    Rel-98-MsrPosition-Rsp-Extension ::= SEQUENCE {
        -- First extension to Release 98
        rel-98-Ext-MeasureInfo    SEQUENCE {
            otd-MeasureInfo-R98-Ext    OTD-MeasureInfo-R98-Ext        OPTIONAL
        },
        ...,
        timeAssistanceMeasurements    GPSTimeAssistanceMeasurements   OPTIONAL
        -- Further R98 extensions here
    }
    -- This is an addition to OTD-MeasureInfo element defined in original message,
    -- If OTD-MeasureInfo is absent, or if one or more OTD-MsrElementRest are present
    -- OTD-MeasureInfo-R98-Ext shall be absent.
    -- OTD-MeasureInfo-R98-Ext
    OTD-MeasureInfo-R98-Ext

_0Rel_98_MsrPosition_Rsp_Extension

    SEQUENCE {
    otd-MeasureInfo-R98-Ext    OTD-MeasureInfo-R98-Ext        OPTIONAL
    }

OTD_MeasureInfo_R98_Ext

    OTD-MeasureInfo-R98-Ext ::= SEQUENCE {
        -- Measurement info elements
        otdMsrFirstSets-R98-Ext        OTD-MsrElementFirst-R98-Ext
    }
    -- OTD measurement information Ext for the first set only
    OTD-MsrElementFirst-R98-Ext

OTD_MsrElementFirst_R98_Ext

    OTD-MsrElementFirst-R98-Ext ::= SEQUENCE {
        -- additional measured neighbors in OTD measurements
        otd-FirstSetMsrs-R98-Ext     SeqOfOTD-FirstSetMsrs-R98-Ext     OPTIONAL
    }
    SeqOfOTD-FirstSetMsrs-R98-Ext

Rel_5_MsrPosition_Rsp_Extension

    Rel-5-MsrPosition-Rsp-Extension ::= SEQUENCE {
        extended-reference    Extended-reference     OPTIONAL,
        -- The extended-reference shall be included by the MS if and only if previously
        -- received from the SMLC in a Measure Position Request. When included, the value sent
        -- by the MS shall equal the value received from the SMLC.
        -- extension to Release 5, for RRLP pseudo-segmentation here
        otd-MeasureInfo-5-Ext    OTD-MeasureInfo-5-Ext    OPTIONAL,
        ulPseudoSegInd            UlPseudoSegInd            OPTIONAL,    -- Included when uplink RRLP
        -- Pseudo-segmentation is used, not included when no uplink pseudo-segmentation is used
        ...
                        -- Possibly more extensions for Release 5 here later
    }
    Extended-reference

Extended_reference

    Extended-reference ::= SEQUENCE {
        smlc-code            INTEGER (0..63),
        transaction-ID        INTEGER (0..262143)
    }
    OTD-MeasureInfo-5-Ext

Rel5_MsrPosition_Req_Extension

    Rel5-MsrPosition-Req-Extension ::= SEQUENCE {
        extended-reference            Extended-reference,
        ...
        -- Possibly more extensions for Release 5 here later
    }
    Rel5-AssistanceData-Extension

Rel5_AssistanceData_Extension

    Rel5-AssistanceData-Extension ::= SEQUENCE {
        extended-reference            Extended-reference,
        ...
    -- Possibly more extensions for Release 5 here later
    }
    Rel-5-ProtocolError-Extension

Rel_5_ProtocolError_Extension

    Rel-5-ProtocolError-Extension::= SEQUENCE {
        extended-reference            Extended-reference     OPTIONAL,
        -- The extended-reference shall be included by the MS if and only if previously
        -- received from the SMLC.
        -- When included, the value sent by the MS shall equal the value received from the SMLC.
        ...
        -- Possibly more extensions for Release 5 here later
    }
    END

RRLP_Component

    RRLP-Component ::= CHOICE {
        msrPositionReq            MsrPosition-Req,
        msrPositionRsp            MsrPosition-Rsp,
        assistanceData            AssistanceData,
        assistanceDataAck        NULL,
        protocolError            ProtocolError,
        ...
    }
    -- add this definition to RRLP-Components module
    -- Measurement Position request component
    MsrPosition-Req

MethodType

    MethodType ::= CHOICE {
        msAssisted        AccuracyOpt,    -- accuracy is optional
        msBased            Accuracy,        -- accuracy is mandatory
        msBasedPref        Accuracy,        -- accuracy is mandatory
        msAssistedPref    Accuracy         -- accuracy is mandatory
    }
    -- Accuracy of the location estimation
    AccuracyOpt

SystemInfoAssistBTS

    SystemInfoAssistBTS ::= CHOICE {
        notPresent        NULL,
        present            AssistBTSData
    }
    -- Actual assistance data for system information base station
    AssistBTSData

ReferenceIdentityType

    ReferenceIdentityType ::= CHOICE {
        bsicAndCarrier    BSICAndCarrier,        -- BSIC and Carrier
        ci                CellID,                -- Cell ID, LAC not needed
        requestIndex    RequestIndex,        -- Index to Requested Neighbor List
        systemInfoIndex    SystemInfoIndex,    -- Index to System info list, this type of ref. identity
                                            -- shall not be used by the MS unless it has received
                                            -- the SystemInfoAssistData from the SMLC for this cell.
        ciAndLAC        CellIDAndLAC        -- CI and LAC
    }
    BSICAndCarrier

OTD_MsrsOfOtherSets

    OTD-MsrsOfOtherSets ::= CHOICE {
        identityNotPresent    OTD-Measurement,
        identityPresent        OTD-MeasurementWithID
    }
    -- For this OTD measurement identity is same as the identity of BTS
    -- in the first set with same sequence number
    OTD-Measurement

NeighborIdentity

    NeighborIdentity ::= CHOICE {
        bsicAndCarrier        BSICAndCarrier,        -- BSIC and Carrier
        ci                    CellID,                -- Cell ID, LAC not needed
        multiFrameCarrier    MultiFrameCarrier,     -- MultiFrameOffest and BSIC
        requestIndex        RequestIndex,        -- Index to Requested Neighbor List
        systemInfoIndex        SystemInfoIndex,    -- Index to System info list, this type of neighbour
                                                -- identity shall not be used by the MS unless it has
                                                -- received the SystemInfoAssistData from the SMLC for
                                                -- this cell.
        ciAndLAC            CellIDAndLAC        -- CI and LAC
    }
    -- Multiframe and carrier
    MultiFrameCarrier

SatStatus

    SatStatus ::= CHOICE {
        -- New satellite, new Navigation Model
        newSatelliteAndModelUC    UncompressedEphemeris,
        -- Existing satellite, Existing Navigation Model
        oldSatelliteAndModel    NULL,
        -- Existing satellite, new Navigation Model
        newNaviModelUC            UncompressedEphemeris,
        ...
    }
    -- Uncompressed satellite emhemeris and clock corrections
    UncompressedEphemeris

SystemInfoAssistBTS_R98_ExpOTD

    SystemInfoAssistBTS-R98-ExpOTD ::= CHOICE {
        notPresent        NULL,
        present            AssistBTSData-R98-ExpOTD
    }
    -- This element completes AssistBTSData IE
    AssistBTSData-R98-ExpOTD

maxNumOfPrivateExtensions

    const integer maxNumOfPrivateExtensions  INTEGER ::= 10
    ExtensionSet

maxExt_GeographicalInformation

    const integer maxExt-GeographicalInformation  INTEGER ::= 20
    -- the maximum length allows for further shapes in GSM 03.32 to be included in later versions
    -- of GSM 09.02
    -- Information Elements copied from TS 29002-750
    -- MAP-LCS-DataTypes {
    --    itu-t identified-organization (4) etsi (0) mobileDomain (0)
    --    gsm-Network (1) modules (3) map-LCS-DataTypes (25) version10 (10)}
    VelocityEstimate

FixType_twoDFix_

    const FixType twoDFix (0)

FixType_threeDFix_

    const FixType threeDFix (1)

maxGPSAssistanceData

    const integer maxGPSAssistanceData    INTEGER ::= 40
    -- Protocol Error Causes
    ErrorCodes

© Copyright Testing Technologies IST GmbH 2012