OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_13x.TC_131

Declared in module SUPL_V2_SET_INITIATED_Tests
Subgroups: TC_131_1, TC_131_2

Test cases Summary
TC_131_1_1 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_131_1_2 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_131_1_3 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_131_1_4 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_131_2_1 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
TC_131_2_2 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
TC_131_2_3 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
TC_131_2_4 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type

## Details

TC_131_1_1

    testcase TC_131_1_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
Purpose: SUPL-2.0-con-131-1-1 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 1: Entering event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 1: Entering event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 1: Entering event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: - Case 1: The SET does not respond as Entering event has not been met. 5. Do nothing (Step only applies to cases 2 and 3) 6. At some time: Case 1 and Case 4: - Case 1: The SET does not respond as Entering event has not been met. 7. Do nothing (Step only applies to cases 2 and 3) 8. Do nothing (Step only applies to cases 2 and 3) 9. Case 1 and Case 4: 120 seconds after step 2: Case 1: force a cellular handover to the GSM or WCDMA Cell ID that is normally used for testing. 10. Case 1 and Case 4: At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 11. Case 1 and Case 4: Case 1: The SET displays the calculated position estimate as Entering event has been met. 12. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 1 and Case 4 the SET shall not respond 4. At step 6: Case 1 and Case 4 the SET shall not respond 7. At step 10: Case 1 and Case 4 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully 8. At step 11: Case 1 and Case 4 the SET shall display the calculated position estimate 9. At step 12: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2.
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_2

    testcase TC_131_1_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
Purpose: SUPL-2.0-con-131-1-2 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 2: Inside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 2: Inside event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in the Area ID list. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 2: Inside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 2: Inside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: - Case 2: The SET displays the calculated position estimate as Inside event has been met 6. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. After at least 60 seconds (set by Minimum Interval Time) after step 5: - Case 2: The SET displays the calculated position estimate as Inside event has been met 8. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more sequence as detailed below may take place before this occurs. If Stop Time is not supported the following sequence takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. Case 2: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Inside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 3. At step 5: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 4 if Start Time is not supported 4. At step 6: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 6. At step 8: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END - The SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. - After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_3

    testcase TC_131_1_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
Purpose: SUPL-2.0-con-131-1-3 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 3: Outside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 3: Outside event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The cell that is normally used for testing is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 3: Outside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 3: Outside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: - Case 3: The SET displays the calculated position estimate as Outside event has been met 6. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. After at least 60 seconds (set by Minimum Interval Time) after step 5: - Case 3: The SET displays the calculated position estimate as Outside event has been met 8. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more sequence as detailed below may take place before this occurs. If Stop Time is not supported the following sequence takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. Case 3: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Outside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 3. At step 5: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 4 if Start Time is not supported 4. At step 6: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 6. At step 8: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END - The SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. - After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_4

    testcase TC_131_1_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
Purpose: SUPL-2.0-con-131-1-4 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 4: Leaving event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 4: Leaving event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in Area ID list. The SET then handsover to a cell that is not normally used for testing and that is not present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 4: Leaving event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 4: Leaving event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 1 and Case 4: - Case 4: The SET does not respond as Leaving event has not been met 5. Do nothing (Applies only to Case 2 and Case 3) 6. At some time: - Case 4: The SET does not respond as Leaving event has not been met 7. Do nothing (Applies only to Case 2 and Case 3) 8. Do nothing (Applies only to Case 2 and Case 3) 9. Case 1 and Case 4: 120 seconds after step 2: Case 4: force a cellular handover to a GSM or WCDMA Cell ID that is not normally used for testing. 10. Case 1 and Case 4: At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 11. Case 1 and Case 4: Case 4: The SET displays the calculated position estimate as Leaving event has been met. 12. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 1: 2. At step 4: Case 1 and Case 4 the SET shall not respond 4. At step 6: Case 1 and Case 4 the SET shall not respond 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 7. At step 10: Case 1 and Case 4 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully 8. At step 11: Case 1 and Case 4 the SET shall display the calculated position estimate 9. At step 12: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2.
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_1

    testcase TC_131_2_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
Purpose: SUPL-2.0-con-131-2-1 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 1: Entering event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 1: Entering event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 1: Entering event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 1: The SET does not respond as Entering event has not been met. 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 1: The SET does not respond as Entering event has not been met. 17. Do nothing (Applies only to Case 2 and Case 3) 18. Case 1 and Case 4: 120 seconds after step 3: Case 1: force a cellular handover to the GSM or WCDMA Cell ID that is normally used for testing. 19. Case 1 and Case 4: Case 1: The SET displays the calculated position estimate as Entering event has been met. 20. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 1and Case 4: The SET shall not display the position estimate. 11. At step 16: Case 1 and Case 4 the SET shall not respond 13: At step 19: Case 1 and Case 4 the SET shall display the calculated position estimate. 14. At step 20: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_2

    testcase TC_131_2_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
Purpose: SUPL-2.0-con-131-2-2 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 2: Inside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. Case 2: Inside event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in the Area ID list. Figure 2: Case 2: SET is inside area 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 2: Inside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 2: Inside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 2: The SET displays the calculated position estimate as Inside event has been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 2: The SET displays the calculated position estimate as Inside event has been met 17. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more display of the calculated position estimate as detailed below may take place before this occurs. If Stop Time is not supported the following takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Case 2: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Inside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 2 and Case 3 The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 11. At step 16: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 15 12. At step 17: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_3

    testcase TC_131_2_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
Purpose: SUPL-2.0-con-131-2-3 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 3: Outside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 3: Outside event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The cell that is normally used for testing is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 3: Outside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 3: Outside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 3: The SET displays the calculated position estimate as Outside event has been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 3: The SET displays the calculated position estimate as Outside event has been met 17. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more display of the calculated position estimate as detailed below may take place before this occurs. If Stop Time is not supported the following takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Case 3: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Outside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 2 and Case 3 The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 11. At step 16: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 15 12. At step 17: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_4

    testcase TC_131_2_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type
Purpose: SUPL-2.0-con-131-2-4 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 4: Leaving event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 4: Leaving event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in Area ID list. The SET then handsover to a cell that is not normally used for testing and that is not present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 4: Leaving event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 4: Leaving event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 4: The SET does not respond as Leaving event has not been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 4: The SET does not respond as Leaving event has not been met 17. Do nothing (Only applies to Case 2 and Case 3) 18. Case 1 and Case 4: 120 seconds after step 3: Case 4: force a cellular handover to a GSM or WCDMA Cell ID that is not normally used for testing. 19. Case 1 and Case 4: Case 4: The SET displays the calculated position estimate as Leaving event has been met. 20. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 1and Case 4: The SET shall not display the position estimate. 11. At step 16: Case 1 and Case 4 the SET shall not respond 13: At step 19: Case 1 and Case 4 the SET shall display the calculated position estimate. 14. At step 20: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012