OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test Cases Modules

LETTER INDEX

TC_000_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports SUPL INIT delivery using OMA Push and, if supported, MT SMS and, or SIP Push Test 4: ics_UDP
TC_001 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_002 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_003 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_005 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_006 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_007_1 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_2 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_3 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_4 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_5 | testcase declared in SUPL_V2_COMMON_Tests
TC_008_1 | testcase declared in SUPL_V2_COMMON_Tests
TC_008_2 | testcase declared in SUPL_V2_COMMON_Tests To test SET correctly uses optional ciphering suites Test 2: ics_PSKTLS_add_cipher
TC_009_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 1: Correct support
TC_009_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 2: Correct discard procedure � incorrect Protection Level
TC_009_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 3: Correct discard procedure � incorrect Key Identity
TC_009_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 4: Correct discard procedure � incorrect Basic Replay Counter
TC_010_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL message - Test 1: Support for higher versions of SUPL 2_X_X
TC_010_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accept compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
TC_010_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accept compatible Version numbers in SUPL messages - Test 3: Correct support with SLP supporting SUPL V3_0 and V2_0
TC_010_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL message - Test 4: Correct support with SLP supporting SUPL V1_0 only, SUPL V1_0 supported by SET
TC_011_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects unsupported Version number in SUPL messages - Test1: Higher version not supported
TC_011_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects unsupported Version number in SUPL messages - Test 2: Lower Version not supportet, SUPL V1_0 not supported by SET
TC_012 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects incorrect UDP message content
TC_020 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_021 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_5 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_6 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_023 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_025_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_025_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_10 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 10: Autonomous GNSS
TC_030_11 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_12_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS Preferred methods
TC_030_12_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS Preferred methods
TC_030_13 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 13: OTDOA
TC_030_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_5 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_7 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_030_9 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based only - GLONASS
TC_031 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_033_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 1: E-SLP address sent in SUPL INIT
TC_033_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 2: Use of provisioned H-SLP address
TC_033_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 3: Use of default E-SLP address
TC_034_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions an Emergency Services Location Request when a normal SUPL session is also active Case 1: Normal SUPL session already in progress before Emergency SUPL session
TC_034_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions an Emergency Services Location Request when a normal SUPL session is also active Case 2: Normal SUPL session attempted during Emergency SUPL session
TC_040_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Real Time Periodic reporting - Test 1: A-GPS SET assisted
TC_040_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Real Time Periodic reporting - Test 2: A-GPS SET based
TC_041_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs basic Quasi Real Time Periodic reporting Test 2: A-GPS SET based
TC_042_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_042_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_042_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_050_1_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_050_1_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_050_1_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_050_1_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_050_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
TC_050_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
TC_050_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
TC_050_2_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_051_1_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_051_1_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_051_1_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_051_1_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_051_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 1: Entering event type
TC_051_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 2: Inside event type
TC_051_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 3: Outside event type
TC_051_2_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_061 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions when the Network cancels a Triggered Location Request
TC_065_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_065_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session).
TC_070_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session).
TC_071_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_071_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET coorectly actions timer UT3 - Test 2: Triggered session.
TC_072 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_073 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT7
TC_074 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT8
TC_100_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_100_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_100_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_101 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_102 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_103_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
TC_103_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
TC_110_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_10 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
TC_110_11_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_11_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_12_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_12_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_13 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 13: OTDOA
TC_110_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_5 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_7 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_110_9 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
TC_130_1_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_130_1_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_130_1_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_130_1_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_130_2_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
TC_130_2_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
TC_130_2_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
TC_130_2_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Leaving event type
TC_131_1_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_131_1_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_131_1_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_131_1_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_131_2_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
TC_131_2_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
TC_131_2_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
TC_131_2_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_140_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_140_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT1 - Test 2: Triggered Session
TC_141_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_141_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
TC_141_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
TC_141_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
TC_142_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_142_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT3 - Test 2: Triggered Session
TC_143 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT7

© Copyright Testing Technologies IST GmbH 2012