OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module MAP_SS_DataTypes_V10

Import Declarations:

- MAP_CommonDataTypes_V10
  all
- ASNAUX
  all
- MAP_BS_Code_V10
  all
- MAP_SS_Code_V10
  all
- MAP_TS_Code_V10
  all
- MAP_ExtensionDataTypes_V10
  all

Data Types Summary
NoReplyConditionTime |
ForwardingFeatureList |
SS_Status |
ForwardingOptions |
CallBarringFeatureList |
CCBS_FeatureList |
CCBS_Index |
USSD_DataCodingScheme |
USSD_String |
Password |
SS_List |
SS_InfoList |
BasicServiceGroupList |
SS_EventSpecification |
ServiceIndicator |
CliRestrictionOption |
OverrideCategory |
GuidanceInfo |
CCBS_RequestState |
RegisterSS_Arg |
ForwardingInfo |
ForwardingFeature |
CallBarringInfo |
CallBarringFeature |
SS_Data |
SS_ForBS_Code |
GenericServiceInfo |
CCBS_Feature |
USSD_Arg |
USSD_Res |
SS_InvocationNotificationArg |
SS_InvocationNotificationRes |
RegisterCC_EntryArg |
CCBS_Data |
RegisterCC_EntryRes |
EraseCC_EntryArg |
EraseCC_EntryRes |
SS_Info |
SS_SubscriptionOption |
InterrogateSS_Res |

Constants Summary
maxNumOfCCBS_Requests |
maxUSSD_StringLength |
maxNumOfSS |
maxNumOfBasicServiceGroups |
maxEventSpecification |
ServiceIndicator_camel_invoked_ |
ServiceIndicator_clir_invoked_ |

## Details

NoReplyConditionTime

    NoReplyConditionTime ::= INTEGER (5..30)
    SS-Info

ForwardingFeatureList

    ForwardingFeatureList ::=
         SEQUENCE SIZE (1..maxNumOfBasicServiceGroups) OF
                                              ForwardingFeature
    ForwardingFeature

SS_Status

    SS-Status ::= OCTET STRING (SIZE (1))
         -- bits 8765: 0000 (unused)
         -- bits 4321: Used to convey the "P bit","R bit","A bit" and "Q bit",
         --            representing supplementary service state information
         --            as defined in TS 3GPP TS 23.011 [22]
         -- bit 4: "Q bit"
         -- bit 3: "P bit"
         -- bit 2: "R bit"
         -- bit 1: "A bit"
    ForwardingOptions

ForwardingOptions

    ForwardingOptions ::= OCTET STRING (SIZE (1))
         -- bit 8: notification to forwarding party
         --   0 no notification
         --   1 notification
         -- bit 7: redirecting presentation
         --   0 no presentation
         --   1 presentation
         -- bit 6: notification to calling party
         --   0 no notification
         --   1 notification
         -- bit 5: 0 (unused)
         -- bits 43: forwarding reason
         --   00 ms not reachable
         --   01 ms busy
         --   10 no reply
         --   11 unconditional when used in a SRI Result,
         --       or call deflection when used in a RCH Argument
         -- bits 21: 00 (unused)
    CallBarringInfo

CallBarringFeatureList

    CallBarringFeatureList ::= SEQUENCE SIZE (1..maxNumOfBasicServiceGroups) OF
                                              CallBarringFeature
    CallBarringFeature

CCBS_FeatureList

    CCBS-FeatureList ::= SEQUENCE SIZE (1..maxNumOfCCBS-Requests) OF
                                              CCBS-Feature
    maxNumOfCCBS-Requests

CCBS_Index

    CCBS-Index  ::= INTEGER (1..maxNumOfCCBS-Requests)
    InterrogateSS-Res

USSD_DataCodingScheme

    USSD-DataCodingScheme ::= OCTET STRING (SIZE (1))
         -- The structure of the USSD-DataCodingScheme is defined by
         -- the Cell Broadcast Data Coding Scheme as described in
         -- TS 3GPP TS 23.038 [25]
    USSD-String

USSD_String

    USSD-String ::= OCTET STRING (SIZE (1..maxUSSD-StringLength))
         -- The structure of the contents of the USSD-String is dependent
         -- on the USSD-DataCodingScheme as described in TS 3GPP TS 23.038 [25].
    maxUSSD-StringLength

Password

    Password ::= NumericString
         (FROM ("0"|"1"|"2"|"3"|"4"|"5"|"6"|"7"|"8"|"9"))
         (SIZE (4))
    GuidanceInfo

SS_List

    SS-List ::= SEQUENCE SIZE (1..maxNumOfSS) OF
                                              SS-Code
    maxNumOfSS

SS_InfoList

    SS-InfoList ::= SEQUENCE SIZE (1..maxNumOfSS) OF
                                              SS-Info
    BasicServiceGroupList

BasicServiceGroupList

    BasicServiceGroupList ::= SEQUENCE SIZE (1..maxNumOfBasicServiceGroups) OF
                                              BasicServiceCode
    maxNumOfBasicServiceGroups

SS_EventSpecification

    SS-EventSpecification ::= SEQUENCE SIZE (1..maxEventSpecification) OF
                                              AddressString
    maxEventSpecification

ServiceIndicator

    ServiceIndicator ::= BIT STRING {
         clir-invoked (0),
         camel-invoked (1)} (SIZE(2..32))
         -- exception handling:
         -- bits 2 to 31 shall be ignored if received and not understood
    RegisterCC-EntryRes

CliRestrictionOption

    ENUMERATED {
     permanent (0),
     temporaryDefaultRestricted (1),
     temporaryDefaultAllowed (2)}
    OverrideCategory

OverrideCategory

    ENUMERATED {
     overrideEnabled (0),
     overrideDisabled (1)}
    SS-ForBS-Code

GuidanceInfo

    ENUMERATED {
     enterPW (0),
     enterNewPW (1),
     enterNewPW-Again (2)}
     -- How this information is really delivered to the subscriber
     -- (display, announcement, ...) is not part of this
     -- specification.
    SS-List

CCBS_RequestState

    ENUMERATED {
     request (0),
     recall    (1),
     active    (2),
     completed (3),
     suspended (4),
     frozen    (5),
     deleted (6)
     }
    SS-InvocationNotificationRes

RegisterSS_Arg

    RegisterSS-Arg ::= SEQUENCE {
         ss-Code                              SS-Code,
         basicService                         BasicServiceCode                  OPTIONAL,
         forwardedToNumber                    [4] AddressString                 OPTIONAL,
         forwardedToSubaddress                [6] ISDN-SubaddressString         OPTIONAL,
         noReplyConditionTime                 [5] NoReplyConditionTime          OPTIONAL,
         ...,
         defaultPriority                      [7] EMLPP-Priority                OPTIONAL,
         nbrUser                              [8] MC-Bearers                    OPTIONAL,
         longFTN-Supported                    [9] NULL                          OPTIONAL }
    NoReplyConditionTime

ForwardingInfo

    ForwardingInfo ::= SEQUENCE {
         ss-Code                              SS-Code                           OPTIONAL,
         forwardingFeatureList                ForwardingFeatureList,
         ...}
    ForwardingFeatureList

ForwardingFeature

    ForwardingFeature ::= SEQUENCE {
         basicService                         BasicServiceCode                  OPTIONAL,
         ss-Status                            [4] SS-Status                     OPTIONAL,
         forwardedToNumber                    [5] ISDN-AddressString            OPTIONAL,
         forwardedToSubaddress                [8] ISDN-SubaddressString         OPTIONAL,
         forwardingOptions                    [6] ForwardingOptions             OPTIONAL,
         noReplyConditionTime                 [7] NoReplyConditionTime          OPTIONAL,
         ...,
         longForwardedToNumber                [9] FTN-AddressString             OPTIONAL }
    SS-Status

CallBarringInfo

    CallBarringInfo ::= SEQUENCE {
         ss-Code                              SS-Code                           OPTIONAL,
         callBarringFeatureList               CallBarringFeatureList,
         ...}
    CallBarringFeatureList

CallBarringFeature

    CallBarringFeature ::= SEQUENCE {
         basicService                         BasicServiceCode                  OPTIONAL,
         ss-Status [4] SS-Status              OPTIONAL,
         ...}
    SS-Data

SS_Data

    SS-Data ::= SEQUENCE {
         ss-Code                              SS-Code                           OPTIONAL,
         ss-Status                            [4] SS-Status                     OPTIONAL,
         ss-SubscriptionOption                SS-SubscriptionOption             OPTIONAL,
         basicServiceGroupList                BasicServiceGroupList             OPTIONAL,
         ...,
         defaultPriority                      EMLPP-Priority                    OPTIONAL,
         nbrUser                              [5] MC-Bearers                    OPTIONAL
         }
    SS-SubscriptionOption

SS_ForBS_Code

    SS-ForBS-Code ::= SEQUENCE {
         ss-Code                              SS-Code,
         basicService                         BasicServiceCode                  OPTIONAL,
         ...,
         longFTN-Supported                    [4]   NULL                        OPTIONAL }
    GenericServiceInfo

GenericServiceInfo

    GenericServiceInfo ::= SEQUENCE {
         ss-Status SS-Status,
         cliRestrictionOption                 CliRestrictionOption              OPTIONAL,
         ...,
         maximumEntitledPriority              [0]  EMLPP-Priority               OPTIONAL,
         defaultPriority                      [1]  EMLPP-Priority               OPTIONAL,
         ccbs-FeatureList                     [2]  CCBS-FeatureList             OPTIONAL,
         nbrSB                                [3]  MaxMC-Bearers                OPTIONAL,
         nbrUser                              [4]  MC-Bearers                   OPTIONAL,
         nbrSN                                [5]  MC-Bearers                   OPTIONAL }
    CCBS-FeatureList

CCBS_Feature

    CCBS-Feature ::= SEQUENCE {
         ccbs-Index                           [0]  CCBS-Index                   OPTIONAL,
         b-subscriberNumber                   [1]  ISDN-AddressString           OPTIONAL,
         b-subscriberSubaddress               [2]  ISDN-SubaddressString        OPTIONAL,
         basicServiceGroup                    [3]  BasicServiceCode             OPTIONAL,
         ...}
    CCBS-Index

USSD_Arg

    USSD-Arg ::= SEQUENCE {
         ussd-DataCodingScheme                USSD-DataCodingScheme,
         ussd-String                          USSD-String,
         ... ,
         alertingPattern                      AlertingPattern                   OPTIONAL,
         msisdn                               [0] ISDN-AddressString            OPTIONAL }
    USSD-Res

USSD_Res

    USSD-Res ::= SEQUENCE {
         ussd-DataCodingScheme                USSD-DataCodingScheme,
         ussd-String                          USSD-String,
         ...}
    USSD-DataCodingScheme

SS_InvocationNotificationArg

    SS-InvocationNotificationArg ::= SEQUENCE {
         imsi                                 [0] IMSI,
         msisdn                               [1] ISDN-AddressString,
         ss-Event                             [2] SS-Code,
         -- The following SS-Code values are allowed :
         -- ect                               SS-Code ::= '00110001'B
         -- multiPTY                          SS-Code ::= '01010001'B
         -- cd                                SS-Code ::= '00100100'B
         -- ccbs                              SS-Code ::= '01000100'B
         ss-EventSpecification                [3] SS-EventSpecification       OPTIONAL,
         extensionContainer                   [4] ExtensionContainer          OPTIONAL,
         ...,
         b-subscriberNumber                   [5] ISDN-AddressString          OPTIONAL,
         ccbs-RequestState                    [6] CCBS-RequestState           OPTIONAL
         }
    CCBS-RequestState

SS_InvocationNotificationRes

    SS-InvocationNotificationRes ::= SEQUENCE {
         extensionContainer                   ExtensionContainer              OPTIONAL,
         ...
         }
    SS-EventSpecification

RegisterCC_EntryArg

    RegisterCC-EntryArg ::= SEQUENCE {
         ss-Code                              [0]  SS-Code,
         ccbs-Data                            [1]  CCBS-Data                  OPTIONAL,
         ...}
    CCBS-Data

CCBS_Data

    CCBS-Data ::= SEQUENCE {
         ccbs-Feature                         [0]  CCBS-Feature,
         translatedB-Number                   [1]  ISDN-AddressString,
         serviceIndicator                     [2]  ServiceIndicator           OPTIONAL,
         callInfo                             [3]  ExternalSignalInfo,
         networkSignalInfo                    [4]  ExternalSignalInfo,
         ...}
    ServiceIndicator

RegisterCC_EntryRes

    RegisterCC-EntryRes ::= SEQUENCE {
         ccbs-Feature                         [0] CCBS-Feature                OPTIONAL,
         ...}
    EraseCC-EntryArg

EraseCC_EntryArg

    EraseCC-EntryArg ::= SEQUENCE {
         ss-Code                              [0]  SS-Code,
         ccbs-Index                           [1]  CCBS-Index                 OPTIONAL,
         ...}
    EraseCC-EntryRes

EraseCC_EntryRes

    EraseCC-EntryRes ::= SEQUENCE {
         ss-Code                              [0] SS-Code,
         ss-Status                            [1] SS-Status                   OPTIONAL,
         ...}
    END

SS_Info

    SS-Info ::= CHOICE {
         forwardingInfo                       [0] ForwardingInfo,
         callBarringInfo                      [1] CallBarringInfo,
         ss-Data                              [3] SS-Data}
    ForwardingInfo

SS_SubscriptionOption

    SS-SubscriptionOption ::= CHOICE {
         cliRestrictionOption                 [2] CliRestrictionOption,
         overrideCategory                     [1] OverrideCategory}
    CliRestrictionOption

InterrogateSS_Res

    InterrogateSS-Res ::= CHOICE {
         ss-Status                            [0] SS-Status,
         basicServiceGroupList                [2] BasicServiceGroupList,
         forwardingFeatureList                [3] ForwardingFeatureList,
         genericServiceInfo                   [4] GenericServiceInfo }
    USSD-Arg

maxNumOfCCBS_Requests

    const integer maxNumOfCCBS-Requests   INTEGER ::= 5
    CCBS-Feature

maxUSSD_StringLength

    const integer maxUSSD-StringLength   INTEGER ::= 160
    Password

maxNumOfSS

    const integer maxNumOfSS  INTEGER ::= 30
    SS-InfoList

maxNumOfBasicServiceGroups

    const integer maxNumOfBasicServiceGroups   INTEGER ::= 13
    SS-InvocationNotificationArg

maxEventSpecification

    const integer maxEventSpecification   INTEGER ::= 2
    RegisterCC-EntryArg

ServiceIndicator_camel_invoked_

    const ServiceIndicator camel-invoked (1)

ServiceIndicator_clir_invoked_

    const ServiceIndicator clir-invoked (0)

© Copyright Testing Technologies IST GmbH 2012