OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module RRLP_Components_V10

Import Declarations:

- MAP_CommonDataTypes_V10
  all
- ASNAUX
  all
- MAP_BS_Code_V10
  all
- MAP_SS_Code_V10
  all
- MAP_LCS_DataTypes_V10
  all
- MAP_OM_DataTypes_V10
  all
- MAP_ER_DataTypes_V10
  all
- MAP_SM_DataTypes_V10
  all
- MAP_TS_Code_V10
  all
- MAP_SS_DataTypes_V10
  all
- MAP_MS_DataTypes_V10
  all
- MAP_ExtensionDataTypes_V10
  all

Data Types Summary
Accuracy |
MeasureResponseTime |
BTSPosition |
BCCHCarrier |
BSIC |
ModuloTimeSlot |
SeqOfMsrAssistBTS |
MultiFrameOffset |
RoughRTD |
SeqOfSystemInfoAssistBTS |
FineRTD |
RelDistance |
RelativeAlt |
_0MultipleSets0 |
_0MultipleSets |
SeqOfReferenceIdentityType |
RequestIndex |
SystemInfoIndex |
CellID |
LAC |
SeqOfOTD_MsrElementRest |
_0OTD_MsrElementFirst0 |
_0OTD_MsrElementFirst |
SeqOfOTD_FirstSetMsrs |
_0OTD_MsrElementRest0 |
_0OTD_MsrElementRest |
SeqOfOTD_MsrsOfOtherSets |
RefQuality |
NumOfMeasurements |
StdResolution |
OTD_FirstSetMsrs |
_0EOTDQuality |
_0EOTDQuality0 |
OTDValue |
_0LocationInfo |
_0LocationInfo0 |
FixType |
SeqOfGPS_MsrSetElement |
_0GPS_MsrSetElement |
GPSTOW24b |
SeqOfGPS_MsrElement |
_0GPS_MsrElement0 |
_0GPS_MsrElement1 |
_0GPS_MsrElement2 |
_0GPS_MsrElement3 |
_0GPS_MsrElement |
GPSAssistanceData |
GANSSAssistanceData |
GPSTOW23b |
GPSWeek |
GPSTOWAssist |
TLMWord |
AntiSpoofFlag |
AlertFlag |
TLMReservedBits |
FrameNumber |
TimeSlot |
BitNumber |
_0DGPSCorrections |
_0DGPSCorrections0 |
SeqOfSatElement |
_0SatElement0 |
_0SatElement1 |
_0SatElement2 |
_0SatElement3 |
_0SatElement4 |
_0SatElement5 |
_0SatElement6 |
_0SatElement |
SatelliteID |
SeqOfNavModelElement |
_0UncompressedEphemeris0 |
_0UncompressedEphemeris17 |
_0UncompressedEphemeris16 |
_0UncompressedEphemeris15 |
_0UncompressedEphemeris14 |
_0UncompressedEphemeris13 |
_0UncompressedEphemeris12 |
_0UncompressedEphemeris11 |
_0UncompressedEphemeris10 |
_0UncompressedEphemeris |
_0UncompressedEphemeris19 |
_0UncompressedEphemeris18 |
_0UncompressedEphemeris20 |
_0UncompressedEphemeris26 |
_0UncompressedEphemeris9 |
_0UncompressedEphemeris25 |
_0UncompressedEphemeris22 |
_0UncompressedEphemeris21 |
_0UncompressedEphemeris24 |
_0UncompressedEphemeris23 |
_0UncompressedEphemeris1 |
_0UncompressedEphemeris2 |
_0UncompressedEphemeris3 |
_0UncompressedEphemeris4 |
_0UncompressedEphemeris5 |
_0UncompressedEphemeris6 |
_0UncompressedEphemeris7 |
_0UncompressedEphemeris8 |
_0EphemerisSubframe1Reserved |
_0EphemerisSubframe1Reserved0 |
_0EphemerisSubframe1Reserved1 |
_0EphemerisSubframe1Reserved2 |
_0IonosphericModel4 |
_0IonosphericModel3 |
_0IonosphericModel6 |
_0IonosphericModel5 |
_0IonosphericModel0 |
_0IonosphericModel2 |
_0IonosphericModel1 |
_0IonosphericModel |
_0UTCModel6 |
_0UTCModel0 |
_0UTCModel1 |
_0UTCModel2 |
_0UTCModel |
_0UTCModel3 |
_0UTCModel4 |
_0UTCModel5 |
_0Almanac |
SeqOfAlmanacElement |
_0AlmanacElement8 |
_0AlmanacElement9 |
_0AlmanacElement |
_0AlmanacElement6 |
_0AlmanacElement7 |
_0AlmanacElement4 |
_0AlmanacElement5 |
_0AlmanacElement2 |
_0AlmanacElement3 |
_0AlmanacElement0 |
_0AlmanacElement1 |
SeqOfAcquisElement |
_0AcquisElement3 |
_0AcquisElement0 |
_0AcquisElement1 |
_0AcquisElement2 |
_0AcquisElement |
_0AddionalDopplerFields0 |
_0AddionalDopplerFields |
_0AddionalAngleFields0 |
_0AddionalAngleFields |
SeqOf_BadSatelliteSet |
SeqOfMsrAssistBTS_R98_ExpOTD |
SeqOfSystemInfoAssistBTS_R98_ExpOTD |
ExpectedOTD |
ExpOTDUncertainty |
GPSReferenceTimeUncertainty |
_0GPSTimeAssistanceMeasurements |
_0GPSTimeAssistanceMeasurements1 |
_0GPSTimeAssistanceMeasurements0 |
SeqOfOTD_FirstSetMsrs_R98_Ext |
_0Extended_reference0 |
_0Extended_reference |
OTD_MeasureInfo_5_Ext |
GANSSPositioningMethod |
SeqOfGANSSGenericAssistDataElement |
_0GANSSGenericAssistDataElement |
_0GANSSGenericAssistDataElement0 |
_0GANSSRefTimeInfo0 |
_0GANSSRefTimeInfo |
GANSSTOD |
GANSSTODUncertainty |
_0GANSSReferenceTime_R10_Ext |
FrameDrift |
_0GANSSIonosphereModel |
_0GANSSIonosphereModel0 |
_0GANSSIonosphereModel1 |
_0GANSSIonoStormFlags |
_0GANSSIonoStormFlags0 |
_0GANSSIonoStormFlags1 |
_0GANSSIonoStormFlags2 |
_0GANSSIonoStormFlags3 |
_0GANSSAddIonosphericModel |
_0GANSSEarthOrientParam5 |
_0GANSSEarthOrientParam |
_0GANSSEarthOrientParam1 |
_0GANSSEarthOrientParam2 |
_0GANSSEarthOrientParam3 |
_0GANSSEarthOrientParam4 |
_0GANSSEarthOrientParam0 |
SeqOfGANSSTimeModel |
_0GANSSTimeModelElement1 |
_0GANSSTimeModelElement0 |
_0GANSSTimeModelElement |
TA0 |
TA1 |
TA2 |
SeqOfGANSSTimeModel_R10_Ext |
_0GANSSTimeModelElement_R10_Ext0 |
_0GANSSTimeModelElement_R10_Ext |
_0GANSSDiffCorrections |
SeqOfSgnTypeElement |
_0SgnTypeElement |
GANSSSignalID |
SeqOfDGANSSSgnElement |
_0DGANSSSgnElement0 |
_0DGANSSSgnElement1 |
_0DGANSSSgnElement2 |
_0DGANSSSgnElement |
SVID |
_0GANSSNavModel |
SeqOfGANSSSatelliteElement |
_0GANSSSatelliteElement1 |
_0GANSSSatelliteElement0 |
_0GANSSSatelliteElement |
_0GANSSSatelliteElement2 |
_0NavModel_KeplerianSet8 |
_0NavModel_KeplerianSet7 |
_0NavModel_KeplerianSet6 |
_0NavModel_KeplerianSet5 |
_0NavModel_KeplerianSet9 |
_0NavModel_KeplerianSet |
_0NavModel_KeplerianSet11 |
_0NavModel_KeplerianSet10 |
_0NavModel_KeplerianSet13 |
_0NavModel_KeplerianSet12 |
_0NavModel_KeplerianSet14 |
_0NavModel_KeplerianSet0 |
_0NavModel_KeplerianSet3 |
_0NavModel_KeplerianSet4 |
_0NavModel_KeplerianSet1 |
_0NavModel_KeplerianSet2 |
_0NavModel_NAVKeplerianSet15 |
_0NavModel_NAVKeplerianSet16 |
_0NavModel_NAVKeplerianSet |
_0NavModel_NAVKeplerianSet13 |
_0NavModel_NAVKeplerianSet0 |
_0NavModel_NAVKeplerianSet14 |
_0NavModel_NAVKeplerianSet1 |
_0NavModel_NAVKeplerianSet2 |
_0NavModel_NAVKeplerianSet11 |
_0NavModel_NAVKeplerianSet12 |
_0NavModel_NAVKeplerianSet3 |
_0NavModel_NAVKeplerianSet10 |
_0NavModel_NAVKeplerianSet8 |
_0NavModel_NAVKeplerianSet9 |
_0NavModel_NAVKeplerianSet4 |
_0NavModel_NAVKeplerianSet5 |
_0NavModel_NAVKeplerianSet6 |
_0NavModel_NAVKeplerianSet7 |
_0NavModel_CNAVKeplerianSet6 |
_0NavModel_CNAVKeplerianSet5 |
_0NavModel_CNAVKeplerianSet8 |
_0NavModel_CNAVKeplerianSet7 |
_0NavModel_CNAVKeplerianSet9 |
_0NavModel_CNAVKeplerianSet |
_0NavModel_CNAVKeplerianSet0 |
_0NavModel_CNAVKeplerianSet15 |
_0NavModel_CNAVKeplerianSet1 |
_0NavModel_CNAVKeplerianSet14 |
_0NavModel_CNAVKeplerianSet2 |
_0NavModel_CNAVKeplerianSet17 |
_0NavModel_CNAVKeplerianSet3 |
_0NavModel_CNAVKeplerianSet16 |
_0NavModel_CNAVKeplerianSet4 |
_0NavModel_CNAVKeplerianSet11 |
_0NavModel_CNAVKeplerianSet10 |
_0NavModel_CNAVKeplerianSet13 |
_0NavModel_CNAVKeplerianSet12 |
_0NavModel_GLONASSecef8 |
_0NavModel_GLONASSecef9 |
_0NavModel_GLONASSecef10 |
_0NavModel_GLONASSecef6 |
_0NavModel_GLONASSecef7 |
_0NavModel_GLONASSecef1 |
_0NavModel_GLONASSecef0 |
_0NavModel_GLONASSecef |
_0NavModel_GLONASSecef5 |
_0NavModel_GLONASSecef4 |
_0NavModel_GLONASSecef3 |
_0NavModel_GLONASSecef2 |
_0NavModel_SBASecef9 |
_0NavModel_SBASecef3 |
_0NavModel_SBASecef8 |
_0NavModel_SBASecef2 |
_0NavModel_SBASecef7 |
_0NavModel_SBASecef5 |
_0NavModel_SBASecef6 |
_0NavModel_SBASecef4 |
_0NavModel_SBASecef1 |
_0NavModel_SBASecef0 |
_0NavModel_SBASecef |
SeqOfStandardClockModelElement |
_0StandardClockModelElement |
_0StandardClockModelElement4 |
_0StandardClockModelElement3 |
_0StandardClockModelElement0 |
_0StandardClockModelElement1 |
_0StandardClockModelElement2 |
_0NAVclockModel |
_0NAVclockModel0 |
_0NAVclockModel1 |
_0NAVclockModel2 |
_0NAVclockModel3 |
_0CNAVclockModel9 |
_0CNAVclockModel8 |
_0CNAVclockModel7 |
_0CNAVclockModel6 |
_0CNAVclockModel5 |
_0CNAVclockModel4 |
_0CNAVclockModel3 |
_0CNAVclockModel10 |
_0CNAVclockModel2 |
_0CNAVclockModel |
_0CNAVclockModel1 |
_0CNAVclockModel0 |
_0CNAVclockModel13 |
_0CNAVclockModel12 |
_0CNAVclockModel11 |
_0GLONASSclockModel |
_0GLONASSclockModel0 |
_0GLONASSclockModel1 |
_0SBASclockModel0 |
_0SBASclockModel |
_0SBASclockModel1 |
SeqOfBadSignalElement |
_0GANSSDataBitAssist |
SeqOfGanssDataBitsElement |
Seq_OfGANSSDataBitsSgn |
SeqOf_GANSSDataBits |
GANSSDataBit |
SeqOfGANSSRefMeasurementElement |
_0GANSSRefMeasurementElement1 |
_0GANSSRefMeasurementElement0 |
_0GANSSRefMeasurementElement2 |
_0GANSSRefMeasurementElement |
_0AdditionalDopplerFields |
_0AdditionalDopplerFields0 |
GANSSRefMeasurementAssist_R10_Ext |
_0GANSSRefMeasurement_R10_Ext_Element |
_0GANSSRefMeasurement_R10_Ext_Element0 |
_0GANSSAlmanacModel0 |
_0GANSSAlmanacModel1 |
_0GANSSAlmanacModel |
SeqOfGANSSAlmanacElement |
_0Almanac_KeplerianSet7 |
_0Almanac_KeplerianSet6 |
_0Almanac_KeplerianSet5 |
_0Almanac_KeplerianSet4 |
_0Almanac_KeplerianSet |
_0Almanac_KeplerianSet8 |
_0Almanac_KeplerianSet3 |
_0Almanac_KeplerianSet2 |
_0Almanac_KeplerianSet1 |
_0Almanac_KeplerianSet0 |
_0Almanac_NAVKeplerianSet0 |
_0Almanac_NAVKeplerianSet3 |
_0Almanac_NAVKeplerianSet4 |
_0Almanac_NAVKeplerianSet1 |
_0Almanac_NAVKeplerianSet2 |
_0Almanac_NAVKeplerianSet8 |
_0Almanac_NAVKeplerianSet7 |
_0Almanac_NAVKeplerianSet6 |
_0Almanac_NAVKeplerianSet5 |
_0Almanac_NAVKeplerianSet |
_0Almanac_ReducedKeplerianSet1 |
_0Almanac_ReducedKeplerianSet0 |
_0Almanac_ReducedKeplerianSet |
_0Almanac_MidiAlmanacSet7 |
_0Almanac_MidiAlmanacSet |
_0Almanac_MidiAlmanacSet0 |
_0Almanac_MidiAlmanacSet1 |
_0Almanac_MidiAlmanacSet2 |
_0Almanac_MidiAlmanacSet3 |
_0Almanac_MidiAlmanacSet4 |
_0Almanac_MidiAlmanacSet5 |
_0Almanac_MidiAlmanacSet6 |
_0Almanac_GlonassAlmanacSet0 |
_0Almanac_GlonassAlmanacSet9 |
_0Almanac_GlonassAlmanacSet |
_0Almanac_GlonassAlmanacSet2 |
_0Almanac_GlonassAlmanacSet1 |
_0Almanac_GlonassAlmanacSet4 |
_0Almanac_GlonassAlmanacSet3 |
_0Almanac_GlonassAlmanacSet6 |
_0Almanac_GlonassAlmanacSet5 |
_0Almanac_GlonassAlmanacSet8 |
_0Almanac_GlonassAlmanacSet11 |
_0Almanac_GlonassAlmanacSet7 |
_0Almanac_GlonassAlmanacSet10 |
_0Almanac_ECEFsbasAlmanacSet2 |
_0Almanac_ECEFsbasAlmanacSet3 |
_0Almanac_ECEFsbasAlmanacSet4 |
_0Almanac_ECEFsbasAlmanacSet5 |
_0Almanac_ECEFsbasAlmanacSet |
_0Almanac_ECEFsbasAlmanacSet0 |
_0Almanac_ECEFsbasAlmanacSet1 |
_0Almanac_ECEFsbasAlmanacSet6 |
_0Almanac_ECEFsbasAlmanacSet7 |
_0GANSSUTCModel6 |
_0GANSSUTCModel5 |
_0GANSSUTCModel4 |
_0GANSSUTCModel3 |
_0GANSSUTCModel2 |
_0GANSSUTCModel1 |
_0GANSSUTCModel0 |
_0GANSSUTCModel |
_0GANSSEphemerisExtensionHeader |
_0GANSSEphemerisExtensionHeader0 |
_0GANSSEphemerisExtensionTime |
_0ReferenceNavModel10 |
_0ReferenceNavModel |
_0ReferenceNavModel8 |
_0ReferenceNavModel9 |
_0ReferenceNavModel4 |
_0ReferenceNavModel5 |
_0ReferenceNavModel6 |
_0ReferenceNavModel7 |
_0ReferenceNavModel0 |
_0ReferenceNavModel11 |
_0ReferenceNavModel12 |
_0ReferenceNavModel1 |
_0ReferenceNavModel13 |
_0ReferenceNavModel2 |
_0ReferenceNavModel14 |
_0ReferenceNavModel3 |
SeqOfGANSSRefOrbit |
GANSSEphemerisDeltaMatrix |
_0GANSSDeltaEpochHeader |
GANSSDeltaElementList |
_0GANSSDeltaElementList |
_0GANSSEphemerisDeltaBitSizes7 |
_0GANSSEphemerisDeltaBitSizes6 |
_0GANSSEphemerisDeltaBitSizes |
_0GANSSEphemerisDeltaBitSizes5 |
_0GANSSEphemerisDeltaBitSizes4 |
_0GANSSEphemerisDeltaBitSizes9 |
_0GANSSEphemerisDeltaBitSizes8 |
_0GANSSEphemerisDeltaBitSizes11 |
_0GANSSEphemerisDeltaBitSizes12 |
_0GANSSEphemerisDeltaBitSizes13 |
_0GANSSEphemerisDeltaBitSizes14 |
_0GANSSEphemerisDeltaBitSizes2 |
_0GANSSEphemerisDeltaBitSizes3 |
_0GANSSEphemerisDeltaBitSizes0 |
_0GANSSEphemerisDeltaBitSizes1 |
_0GANSSEphemerisDeltaBitSizes10 |
_0GANSSEphemerisDeltaBitSizes15 |
_0GANSSEphemerisDeltaScales10 |
_0GANSSEphemerisDeltaScales6 |
_0GANSSEphemerisDeltaScales7 |
_0GANSSEphemerisDeltaScales4 |
_0GANSSEphemerisDeltaScales15 |
_0GANSSEphemerisDeltaScales5 |
_0GANSSEphemerisDeltaScales14 |
_0GANSSEphemerisDeltaScales2 |
_0GANSSEphemerisDeltaScales13 |
_0GANSSEphemerisDeltaScales3 |
_0GANSSEphemerisDeltaScales12 |
_0GANSSEphemerisDeltaScales0 |
_0GANSSEphemerisDeltaScales1 |
_0GANSSEphemerisDeltaScales11 |
_0GANSSEphemerisDeltaScales9 |
_0GANSSEphemerisDeltaScales8 |
_0GANSSEphemerisDeltaScales |
_0GANSSSatEventsInfo |
_0GANSSSatEventsInfo0 |
_0UTCmodelSet2 |
_0UTCmodelSet27 |
_0UTCmodelSet26 |
_0UTCmodelSet24 |
_0UTCmodelSet25 |
_0UTCmodelSet22 |
_0UTCmodelSet23 |
_0UTCmodelSet20 |
_0UTCmodelSet21 |
_0UTCmodelSet32 |
_0UTCmodelSet31 |
_0UTCmodelSet30 |
_0UTCmodelSet3 |
_0UTCmodelSet33 |
_0UTCmodelSet41 |
_0UTCmodelSet40 |
_0UTCmodelSet43 |
_0UTCmodelSet42 |
_0UTCmodelSet45 |
_0UTCmodelSet44 |
_0UTCmodelSet47 |
_0UTCmodelSet46 |
_0UTCmodelSet4 |
GANSS_ID1 |
GANSS_ID3 |
_0GANSS_ID3_element |
GANSSDiffCorrectionsValidityPeriod |
SeqOfDGANSSExtensionSgnElement |
_0DGANSSExtensionSgnElement |
_0DGANSSExtensionSgnElement0 |
RequiredResponseTime |
_0GPSClockModel |
_0GPSClockModel2 |
_0GPSClockModel0 |
_0GPSClockModel1 |
_0GPSEphemerisExtensionHeader0 |
_0GPSEphemerisExtensionHeader |
_0GPSEphemerisExtensionTime |
SeqOfGPSRefOrbit |
GPSEphemerisDeltaMatrix |
_0GPSDeltaEpochHeader |
GPSDeltaElementList |
_0GPSDeltaElementList |
_0GPSEphemerisDeltaBitSizes3 |
_0GPSEphemerisDeltaBitSizes2 |
_0GPSEphemerisDeltaBitSizes5 |
_0GPSEphemerisDeltaBitSizes4 |
_0GPSEphemerisDeltaBitSizes7 |
_0GPSEphemerisDeltaBitSizes6 |
_0GPSEphemerisDeltaBitSizes |
_0GPSEphemerisDeltaBitSizes9 |
_0GPSEphemerisDeltaBitSizes8 |
_0GPSEphemerisDeltaBitSizes1 |
_0GPSEphemerisDeltaBitSizes0 |
_0GPSEphemerisDeltaBitSizes14 |
_0GPSEphemerisDeltaBitSizes13 |
_0GPSEphemerisDeltaBitSizes10 |
_0GPSEphemerisDeltaBitSizes12 |
_0GPSEphemerisDeltaBitSizes11 |
_0GPSEphemerisDeltaScales13 |
_0GPSEphemerisDeltaScales14 |
_0GPSEphemerisDeltaScales10 |
_0GPSEphemerisDeltaScales0 |
_0GPSEphemerisDeltaScales11 |
_0GPSEphemerisDeltaScales12 |
_0GPSEphemerisDeltaScales1 |
_0GPSEphemerisDeltaScales2 |
_0GPSEphemerisDeltaScales3 |
_0GPSEphemerisDeltaScales4 |
_0GPSEphemerisDeltaScales5 |
_0GPSEphemerisDeltaScales6 |
_0GPSEphemerisDeltaScales7 |
_0GPSEphemerisDeltaScales8 |
_0GPSEphemerisDeltaScales9 |
_0GPSEphemerisDeltaScales |
_0GPSSatEventsInfo |
_0GPSSatEventsInfo0 |
DGPSCorrectionsValidityPeriod |
_0DGPSExtensionSatElement0 |
_0DGPSExtensionSatElement |
_0GPSReferenceTime_R10_Ext |
GPSAcquisAssist_R10_Ext |
_0GPSAcquisAssist_R10_Ext_Element |
_0GPSAcquisAssist_R10_Ext_Element0 |
_0GANSSLocationInfo |
_0GANSSLocationInfo0 |
_0GANSSLocationInfo1 |
PositionData |
GANSSTODm |
_0ReferenceFrame |
_0ReferenceFrame0 |
SeqOfGANSS_MsrSetElement |
_0GANSS_MsrSetElement |
SeqOfGANSS_MsrElement |
_0GANSS_MsrElement |
SeqOfGANSS_SgnTypeElement |
_0GANSS_SgnTypeElement |
SeqOfGANSS_SgnElement |
_0GANSS_SgnElement5 |
_0GANSS_SgnElement4 |
_0GANSS_SgnElement |
_0GANSS_SgnElement3 |
_0GANSS_SgnElement2 |
_0GANSS_SgnElement1 |
_0GANSS_SgnElement0 |
NonGANSSPositionMethods |
GANSSPositionMethods |
_0GANSSPositionMethod |
GANSSPositioningMethodTypes |
GANSSSignals |
SBASID |
MultipleMeasurementSets |
GPSAssistance |
CommonGANSSAssistance |
SpecificGANSSAssistance |
_0GANSSAssistanceForOneGANSS |
GANSSAssistance |
GANSSAdditionalAssistanceChoices |
_0GANSSAdditionalAssistanceChoicesForOneGANSS |
GANSSModelID |
PositionMethod |
UseMultipleSets |
EnvironmentCharacter |
TimeSlotScheme |
ReferenceRelation |
MpathIndic |
LocErrorReason |
ErrorCodes |
MoreAssDataToBeSent |
UlPseudoSegInd |
MsrPosition_Req |
MsrPosition_Rsp |
AssistanceData |
ProtocolError |
PosCapability_Req |
PosCapability_Rsp |
PositionInstruct |
AccuracyOpt |
ReferenceAssistData |
MsrAssistData |
MsrAssistBTS |
SystemInfoAssistData |
AssistBTSData |
CalcAssistanceBTS |
ReferenceWGS84 |
MultipleSets |
ReferenceIdentity |
BSICAndCarrier |
CellIDAndLAC |
OTD_MeasureInfo |
OTD_MsrElementFirst |
OTD_MsrElementRest |
TOA_MeasurementsOfRef |
OTD_Measurement |
OTD_MeasurementWithID |
EOTDQuality |
MultiFrameCarrier |
LocationInfo |
GPS_MeasureInfo |
GPS_MsrSetElement |
GPS_MsrElement |
LocationError |
AdditionalAssistanceData |
GPS_AssistData |
ControlHeader |
ReferenceTime |
GPSTime |
GPSTOWAssistElement |
GSMTime |
RefLocation |
DGPSCorrections |
SatElement |
NavigationModel |
NavModelElement |
UncompressedEphemeris |
EphemerisSubframe1Reserved |
IonosphericModel |
UTCModel |
Almanac |
AlmanacElement |
AcquisAssist |
TimeRelation |
AcquisElement |
AddionalDopplerFields |
AddionalAngleFields |
Rel98_MsrPosition_Req_Extension |
Rel98_AssistanceData_Extension |
Rel98_Ext_ExpOTD |
MsrAssistData_R98_ExpOTD |
MsrAssistBTS_R98_ExpOTD |
SystemInfoAssistData_R98_ExpOTD |
AssistBTSData_R98_ExpOTD |
GPSTimeAssistanceMeasurements |
Rel_98_MsrPosition_Rsp_Extension |
_0Rel_98_MsrPosition_Rsp_Extension |
OTD_MeasureInfo_R98_Ext |
OTD_MsrElementFirst_R98_Ext |
Rel_5_MsrPosition_Rsp_Extension |
Extended_reference |
Rel5_MsrPosition_Req_Extension |
Rel5_AssistanceData_Extension |
Rel_5_ProtocolError_Extension |
Rel7_MsrPosition_Req_Extension |
GANSS_AssistData |
GANSS_ControlHeader |
GANSSCommonAssistData |
GANSSGenericAssistDataElement |
GANSSReferenceTime |
GANSSRefTimeInfo |
GANSSReferenceTime_R10_Ext |
GANSSTOD_GSMTimeAssociation |
GANSSRefLocation |
GANSSIonosphericModel |
GANSSIonosphereModel |
GANSSIonoStormFlags |
GANSSAddIonosphericModel |
GANSSEarthOrientParam |
GANSSTimeModelElement |
GANSSTimeModelElement_R10_Ext |
GANSSDiffCorrections |
SgnTypeElement |
DGANSSSgnElement |
GANSSNavModel |
GANSSSatelliteElement |
NavModel_KeplerianSet |
NavModel_NAVKeplerianSet |
NavModel_CNAVKeplerianSet |
NavModel_GLONASSecef |
NavModel_SBASecef |
StandardClockModelElement |
NAVclockModel |
CNAVclockModel |
GLONASSclockModel |
SBASclockModel |
GANSSRealTimeIntegrity |
BadSignalElement |
GANSSDataBitAssist |
GanssDataBitsElement |
GANSSDataBitsSgnElement |
GANSSRefMeasurementAssist |
GANSSRefMeasurementElement |
AdditionalDopplerFields |
GANSSRefMeasurement_R10_Ext_Element |
GANSSAlmanacModel |
Almanac_KeplerianSet |
Almanac_NAVKeplerianSet |
Almanac_ReducedKeplerianSet |
Almanac_MidiAlmanacSet |
Almanac_GlonassAlmanacSet |
Almanac_ECEFsbasAlmanacSet |
GANSSAlmanacModel_R10_Ext |
GANSSUTCModel |
GANSSEphemerisExtension |
GANSSEphemerisExtensionHeader |
GANSSEphemerisExtensionTime |
ReferenceNavModel |
GANSSReferenceOrbit |
GANSSEphemerisDeltaEpoch |
GANSSDeltaEpochHeader |
GANSSEphemerisDeltaBitSizes |
GANSSEphemerisDeltaScales |
GANSSEphemerisExtensionCheck |
GANSSSatEventsInfo |
UTCmodelSet2 |
UTCmodelSet3 |
UTCmodelSet4 |
GANSS_ID1_element |
GANSS_ID3_element |
DGANSSExtensionSgnTypeElement |
DGANSSExtensionSgnElement |
Add_GPS_AssistData |
Add_GPS_ControlHeader |
GPSClockModel |
GPSEphemerisExtension |
GPSEphemerisExtensionHeader |
GPSEphemerisExtensionTime |
GPSReferenceOrbit |
GPSEphemerisDeltaEpoch |
GPSDeltaEpochHeader |
GPSEphemerisDeltaBitSizes |
GPSEphemerisDeltaScales |
GPSEphemerisExtensionCheck |
GPSSatEventsInfo |
DGPSExtensionSatElement |
GPSReferenceTime_R10_Ext |
GPSAcquisAssist_R10_Ext_Element |
GPSAlmanac_R10_Ext |
Rel_7_MsrPosition_Rsp_Extension |
GANSSLocationInfo |
ReferenceFrame |
GANSSMeasureInfo |
GANSS_MsrSetElement |
GANSS_MsrElement |
GANSS_SgnTypeElement |
GANSS_SgnElement |
Rel7_AssistanceData_Extension |
PosCapabilities |
GANSSPositionMethod |
AssistanceSupported |
GANSSAssistanceSet |
GANSSAssistanceForOneGANSS |
GANSSAdditionalAssistanceChoicesForOneGANSS |
AssistanceNeeded |
MethodType |
SystemInfoAssistBTS |
ReferenceIdentityType |
OTD_MsrsOfOtherSets |
NeighborIdentity |
SatStatus |
SystemInfoAssistBTS_R98_ExpOTD |
GANSSOrbitModel |
GANSSClockModel |
GANSSAlmanacElement |
GANSSAddUTCModel |
GANSSAuxiliaryInformation |

Constants Summary
FixType_twoDFix_ |
FixType_threeDFix_ |
maxGPSAssistanceData |
maxGANSSAssistanceData |
GANSSPositioningMethod_gps_ |
GANSSPositioningMethod_glonass_ |
GANSSPositioningMethod_modernizedGPS_ |
GANSSPositioningMethod_qzss_ |
GANSSPositioningMethod_galileo_ |
GANSSPositioningMethod_sbas_ |
PositionData_gps_ |
PositionData_e_otd_ |
PositionData_glonass_ |
PositionData_qzss_ |
PositionData_galileo_ |
PositionData_modernizedGPS_ |
PositionData_sbas_ |
NonGANSSPositionMethods_msBasedGPS_ |
NonGANSSPositionMethods_msAssistedGPS_ |
NonGANSSPositionMethods_msBasedEOTD_ |
NonGANSSPositionMethods_standaloneGPS_ |
NonGANSSPositionMethods_msAssistedEOTD_ |
GANSSPositioningMethodTypes_msAssisted_ |
GANSSPositioningMethodTypes_msBased_ |
GANSSPositioningMethodTypes_standalone_ |
GANSSSignals_signal6_ |
GANSSSignals_signal5_ |
GANSSSignals_signal7_ |
GANSSSignals_signal8_ |
GANSSSignals_signal3_ |
GANSSSignals_signal1_ |
GANSSSignals_signal2_ |
GANSSSignals_signal4_ |
SBASID_waas_ |
SBASID_gagan_ |
SBASID_masas_ |
SBASID_egnos_ |
MultipleMeasurementSets_gps_ |
MultipleMeasurementSets_eotd_ |
MultipleMeasurementSets_ganss_ |
GPSAssistance_ephemerisExtension_ |
GPSAssistance_realTimeIntegrity_ |
GPSAssistance_acquisitionAssistance_ |
GPSAssistance_dGPScorrections_ |
GPSAssistance_navigationmodel_ |
GPSAssistance_referenceTime_ |
GPSAssistance_ionosphericModel_ |
GPSAssistance_uTCmodel_ |
GPSAssistance_ephemerisExtensionCheck_ |
GPSAssistance_referenceLocation_ |
GPSAssistance_almanac_ |
CommonGANSSAssistance_ionosphericModel_ |
CommonGANSSAssistance_referenceLocation_ |
CommonGANSSAssistance_earthOrientationParam_ |
CommonGANSSAssistance_referenceTime_ |
CommonGANSSAssistance_addIonosphericModel_ |
GANSSAssistance_differentialCorrections_ |
GANSSAssistance_timeModelGNSS_GNSS_ |
GANSSAssistance_auxiliaryInformation_ |
GANSSAssistance_realTimeIntegrity_ |
GANSSAssistance_almanac_ |
GANSSAssistance_addUTCmodel_ |
GANSSAssistance_referenceMeasurementInformation_ |
GANSSAssistance_ephemerisExtensionCheck_ |
GANSSAssistance_timeModelGNSS_UTC_ |
GANSSAssistance_ephemerisExtension_ |
GANSSAssistance_databitassistance_ |
GANSSAssistance_navigationModel_ |
GANSSModelID_model6_ |
GANSSModelID_model1_ |
GANSSModelID_model4_ |
GANSSModelID_model3_ |
GANSSModelID_model5_ |
GANSSModelID_model7_ |
GANSSModelID_model8_ |
GANSSModelID_model2_ |

## Details

Accuracy

    Accuracy ::= INTEGER (0..127)
    -- Position Method
    PositionMethod

MeasureResponseTime

    MeasureResponseTime ::= INTEGER (0..7)
    -- useMultiple Sets, FFS!
    UseMultipleSets

BTSPosition

    Ext-GeographicalInformation
    -- RF channel number of BCCH
    BCCHCarrier

BCCHCarrier

    BCCHCarrier ::= INTEGER (0..1023)
    -- Base station Identity Code
    BSIC

BSIC

    BSIC ::= INTEGER (0..63)
    -- Timeslot scheme
    TimeSlotScheme

ModuloTimeSlot

    ModuloTimeSlot ::= INTEGER (0..3)
    -- E-OTD measurement assistance data IE
    -- The total number of neighbors in this element (MsrAssistData)
    -- and in SystemInfoAssistData element (presented neighbors
    -- can be at a maximum 15!)
    MsrAssistData

SeqOfMsrAssistBTS

    SeqOfMsrAssistBTS ::= SEQUENCE (SIZE(1..15)) OF MsrAssistBTS
    MsrAssistBTS

MultiFrameOffset

    MultiFrameOffset ::= INTEGER (0..51)
    -- The Multiframe Offset value 51 shall not be encoded by the transmitting entity and
    -- shall be treated by the receiving entity as 0.
    -- Rough RTD value between one base station and reference BTS
    RoughRTD

RoughRTD

    RoughRTD ::= INTEGER (0..1250)
    -- The RoughRTD value 1250 shall not be encoded by the transmitting entity and shall
    -- be treated by the receiving entity as 0.
    -- E-OTD Measurement assistance data for system information List IE
    -- The total number of base stations in this element (SystemInfoAssistData
    -- presented neighbors) and in MsrAssistData element can be at a maximum 15.
    SystemInfoAssistData

SeqOfSystemInfoAssistBTS

    SeqOfSystemInfoAssistBTS::= SEQUENCE (SIZE(1..32)) OF SystemInfoAssistBTS
    -- whether n.th is present or not ?
    SystemInfoAssistBTS

FineRTD

    FineRTD ::= INTEGER (0..255)
    -- Relative north/east distance
    RelDistance

RelDistance

    RelDistance ::= INTEGER (-200000..200000)
    -- Relative altitude
    RelativeAlt

RelativeAlt

    RelativeAlt ::= INTEGER (-4000..4000)
    -- Measure position response IEs
    -- Reference Identity
    -- Multiple sets
    MultipleSets

_0MultipleSets0

    INTEGER (1..3)

_0MultipleSets

    INTEGER (2..3)

SeqOfReferenceIdentityType

    SeqOfReferenceIdentityType ::= SEQUENCE (SIZE(1..3)) OF ReferenceIdentityType
    -- Cell identity
    ReferenceIdentityType

RequestIndex

    RequestIndex ::= INTEGER (1..16)
    SystemInfoIndex

SystemInfoIndex

    SystemInfoIndex ::= INTEGER (1..32)
    CellIDAndLAC

CellID

    CellID ::= INTEGER (0..65535)
    LAC

LAC

    LAC ::= INTEGER (0..65535)
    -- OTD-MeasureInfo
    OTD-MeasureInfo

SeqOfOTD_MsrElementRest

    SeqOfOTD-MsrElementRest ::= SEQUENCE (SIZE(1..2)) OF OTD-MsrElementRest
    -- OTD measurent information for 1 set
    OTD-MsrElementFirst

_0OTD_MsrElementFirst0

    INTEGER (0..960)        OPTIONAL

_0OTD_MsrElementFirst

    INTEGER (0..42431)

SeqOfOTD_FirstSetMsrs

    SeqOfOTD-FirstSetMsrs ::= SEQUENCE (SIZE(1..10)) OF OTD-FirstSetMsrs
    -- OTD measurent information 2 and 3 sets if exist
    OTD-MsrElementRest

_0OTD_MsrElementRest0

    INTEGER (0..960)            OPTIONAL

_0OTD_MsrElementRest

    INTEGER (0..42431)

SeqOfOTD_MsrsOfOtherSets

    SeqOfOTD-MsrsOfOtherSets ::= SEQUENCE (SIZE(1..10)) OF OTD-MsrsOfOtherSets
    -- Standard deviation of the TOA measurements from the reference BTS
    TOA-MeasurementsOfRef

RefQuality

    RefQuality ::= INTEGER (0..31)            -- St Dev of TOA of reference as defined in annex
    NumOfMeasurements

NumOfMeasurements

    NumOfMeasurements ::= INTEGER (0..7)    -- No. of measurements for RefQuality as defined in annex
    StdResolution

StdResolution

    StdResolution ::= INTEGER (0..3)        -- Values of resolution are defined in annex
    OTD-FirstSetMsrs

OTD_FirstSetMsrs

    OTD-MeasurementWithID
    -- Neighbour info in OTD measurements 0-10 times in TD measurement info
    OTD-MsrsOfOtherSets

_0EOTDQuality

    INTEGER    (0..7)

_0EOTDQuality0

    INTEGER (0..31)

OTDValue

    OTDValue ::= INTEGER (0..39999)
    -- Location information IE
    LocationInfo

_0LocationInfo

    INTEGER (0..65535)

_0LocationInfo0

    INTEGER (0..14399999)    OPTIONAL

FixType

    FixType ::= INTEGER {
        twoDFix (0),
        threeDFix (1)
    } (0..1)
    -- GPS-Measurement information
    GPS-MeasureInfo

SeqOfGPS_MsrSetElement

    SeqOfGPS-MsrSetElement ::= SEQUENCE (SIZE(1..3)) OF GPS-MsrSetElement
    -- OTD measurent information 1-3 times in message
    GPS-MsrSetElement

_0GPS_MsrSetElement

    INTEGER (0..65535)    OPTIONAL

GPSTOW24b

    GPSTOW24b ::= INTEGER (0..14399999)
    -- measured elements in measurement parameters field
    SeqOfGPS-MsrElement

SeqOfGPS_MsrElement

    SeqOfGPS-MsrElement ::= SEQUENCE (SIZE(1..16)) OF GPS-MsrElement
    GPS-MsrElement

_0GPS_MsrElement0

    INTEGER (-32768..32767)

_0GPS_MsrElement1

    INTEGER (0..1022)

_0GPS_MsrElement2

    INTEGER (0..1024)

_0GPS_MsrElement3

    INTEGER (0..63)

_0GPS_MsrElement

    INTEGER (0..63)

GPSAssistanceData

    GPSAssistanceData ::= OCTET STRING (SIZE (1..maxGPSAssistanceData))
    -- GPSAssistanceData has identical structure and encoding to octets 3 to n of the
    -- GPS Assistance Data IE in 3GPP TS 49.031
    maxGPSAssistanceData

GANSSAssistanceData

    GANSSAssistanceData ::= OCTET STRING (SIZE (1..maxGANSSAssistanceData))
    -- GANSSAssistanceData has identical structure and encoding to octets 3 to n of the
    -- GANSS Assistance Data IE in 3GPP TS 49.031
    maxGANSSAssistanceData

GPSTOW23b

    GPSTOW23b ::= INTEGER (0..7559999)
    -- GPS week number
    GPSWeek

GPSWeek

    GPSWeek ::= INTEGER (0..1023)
    -- GPSTOWAssist consists of TLM message, Anti-spoof flag, Alert flag, and 2 reserved bits in TLM Word
    -- for each visible satellite.
    -- N_SAT can be read from number of elements in GPSTOWAssist
    GPSTOWAssist

GPSTOWAssist

    GPSTOWAssist ::= SEQUENCE (SIZE(1..12)) OF GPSTOWAssistElement
    GPSTOWAssistElement

TLMWord

    TLMWord ::= INTEGER (0..16383)
    -- Anti-Spoof flag
    AntiSpoofFlag

AntiSpoofFlag

    AntiSpoofFlag ::= INTEGER (0..1)
    -- Alert flag
    AlertFlag

AlertFlag

    AlertFlag ::= INTEGER (0..1)
    -- Reserved bits in TLM word, MSB occurs earlier in TLM Word transmitted by satellite
    TLMReservedBits

TLMReservedBits

    TLMReservedBits ::= INTEGER (0..3)
    GSMTime

FrameNumber

    FrameNumber ::= INTEGER (0..2097151)
    -- Time slot number
    TimeSlot

TimeSlot

    TimeSlot ::= INTEGER (0..7)
    -- Bit number
    BitNumber

BitNumber

    BitNumber ::= INTEGER (0..156)
    -- Reference Location IE
    RefLocation

_0DGPSCorrections

    INTEGER (0..604799)

_0DGPSCorrections0

    INTEGER (0..7)

SeqOfSatElement

    SeqOfSatElement ::= SEQUENCE (SIZE (1..16)) OF SatElement
    -- number of correction for satellites
    SatElement

_0SatElement0

    INTEGER (0..3)

_0SatElement1

    INTEGER (-2047..2047)

_0SatElement2

    INTEGER (-127..127)

_0SatElement3

    INTEGER (-127..127)

_0SatElement4

    INTEGER (-7..7)

_0SatElement5

    INTEGER (-127..127)

_0SatElement6

    INTEGER (-7..7)

_0SatElement

    INTEGER (0..239)

SatelliteID

    SatelliteID ::= INTEGER (0..63)    -- identifies satellite
    -- Navigation Model IE
    NavigationModel

SeqOfNavModelElement

    SeqOfNavModelElement ::= SEQUENCE (SIZE(1..16)) OF NavModelElement
    NavModelElement

_0UncompressedEphemeris0

    INTEGER (0..15)

_0UncompressedEphemeris17

    INTEGER (0..1)

_0UncompressedEphemeris16

    INTEGER (0..37799)

_0UncompressedEphemeris15

    INTEGER (0..4294967295)

_0UncompressedEphemeris14

    INTEGER (-32768..32767)

_0UncompressedEphemeris13

    INTEGER (0..4294967295)

_0UncompressedEphemeris12

    INTEGER (-32768..32767)

_0UncompressedEphemeris11

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris10

    INTEGER (-32768..32767)

_0UncompressedEphemeris

    INTEGER (0..3)

_0UncompressedEphemeris19

    INTEGER (-32768..32767)

_0UncompressedEphemeris18

    INTEGER (0..31)

_0UncompressedEphemeris20

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris26

    INTEGER (-8192..8191)

_0UncompressedEphemeris9

    INTEGER (-32768..32767)

_0UncompressedEphemeris25

    INTEGER (-8388608..8388607)

_0UncompressedEphemeris22

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris21

    INTEGER (-32768..32767)

_0UncompressedEphemeris24

    INTEGER (-2147483648..2147483647)

_0UncompressedEphemeris23

    INTEGER (-32768..32767)

_0UncompressedEphemeris1

    INTEGER (0..63)

_0UncompressedEphemeris2

    INTEGER    (0..1023)

_0UncompressedEphemeris3

    INTEGER (0..1)

_0UncompressedEphemeris4

    INTEGER (-128..127)

_0UncompressedEphemeris5

    INTEGER (0..37799)

_0UncompressedEphemeris6

    INTEGER (-128..127)

_0UncompressedEphemeris7

    INTEGER (-32768..32767)

_0UncompressedEphemeris8

    INTEGER (-2097152..2097151)

_0EphemerisSubframe1Reserved

    INTEGER (0..8388607)

_0EphemerisSubframe1Reserved0

    INTEGER (0..16777215)

_0EphemerisSubframe1Reserved1

    INTEGER (0..16777215)

_0EphemerisSubframe1Reserved2

    INTEGER (0..65535)

_0IonosphericModel4

    INTEGER (-128..127)

_0IonosphericModel3

    INTEGER (-128..127)

_0IonosphericModel6

    INTEGER (-128..127)

_0IonosphericModel5

    INTEGER (-128..127)

_0IonosphericModel0

    INTEGER (-128..127)

_0IonosphericModel2

    INTEGER (-128..127)

_0IonosphericModel1

    INTEGER (-128..127)

_0IonosphericModel

    INTEGER (-128..127)

_0UTCModel6

    INTEGER (-128..127)

_0UTCModel0

    INTEGER (-2147483648..2147483647)

_0UTCModel1

    INTEGER (0..255)

_0UTCModel2

    INTEGER (0..255)

_0UTCModel

    INTEGER (-8388608..8388607)

_0UTCModel3

    INTEGER (-128..127)

_0UTCModel4

    INTEGER (0..255)

_0UTCModel5

    INTEGER (-128..127)

_0Almanac

    INTEGER (0..255)

SeqOfAlmanacElement

    SeqOfAlmanacElement ::= SEQUENCE (SIZE(1..64)) OF AlmanacElement
    -- Almanac info once per satellite
    AlmanacElement

_0AlmanacElement8

    INTEGER (-1024..1023)

_0AlmanacElement9

    INTEGER (-1024..1023)

_0AlmanacElement

    INTEGER (0..65535)

_0AlmanacElement6

    INTEGER (-8388608..8388607)

_0AlmanacElement7

    INTEGER (-8388608..8388607)

_0AlmanacElement4

    INTEGER (0..16777215)

_0AlmanacElement5

    INTEGER (-8388608..8388607)

_0AlmanacElement2

    INTEGER (-32768..32767)

_0AlmanacElement3

    INTEGER (0..255)

_0AlmanacElement0

    INTEGER (0..255)

_0AlmanacElement1

    INTEGER (-32768..32767)

SeqOfAcquisElement

    SeqOfAcquisElement ::= SEQUENCE (SIZE(1..16)) OF AcquisElement
    -- the relationship between GPS time and air-interface timing
    TimeRelation

_0AcquisElement3

    INTEGER (0..15)

_0AcquisElement0

    INTEGER (0..1022)

_0AcquisElement1

    INTEGER (0..19)

_0AcquisElement2

    INTEGER (0..3)

_0AcquisElement

    INTEGER (-2048..2047)

_0AddionalDopplerFields0

    INTEGER (0..7)

_0AddionalDopplerFields

    INTEGER (0..63)

_0AddionalAngleFields0

    INTEGER (0..7)

_0AddionalAngleFields

    INTEGER (0..31)

SeqOf_BadSatelliteSet

    SeqOf-BadSatelliteSet ::= SEQUENCE (SIZE(1..16)) OF SatelliteID
    -- Extension Elements
    -- Release 98 Extensions here
    Rel98-MsrPosition-Req-Extension

SeqOfMsrAssistBTS_R98_ExpOTD

    SeqOfMsrAssistBTS-R98-ExpOTD ::= SEQUENCE (SIZE(1..15)) OF MsrAssistBTS-R98-ExpOTD
    -- This element completes MsrAssistBTS IE
    MsrAssistBTS-R98-ExpOTD

SeqOfSystemInfoAssistBTS_R98_ExpOTD

    SeqOfSystemInfoAssistBTS-R98-ExpOTD ::= SEQUENCE (SIZE(1..32)) OF SystemInfoAssistBTS-R98-ExpOTD
    -- whether n.th is present or not ?
    SystemInfoAssistBTS-R98-ExpOTD

ExpectedOTD

    ExpectedOTD ::= INTEGER (0..1250)
    -- The ExpectedOTD value 1250 shall not be encoded by the transmitting entity and
    -- shall be treated by the receiving entity as 0.
    -- Uncertainty of Exptected OTD in bits
    ExpOTDUncertainty

ExpOTDUncertainty

    ExpOTDUncertainty ::= INTEGER(0..7)
    -- Release 98 extensions
    GPSReferenceTimeUncertainty

GPSReferenceTimeUncertainty

    GPSReferenceTimeUncertainty ::= INTEGER (0 .. 127)         -- Coding according to Annex
    GPSTimeAssistanceMeasurements

_0GPSTimeAssistanceMeasurements

    INTEGER (0 .. 63)    OPTIONAL

_0GPSTimeAssistanceMeasurements1

    INTEGER (0 .. 127)             OPTIONAL

_0GPSTimeAssistanceMeasurements0

    INTEGER (0 .. 9999)         OPTIONAL

SeqOfOTD_FirstSetMsrs_R98_Ext

    SeqOfOTD-FirstSetMsrs-R98-Ext ::= SEQUENCE (SIZE(1..5)) OF OTD-FirstSetMsrs
    Rel-5-MsrPosition-Rsp-Extension

_0Extended_reference0

    INTEGER (0..262143)

_0Extended_reference

    INTEGER (0..63)

OTD_MeasureInfo_5_Ext

    SeqOfOTD-MsrElementRest
    -- if more than one measurement sets are present this element is repeated
    -- NumberOfSets - 1 (-1 = first set) combined in OTD-MeasureInfo-5-Ext and
    -- OTD-MeasureInfo (e.g. if NumberOfSets is 3, then one otdMsrRestSets may
    -- be sent in OTD-MeasureInfo-5-Ext and one in OTD-MeasureInfo)
    -- First part of Uplink RRLP Pseudo-segmentation indication, possibly more may be defined
    -- in the future for segmentation with more than two segments.
    UlPseudoSegInd

GANSSPositioningMethod

    GANSSPositioningMethod ::= BIT STRING {
        gps                (0),
        galileo           (1),
        sbas                (2),
        modernizedGPS      (3),
        qzss                (4),
        glonass           (5) } (SIZE (2..16))
    GANSS-AssistData

SeqOfGANSSGenericAssistDataElement

    SeqOfGANSSGenericAssistDataElement ::= SEQUENCE (SIZE (1..8)) OF GANSSGenericAssistDataElement
    -- GANSS Generic Assistance Data Elements
    GANSSGenericAssistDataElement

_0GANSSGenericAssistDataElement

    INTEGER (0..7)    OPTIONAL

_0GANSSGenericAssistDataElement0

    INTEGER (0..7)     OPTIONAL

_0GANSSRefTimeInfo0

    INTEGER (0 .. 7)          OPTIONAL

_0GANSSRefTimeInfo

    INTEGER(0 .. 8191)      OPTIONAL

GANSSTOD

    GANSSTOD ::= INTEGER (0 .. 86399)
    -- GANSS TOD uncertainty
    GANSSTODUncertainty

GANSSTODUncertainty

    GANSSTODUncertainty ::= INTEGER (0 .. 127) -- Coding according to Annex
    -- GANSS Reference Time Rel-10 Extension:
    GANSSReferenceTime-R10-Ext

_0GANSSReferenceTime_R10_Ext

    INTEGER(0..7)

FrameDrift

    FrameDrift ::= INTEGER(-64 .. 63)
    -- GANSS Reference Location IE
    GANSSRefLocation

_0GANSSIonosphereModel

    INTEGER (0 .. 4095)

_0GANSSIonosphereModel0

    INTEGER (0 .. 4095)

_0GANSSIonosphereModel1

    INTEGER (0 .. 4095)

_0GANSSIonoStormFlags

    INTEGER (0 .. 1)

_0GANSSIonoStormFlags0

    INTEGER (0 .. 1)

_0GANSSIonoStormFlags1

    INTEGER (0 .. 1)

_0GANSSIonoStormFlags2

    INTEGER (0 .. 1)

_0GANSSIonoStormFlags3

    INTEGER (0 .. 1)

_0GANSSAddIonosphericModel

    BIT STRING (SIZE (2))

_0GANSSEarthOrientParam5

    INTEGER (-262144..262143)

_0GANSSEarthOrientParam

    INTEGER (0..65535)

_0GANSSEarthOrientParam1

    INTEGER (-16384..16383)

_0GANSSEarthOrientParam2

    INTEGER (-1048576..1048575)

_0GANSSEarthOrientParam3

    INTEGER (-16384..16383)

_0GANSSEarthOrientParam4

    INTEGER (-1073741824..1073741823)

_0GANSSEarthOrientParam0

    INTEGER (-1048576..1048575)

SeqOfGANSSTimeModel

    SeqOfGANSSTimeModel ::= SEQUENCE (SIZE(1..7)) OF GANSSTimeModelElement
    GANSSTimeModelElement

_0GANSSTimeModelElement1

    INTEGER (0 .. 8191)     OPTIONAL

_0GANSSTimeModelElement0

    INTEGER (0 .. 7)

_0GANSSTimeModelElement

    INTEGER(0 .. 65535)

TA0

    TA0 ::= INTEGER (-2147483648 .. 2147483647)
    -- GANSS time model parameter A1
    TA1

TA1

    TA1 ::= INTEGER (-8388608 .. 8388607)
    -- GANSS time model parameter A2
    TA2

TA2

    TA2 ::= INTEGER (-64 .. 63)
    -- GANSS Time Model Rel-10 Extension:
    SeqOfGANSSTimeModel-R10-Ext

SeqOfGANSSTimeModel_R10_Ext

    SeqOfGANSSTimeModel-R10-Ext ::= SEQUENCE (SIZE(1..7)) OF GANSSTimeModelElement-R10-Ext
    GANSSTimeModelElement-R10-Ext

_0GANSSTimeModelElement_R10_Ext0

    INTEGER (-128..127)

_0GANSSTimeModelElement_R10_Ext

    INTEGER (0 .. 7)

_0GANSSDiffCorrections

    INTEGER (0 .. 119)

SeqOfSgnTypeElement

    SeqOfSgnTypeElement ::= SEQUENCE (SIZE (1..3)) OF SgnTypeElement -- max three signals per GNSS
    -- DGANSS signal type element, once per GNSS signal type included in DGANSS
    SgnTypeElement

_0SgnTypeElement

    INTEGER (0 .. 7)

GANSSSignalID

    GANSSSignalID ::= INTEGER (0 .. 7)    -- Coding according to Annex
    SeqOfDGANSSSgnElement

SeqOfDGANSSSgnElement

    SeqOfDGANSSSgnElement ::= SEQUENCE (SIZE (1..16)) OF DGANSSSgnElement
    -- number of correction for signals
    DGANSSSgnElement

_0DGANSSSgnElement0

    INTEGER (0..3)

_0DGANSSSgnElement1

    INTEGER (-2047..2047)

_0DGANSSSgnElement2

    INTEGER (-127..127)

_0DGANSSSgnElement

    INTEGER (0 .. 1023)

SVID

    SVID ::= INTEGER (0 .. 63)    -- Coding according to Annex
    -- GANSS Navigation Model IE
    GANSSNavModel

_0GANSSNavModel

    INTEGER (0 .. 1)

SeqOfGANSSSatelliteElement

    SeqOfGANSSSatelliteElement ::= SEQUENCE (SIZE(1..32)) OF GANSSSatelliteElement
    GANSSSatelliteElement

_0GANSSSatelliteElement1

    BIT STRING (SIZE(1))     OPTIONAL

_0GANSSSatelliteElement0

    INTEGER (0 .. 1023)

_0GANSSSatelliteElement

    BIT STRING (SIZE(5))

_0GANSSSatelliteElement2

    INTEGER (0 .. 1)         OPTIONAL

_0NavModel_KeplerianSet8

    INTEGER (-2147483648..2147483647)

_0NavModel_KeplerianSet7

    INTEGER (-2147483648..2147483647)

_0NavModel_KeplerianSet6

    INTEGER (0.. 4294967295)

_0NavModel_KeplerianSet5

    INTEGER (-8192..8191)

_0NavModel_KeplerianSet9

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet

    INTEGER (0 .. 16383)

_0NavModel_KeplerianSet11

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet10

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet13

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet12

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet14

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet0

    INTEGER (-2147483648..2147483647)

_0NavModel_KeplerianSet3

    INTEGER (-8388608..8388607)

_0NavModel_KeplerianSet4

    INTEGER (0..4294967295)

_0NavModel_KeplerianSet1

    INTEGER (-32768..32767)

_0NavModel_KeplerianSet2

    INTEGER (-2147483648..2147483647)

_0NavModel_NAVKeplerianSet15

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet16

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet

    INTEGER (0..15)

_0NavModel_NAVKeplerianSet13

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet0

    INTEGER (0..1)

_0NavModel_NAVKeplerianSet14

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet1

    INTEGER (0..37799)

_0NavModel_NAVKeplerianSet2

    INTEGER (-2147483648..2147483647)

_0NavModel_NAVKeplerianSet11

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet12

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet3

    INTEGER (-32768..32767)

_0NavModel_NAVKeplerianSet10

    INTEGER (-2147483648..2147483647)

_0NavModel_NAVKeplerianSet8

    INTEGER (0..4294967295)

_0NavModel_NAVKeplerianSet9

    INTEGER (-2147483648..2147483647)

_0NavModel_NAVKeplerianSet4

    INTEGER (-2147483648..2147483647)

_0NavModel_NAVKeplerianSet5

    INTEGER (-8388608..8388607)

_0NavModel_NAVKeplerianSet6

    INTEGER (0..4294967295)

_0NavModel_NAVKeplerianSet7

    INTEGER (-8192..8191)

_0NavModel_CNAVKeplerianSet6

    INTEGER (0..8589934591)

_0NavModel_CNAVKeplerianSet5

    INTEGER (-4294967296..4294967295)

_0NavModel_CNAVKeplerianSet8

    INTEGER (-4294967296..4294967295)

_0NavModel_CNAVKeplerianSet7

    INTEGER (-4294967296..4294967295)

_0NavModel_CNAVKeplerianSet9

    INTEGER (-65536..65535)

_0NavModel_CNAVKeplerianSet

    INTEGER (0..2015)

_0NavModel_CNAVKeplerianSet0

    INTEGER (-16..15)

_0NavModel_CNAVKeplerianSet15

    INTEGER (-8388608..8388607)

_0NavModel_CNAVKeplerianSet1

    INTEGER (-33554432..33554431)

_0NavModel_CNAVKeplerianSet14

    INTEGER (-8388608..8388607)

_0NavModel_CNAVKeplerianSet2

    INTEGER (-16777216..16777215)

_0NavModel_CNAVKeplerianSet17

    INTEGER (-1048576..1048575)

_0NavModel_CNAVKeplerianSet3

    INTEGER (-65536..65535)

_0NavModel_CNAVKeplerianSet16

    INTEGER (-1048576..1048575)

_0NavModel_CNAVKeplerianSet4

    INTEGER (-4194304..4194303)

_0NavModel_CNAVKeplerianSet11

    INTEGER (-16384..16383)

_0NavModel_CNAVKeplerianSet10

    INTEGER (-4294967296..4294967295)

_0NavModel_CNAVKeplerianSet13

    INTEGER (-32768..32767)

_0NavModel_CNAVKeplerianSet12

    INTEGER (-32768..32767)

_0NavModel_GLONASSecef8

    INTEGER (-67108864..67108863)

_0NavModel_GLONASSecef9

    INTEGER (-8388608..8388607)

_0NavModel_GLONASSecef10

    INTEGER (-16..15)

_0NavModel_GLONASSecef6

    INTEGER (-8388608..8388607)

_0NavModel_GLONASSecef7

    INTEGER (-16..15)

_0NavModel_GLONASSecef1

    INTEGER (0..3)

_0NavModel_GLONASSecef0

    BIT STRING (SIZE(2))

_0NavModel_GLONASSecef

    INTEGER (0..31)

_0NavModel_GLONASSecef5

    INTEGER (-67108864..67108863)

_0NavModel_GLONASSecef4

    INTEGER (-16..15)

_0NavModel_GLONASSecef3

    INTEGER (-8388608..8388607)

_0NavModel_GLONASSecef2

    INTEGER (-67108864..67108863)

_0NavModel_SBASecef9

    INTEGER (-512..511)

_0NavModel_SBASecef3

    INTEGER (-16777216..16777215)

_0NavModel_SBASecef8

    INTEGER (-512..511)

_0NavModel_SBASecef2

    INTEGER (-536870912..536870911)

_0NavModel_SBASecef7

    INTEGER (-512..511)

_0NavModel_SBASecef5

    INTEGER (-65536..65535)

_0NavModel_SBASecef6

    INTEGER (-131072..131071)

_0NavModel_SBASecef4

    INTEGER (-65536..65535)

_0NavModel_SBASecef1

    INTEGER (-536870912..536870911)

_0NavModel_SBASecef0

    BIT STRING (SIZE(4))

_0NavModel_SBASecef

    INTEGER (0..5399)                     OPTIONAL

SeqOfStandardClockModelElement

    SeqOfStandardClockModelElement ::= SEQUENCE (SIZE(1..2)) OF StandardClockModelElement
    StandardClockModelElement

_0StandardClockModelElement

    INTEGER (0 .. 16383)

_0StandardClockModelElement4

    INTEGER (0 .. 1)                     OPTIONAL

_0StandardClockModelElement3

    INTEGER (-512 .. 511)                 OPTIONAL

_0StandardClockModelElement0

    INTEGER (-2048 .. 2047)

_0StandardClockModelElement1

    INTEGER (-131072 .. 131071)

_0StandardClockModelElement2

    INTEGER (-134217728 .. 134217727)

_0NAVclockModel

    INTEGER (0.. 37799)

_0NAVclockModel0

    INTEGER (-128..127)

_0NAVclockModel1

    INTEGER (-32768..32767)

_0NAVclockModel2

    INTEGER (-2097152..2097151)

_0NAVclockModel3

    INTEGER (-128..127)

_0CNAVclockModel9

    INTEGER (-4096..4095)             OPTIONAL

_0CNAVclockModel8

    INTEGER (-4096..4095)             OPTIONAL

_0CNAVclockModel7

    INTEGER (-4096..4095)

_0CNAVclockModel6

    INTEGER (-33554432..33554431)

_0CNAVclockModel5

    INTEGER (-524288..524287)

_0CNAVclockModel4

    INTEGER (-512..511)

_0CNAVclockModel3

    INTEGER (0..7)

_0CNAVclockModel10

    INTEGER (-4096..4095)             OPTIONAL

_0CNAVclockModel2

    INTEGER (0..7)

_0CNAVclockModel

    INTEGER (0..2015)

_0CNAVclockModel1

    INTEGER (-16..15)

_0CNAVclockModel0

    INTEGER (0..2015)

_0CNAVclockModel13

    INTEGER (-4096..4095)             OPTIONAL

_0CNAVclockModel12

    INTEGER (-4096..4095)             OPTIONAL

_0CNAVclockModel11

    INTEGER (-4096..4095)             OPTIONAL

_0GLONASSclockModel

    INTEGER (-2097152..2097151)

_0GLONASSclockModel0

    INTEGER (-1024..1023)

_0GLONASSclockModel1

    INTEGER (-16..15)                 OPTIONAL

_0SBASclockModel0

    INTEGER (-2048..2047)

_0SBASclockModel

    INTEGER (0..5399)

_0SBASclockModel1

    INTEGER (-128..127)

SeqOfBadSignalElement

    SeqOfBadSignalElement ::= SEQUENCE (SIZE(1..16)) OF BadSignalElement
    BadSignalElement

_0GANSSDataBitAssist

    INTEGER (0 .. 59)

SeqOfGanssDataBitsElement

    SeqOfGanssDataBitsElement ::= SEQUENCE (SIZE(1 .. 32))OF GanssDataBitsElement
    GanssDataBitsElement

Seq_OfGANSSDataBitsSgn

    Seq-OfGANSSDataBitsSgn ::= SEQUENCE (SIZE(1..8)) OF GANSSDataBitsSgnElement
    GANSSDataBitsSgnElement

SeqOf_GANSSDataBits

    SeqOf-GANSSDataBits ::= SEQUENCE (SIZE(1 .. 1024)) OF GANSSDataBit
    GANSSDataBit

GANSSDataBit

    GANSSDataBit ::= INTEGER(0 .. 1)
    -- GANSS Reference Measurement Assistance IE
    -- Code and Doppler assistance from the network.
    GANSSRefMeasurementAssist

SeqOfGANSSRefMeasurementElement

    SeqOfGANSSRefMeasurementElement ::= SEQUENCE (SIZE(1 .. 16)) OF GANSSRefMeasurementElement
    GANSSRefMeasurementElement

_0GANSSRefMeasurementElement1

    INTEGER (0 .. 127)

_0GANSSRefMeasurementElement0

    INTEGER (0 .. 1022)

_0GANSSRefMeasurementElement2

    INTEGER (0 .. 31)

_0GANSSRefMeasurementElement

    INTEGER (-2048 .. 2047)

_0AdditionalDopplerFields

    INTEGER (0..63)

_0AdditionalDopplerFields0

    INTEGER (0..4)

GANSSRefMeasurementAssist_R10_Ext

    GANSSRefMeasurementAssist-R10-Ext ::= SEQUENCE (SIZE(1 .. 16)) OF
                                                                GANSSRefMeasurement-R10-Ext-Element
    GANSSRefMeasurement-R10-Ext-Element

_0GANSSRefMeasurement_R10_Ext_Element

    INTEGER(0..15)

_0GANSSRefMeasurement_R10_Ext_Element0

    INTEGER(0..15)

_0GANSSAlmanacModel0

    INTEGER (0 .. 255)     OPTIONAL

_0GANSSAlmanacModel1

    INTEGER (0 .. 3)     OPTIONAL

_0GANSSAlmanacModel

    INTEGER (0 .. 255)

SeqOfGANSSAlmanacElement

    SeqOfGANSSAlmanacElement ::= SEQUENCE (SIZE(1 .. 36)) OF GANSSAlmanacElement
    -- GANSS Almanac Model
    GANSSAlmanacElement

_0Almanac_KeplerianSet7

    INTEGER (-8192 .. 8191)

_0Almanac_KeplerianSet6

    INTEGER (-32768 .. 32767)

_0Almanac_KeplerianSet5

    INTEGER (-32768 .. 32767)

_0Almanac_KeplerianSet4

    INTEGER (-32768 .. 32767)

_0Almanac_KeplerianSet

    INTEGER (0 .. 2047)

_0Almanac_KeplerianSet8

    INTEGER (-1024..1023)

_0Almanac_KeplerianSet3

    INTEGER (-65536 .. 65535)

_0Almanac_KeplerianSet2

    INTEGER (0 .. 15)

_0Almanac_KeplerianSet1

    INTEGER (-1024 .. 1023)

_0Almanac_KeplerianSet0

    INTEGER (-1024 .. 1023)

_0Almanac_NAVKeplerianSet0

    INTEGER (-32768..32767)

_0Almanac_NAVKeplerianSet3

    INTEGER (0..16777215)

_0Almanac_NAVKeplerianSet4

    INTEGER (-8388608..8388607)

_0Almanac_NAVKeplerianSet1

    INTEGER (-32768..32767)

_0Almanac_NAVKeplerianSet2

    INTEGER (0..255)

_0Almanac_NAVKeplerianSet8

    INTEGER (-1024..1023)

_0Almanac_NAVKeplerianSet7

    INTEGER (-1024..1023)

_0Almanac_NAVKeplerianSet6

    INTEGER (-8388608..8388607)

_0Almanac_NAVKeplerianSet5

    INTEGER (-8388608..8388607)

_0Almanac_NAVKeplerianSet

    INTEGER (0..65535)

_0Almanac_ReducedKeplerianSet1

    INTEGER (-64..63)

_0Almanac_ReducedKeplerianSet0

    INTEGER (-64..63)

_0Almanac_ReducedKeplerianSet

    INTEGER (-128..127)

_0Almanac_MidiAlmanacSet7

    INTEGER (-512..511)

_0Almanac_MidiAlmanacSet

    INTEGER (0..2047)

_0Almanac_MidiAlmanacSet0

    INTEGER (-1024..1023)

_0Almanac_MidiAlmanacSet1

    INTEGER (-1024..1023)

_0Almanac_MidiAlmanacSet2

    INTEGER (0..131071)

_0Almanac_MidiAlmanacSet3

    INTEGER (-32768..32767)

_0Almanac_MidiAlmanacSet4

    INTEGER (-32768..32767)

_0Almanac_MidiAlmanacSet5

    INTEGER (-32768..32767)

_0Almanac_MidiAlmanacSet6

    INTEGER (-1024..1023)

_0Almanac_GlonassAlmanacSet0

    INTEGER (1..24)

_0Almanac_GlonassAlmanacSet9

    INTEGER (-512..511)

_0Almanac_GlonassAlmanacSet

    INTEGER (1..1461)

_0Almanac_GlonassAlmanacSet2

    INTEGER (-1048576..1048575)

_0Almanac_GlonassAlmanacSet1

    INTEGER (0..31)

_0Almanac_GlonassAlmanacSet4

    INTEGER (-131072..131071)

_0Almanac_GlonassAlmanacSet3

    INTEGER (0..2097151)

_0Almanac_GlonassAlmanacSet6

    INTEGER (-64..63)

_0Almanac_GlonassAlmanacSet5

    INTEGER (-2097152..2097151)

_0Almanac_GlonassAlmanacSet8

    INTEGER (-32768..32767)

_0Almanac_GlonassAlmanacSet11

    BIT STRING (SIZE(2))             OPTIONAL

_0Almanac_GlonassAlmanacSet7

    INTEGER (0..32767)

_0Almanac_GlonassAlmanacSet10

    INTEGER (0..1)

_0Almanac_ECEFsbasAlmanacSet2

    INTEGER (-16384..16383)

_0Almanac_ECEFsbasAlmanacSet3

    INTEGER (-256..255)

_0Almanac_ECEFsbasAlmanacSet4

    INTEGER (-4..3)

_0Almanac_ECEFsbasAlmanacSet5

    INTEGER (-4..3)

_0Almanac_ECEFsbasAlmanacSet

    INTEGER (0..3)

_0Almanac_ECEFsbasAlmanacSet0

    BIT STRING (SIZE(8))

_0Almanac_ECEFsbasAlmanacSet1

    INTEGER (-16384..16383)

_0Almanac_ECEFsbasAlmanacSet6

    INTEGER (-8..7)

_0Almanac_ECEFsbasAlmanacSet7

    INTEGER (0..2047)

_0GANSSUTCModel6

    INTEGER (-128..127)

_0GANSSUTCModel5

    INTEGER (-128..127)

_0GANSSUTCModel4

    INTEGER (0..255)

_0GANSSUTCModel3

    INTEGER (-128..127)

_0GANSSUTCModel2

    INTEGER (0..255)

_0GANSSUTCModel1

    INTEGER (0..255)

_0GANSSUTCModel0

    INTEGER (-2147483648..2147483647)

_0GANSSUTCModel

    INTEGER (-8388608..8388607)

_0GANSSEphemerisExtensionHeader

    INTEGER(1..8)

_0GANSSEphemerisExtensionHeader0

    INTEGER(1..512)

_0GANSSEphemerisExtensionTime

    INTEGER(0..8191)

_0ReferenceNavModel10

    INTEGER (-32768..32767)

_0ReferenceNavModel

    INTEGER (0..37799)

_0ReferenceNavModel8

    INTEGER (-2147483648..2147483647)

_0ReferenceNavModel9

    INTEGER (-32768..32767)

_0ReferenceNavModel4

    INTEGER (0..4294967295)

_0ReferenceNavModel5

    INTEGER (-8192..8191)

_0ReferenceNavModel6

    INTEGER (0.. 4294967295)

_0ReferenceNavModel7

    INTEGER (-2147483648..2147483647)

_0ReferenceNavModel0

    INTEGER (-2147483648..2147483647)

_0ReferenceNavModel11

    INTEGER (-32768..32767)

_0ReferenceNavModel12

    INTEGER (-32768..32767)

_0ReferenceNavModel1

    INTEGER (-32768..32767)

_0ReferenceNavModel13

    INTEGER (-32768..32767)

_0ReferenceNavModel2

    INTEGER (-2147483648..2147483647)

_0ReferenceNavModel14

    INTEGER (-32768..32767)

_0ReferenceNavModel3

    INTEGER (-8388608..8388607)

SeqOfGANSSRefOrbit

    SeqOfGANSSRefOrbit ::= SEQUENCE (SIZE(1..32)) OF GANSSReferenceOrbit
    --The number of reference orbits can be read from number of elements in this sequence
    GANSSReferenceOrbit

GANSSEphemerisDeltaMatrix

    GANSSEphemerisDeltaMatrix ::= SEQUENCE (SIZE(1 .. 128)) OF GANSSEphemerisDeltaEpoch
    GANSSEphemerisDeltaEpoch

_0GANSSDeltaEpochHeader

    INTEGER(1..8)                    OPTIONAL

GANSSDeltaElementList

    GANSSDeltaElementList ::= SEQUENCE (SIZE(1 .. 32)) OF OCTET STRING(SIZE (1..49))
    -- Each octet string element in GANSSDeltaElementList corresponds to one PRN within one epoch
    -- Table 55.11 of the annex shows the organization of the delta ephemeris octet string.
    -- Decoding of each of the octet strings is accomplished by consulting the ephemerisDeltaSizes
    -- table to learn the length and order of each of the parameters in the ephemerisDelta payload.
    -- Post decode scaling is accomplished by consulting the ephemerisDeltaScales table to learn the
    -- scale factors to apply to the terms in the delta ephemeris.
    -- Ephemeris Delta Bit Sizes.
    GANSSEphemerisDeltaBitSizes

_0GANSSDeltaElementList

    OCTET STRING(SIZE (1..49))
    -- Each octet string element in GANSSDeltaElementList corresponds to one PRN within one epoch
    -- Table 55.11 of the annex shows the organization of the delta ephemeris octet string.
    -- Decoding of each of the octet strings is accomplished by consulting the ephemerisDeltaSizes
    -- table to learn the length and order of each of the parameters in the ephemerisDelta payload.
    -- Post decode scaling is accomplished by consulting the ephemerisDeltaScales table to learn the
    -- scale factors to apply to the terms in the delta ephemeris.
    -- Ephemeris Delta Bit Sizes.
    GANSSEphemerisDeltaBitSizes

_0GANSSEphemerisDeltaBitSizes7

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes6

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes5

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes4

    INTEGER(1..14)

_0GANSSEphemerisDeltaBitSizes9

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes8

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes11

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes12

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes13

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes14

    INTEGER(1..10)

_0GANSSEphemerisDeltaBitSizes2

    INTEGER(1..24)

_0GANSSEphemerisDeltaBitSizes3

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes0

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes1

    INTEGER(1..32)

_0GANSSEphemerisDeltaBitSizes10

    INTEGER(1..16)

_0GANSSEphemerisDeltaBitSizes15

    INTEGER(1..10)

_0GANSSEphemerisDeltaScales10

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales6

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales7

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales4

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales15

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales5

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales14

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales2

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales13

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales3

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales12

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales0

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales1

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales11

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales9

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales8

    INTEGER(-16..15)

_0GANSSEphemerisDeltaScales

    INTEGER(-16..15)

_0GANSSSatEventsInfo

    BIT STRING (SIZE (64))

_0GANSSSatEventsInfo0

    BIT STRING (SIZE (64))

_0UTCmodelSet2

    INTEGER (-32768..32767)

_0UTCmodelSet27

    INTEGER (-128..127)

_0UTCmodelSet26

    BIT STRING (SIZE(4))

_0UTCmodelSet24

    INTEGER (0..8191)

_0UTCmodelSet25

    INTEGER (0..255)

_0UTCmodelSet22

    INTEGER (-128.. 127)

_0UTCmodelSet23

    INTEGER (0..65535)

_0UTCmodelSet20

    INTEGER (-4096.. 4095)

_0UTCmodelSet21

    INTEGER (-64..63)

_0UTCmodelSet32

    INTEGER (-512..511)                     OPTIONAL

_0UTCmodelSet31

    INTEGER (-1024..1023)                     OPTIONAL

_0UTCmodelSet30

    INTEGER (-2147483648..2147483647)

_0UTCmodelSet3

    INTEGER (1..1461)

_0UTCmodelSet33

    BIT STRING (SIZE(2))                     OPTIONAL

_0UTCmodelSet41

    INTEGER (0..255)

_0UTCmodelSet40

    INTEGER (-2147483648..2147483647)

_0UTCmodelSet43

    INTEGER (-128..127)

_0UTCmodelSet42

    INTEGER (0..255)

_0UTCmodelSet45

    INTEGER (-128..127)

_0UTCmodelSet44

    INTEGER (0..255)

_0UTCmodelSet47

    INTEGER (0..7)

_0UTCmodelSet46

    INTEGER (-128..127)

_0UTCmodelSet4

    INTEGER (-8388608..8388607)

GANSS_ID1

    GANSS-ID1 ::= SEQUENCE (SIZE(1..64)) OF GANSS-ID1-element
    GANSS-ID1-element

GANSS_ID3

    GANSS-ID3 ::= SEQUENCE (SIZE(1..64)) OF GANSS-ID3-element
    GANSS-ID3-element

_0GANSS_ID3_element

    INTEGER (-7..13)

GANSSDiffCorrectionsValidityPeriod

    GANSSDiffCorrectionsValidityPeriod ::= SEQUENCE (SIZE (1..3)) OF DGANSSExtensionSgnTypeElement
    DGANSSExtensionSgnTypeElement

SeqOfDGANSSExtensionSgnElement

    SeqOfDGANSSExtensionSgnElement ::= SEQUENCE (SIZE (1..16)) OF DGANSSExtensionSgnElement
    DGANSSExtensionSgnElement

_0DGANSSExtensionSgnElement

    INTEGER(0..7)

_0DGANSSExtensionSgnElement0

    INTEGER(0..7)

RequiredResponseTime

    RequiredResponseTime ::= INTEGER  (1..128)
    -- Control header for additional GPS assistance data
    Add-GPS-AssistData

_0GPSClockModel

    INTEGER (-128..127)

_0GPSClockModel2

    INTEGER (-128..127)

_0GPSClockModel0

    INTEGER (-32768..32767)

_0GPSClockModel1

    INTEGER (-2097152..2097151)

_0GPSEphemerisExtensionHeader0

    INTEGER(1..512)

_0GPSEphemerisExtensionHeader

    INTEGER(1..8)

_0GPSEphemerisExtensionTime

    INTEGER (0..604799)

SeqOfGPSRefOrbit

    SeqOfGPSRefOrbit ::= SEQUENCE (SIZE(1..32)) OF GPSReferenceOrbit
    --The number of reference orbits can be read from number of elements in this sequence
    GPSReferenceOrbit

GPSEphemerisDeltaMatrix

    GPSEphemerisDeltaMatrix ::= SEQUENCE (SIZE(1 .. 128)) OF GPSEphemerisDeltaEpoch
    GPSEphemerisDeltaEpoch

_0GPSDeltaEpochHeader

    INTEGER(1..8)                OPTIONAL

GPSDeltaElementList

    GPSDeltaElementList ::= SEQUENCE (SIZE(1 .. 32)) OF OCTET STRING(SIZE (1..47))
    -- Each octet string element in GPSDeltaElementList corresponds to one PRN within one epoch
    -- Table A.29.m of the annex shows the organization of the delta ephemeris octet string.
    -- Decoding of each of the octet strings is accomplished by consulting the ephemerisDeltaSizes
    -- table to learn the length and order of each of the parameters in the ephemerisDelta payload
    -- Post decode scaling is accomplished by consulting the ephemerisDeltaScales table to learn the.
    -- scale factors to apply to the terms in the delta ephemeris
    -- Ephemeris Delta Bit Sizes.
    GPSEphemerisDeltaBitSizes

_0GPSDeltaElementList

    OCTET STRING(SIZE (1..47))
    -- Each octet string element in GPSDeltaElementList corresponds to one PRN within one epoch
    -- Table A.29.m of the annex shows the organization of the delta ephemeris octet string.
    -- Decoding of each of the octet strings is accomplished by consulting the ephemerisDeltaSizes
    -- table to learn the length and order of each of the parameters in the ephemerisDelta payload
    -- Post decode scaling is accomplished by consulting the ephemerisDeltaScales table to learn the.
    -- scale factors to apply to the terms in the delta ephemeris
    -- Ephemeris Delta Bit Sizes.
    GPSEphemerisDeltaBitSizes

_0GPSEphemerisDeltaBitSizes3

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes2

    INTEGER(1..24)

_0GPSEphemerisDeltaBitSizes5

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes4

    INTEGER(1..14)

_0GPSEphemerisDeltaBitSizes7

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes6

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes9

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes8

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes1

    INTEGER(1..32)

_0GPSEphemerisDeltaBitSizes0

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes14

    INTEGER(1..10)

_0GPSEphemerisDeltaBitSizes13

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes10

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes12

    INTEGER(1..16)

_0GPSEphemerisDeltaBitSizes11

    INTEGER(1..16)

_0GPSEphemerisDeltaScales13

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales14

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales10

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales0

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales11

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales12

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales1

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales2

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales3

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales4

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales5

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales6

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales7

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales8

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales9

    INTEGER(-16..15)

_0GPSEphemerisDeltaScales

    INTEGER(-16..15)

_0GPSSatEventsInfo

    BIT STRING (SIZE (32))

_0GPSSatEventsInfo0

    BIT STRING (SIZE (32))

DGPSCorrectionsValidityPeriod

    DGPSCorrectionsValidityPeriod ::= SEQUENCE (SIZE (1..16)) OF DGPSExtensionSatElement
    DGPSExtensionSatElement

_0DGPSExtensionSatElement0

    INTEGER(0..7)

_0DGPSExtensionSatElement

    INTEGER(0..7)

_0GPSReferenceTime_R10_Ext

    INTEGER(0..7)

GPSAcquisAssist_R10_Ext

    GPSAcquisAssist-R10-Ext ::= SEQUENCE(SIZE (1..16)) OF GPSAcquisAssist-R10-Ext-Element
    GPSAcquisAssist-R10-Ext-Element

_0GPSAcquisAssist_R10_Ext_Element

    INTEGER(0..15)

_0GPSAcquisAssist_R10_Ext_Element0

    INTEGER(0..15)

_0GANSSLocationInfo

    INTEGER (0 .. 16384)     OPTIONAL

_0GANSSLocationInfo0

    INTEGER (0 .. 7)         OPTIONAL

_0GANSSLocationInfo1

    INTEGER(0 .. 1)         OPTIONAL

PositionData

    PositionData ::= BIT STRING {
         e-otd               (0),
        gps                (1),
        galileo           (2),
        sbas                (3),
        modernizedGPS      (4),
        qzss                (5),
        glonass           (6) } (SIZE (3..16))
    -- GANSS TOD modulo 1 hour
    GANSSTODm

GANSSTODm

    GANSSTODm ::= INTEGER (0 .. 3599999)
    ReferenceFrame

_0ReferenceFrame

    INTEGER (0 .. 65535)

_0ReferenceFrame0

    INTEGER (0 .. 63) OPTIONAL

SeqOfGANSS_MsrSetElement

    SeqOfGANSS-MsrSetElement ::= SEQUENCE (SIZE(1..3)) OF GANSS-MsrSetElement
    -- GANSS measurement information 1-3 times in a message
    GANSS-MsrSetElement

_0GANSS_MsrSetElement

    INTEGER (0 .. 127)     OPTIONAL

SeqOfGANSS_MsrElement

    SeqOfGANSS-MsrElement ::= SEQUENCE (SIZE(1..8)) OF GANSS-MsrElement
    GANSS-MsrElement

_0GANSS_MsrElement

    INTEGER (0..7)     OPTIONAL

SeqOfGANSS_SgnTypeElement

    SeqOfGANSS-SgnTypeElement ::= SEQUENCE (SIZE(1..8)) OF GANSS-SgnTypeElement
    GANSS-SgnTypeElement

_0GANSS_SgnTypeElement

    INTEGER (0 .. 127)                OPTIONAL

SeqOfGANSS_SgnElement

    SeqOfGANSS-SgnElement ::= SEQUENCE (SIZE(1..16)) OF GANSS-SgnElement
    GANSS-SgnElement

_0GANSS_SgnElement5

    INTEGER (0 .. 33554431)     OPTIONAL

_0GANSS_SgnElement4

    INTEGER (-32768 .. 32767)     OPTIONAL

_0GANSS_SgnElement

    INTEGER (0 .. 63)

_0GANSS_SgnElement3

    INTEGER (0..63)

_0GANSS_SgnElement2

    INTEGER (0 .. 127)             OPTIONAL

_0GANSS_SgnElement1

    INTEGER (0 .. 2097151)

_0GANSS_SgnElement0

    INTEGER (0 .. 3)             OPTIONAL

NonGANSSPositionMethods

    NonGANSSPositionMethods ::= BIT STRING {
        msAssistedEOTD     (0),
        msBasedEOTD          (1),
        msAssistedGPS     (2), -- If this bit is set, gpsAssistance in AssistanceSupported IE
                              -- shall be present
        msBasedGPS          (3), -- If this bit is set, gpsAssistance in AssistanceSupported IE
                              -- shall be present
        standaloneGPS     (4) } (SIZE (1..16))
    GANSSPositionMethods

GANSSPositionMethods

    GANSSPositionMethods ::= SEQUENCE (SIZE(1..16)) OF GANSSPositionMethod
    GANSSPositionMethod

_0GANSSPositionMethod

    INTEGER (0..7)                 OPTIONAL

GANSSPositioningMethodTypes

    GANSSPositioningMethodTypes ::= BIT STRING {
        msAssisted    (0),    -- If this bit is set, gANSSAssistanceSet in AssistanceSupported IE
                            -- shall be present.
        msBased         (1),    -- If this bit is set, gANSSAssistanceSet in AssistanceSupported IE
                            -- shall be present.
        standalone    (2) } (SIZE (1..8))
    -- indicates MS support for particular GANSS signals and frequencies
    GANSSSignals

GANSSSignals

    GANSSSignals ::= BIT STRING {
        signal1 (0),
        signal2 (1),
        signal3 (2),
        signal4 (3),
        signal5 (4),
        signal6 (5),
        signal7 (6),
        signal8 (7) } (SIZE (1..8))
    SBASID

SBASID

    SBASID ::= BIT STRING {
        waas      (0),
        egnos      (1),
        masas      (2),
        gagan      (3) } (SIZE (1..8))
    -- indicates MS support of multiple measurement sets for MS assisted position methods
    MultipleMeasurementSets

MultipleMeasurementSets

    MultipleMeasurementSets ::= BIT STRING {
        eotd     (0),
        gps          (1),
        ganss     (2) } (SIZE (1..8))
    -- indicates MS support of different types of assistance data
    AssistanceSupported

GPSAssistance

    GPSAssistance ::= BIT STRING {
        almanac                    (0),
        uTCmodel                (1),
        ionosphericModel        (2),
        navigationmodel            (3),
        dGPScorrections            (4),
        referenceLocation        (5),
        referenceTime            (6),
        acquisitionAssistance    (7),
        realTimeIntegrity        (8),
        ephemerisExtension        (9),
        ephemerisExtensionCheck    (10)} (SIZE (1..16))
    -- GANSS assistance data supported
    GANSSAssistanceSet

CommonGANSSAssistance

    CommonGANSSAssistance ::= BIT STRING {
        referenceTime             (0),
        referenceLocation         (1),
        ionosphericModel         (3),
        addIonosphericModel         (4),
        earthOrientationParam     (5)  } (SIZE (1..8))
    SpecificGANSSAssistance

SpecificGANSSAssistance

    SpecificGANSSAssistance ::= SEQUENCE (SIZE(1..16)) OF GANSSAssistanceForOneGANSS
    -- assistance data supported for a particular GANSS system
    GANSSAssistanceForOneGANSS

_0GANSSAssistanceForOneGANSS

    INTEGER (0..7)     OPTIONAL

GANSSAssistance

    GANSSAssistance ::= BIT STRING {
        realTimeIntegrity                (0),
        differentialCorrections            (1),
        almanac                            (2),
        referenceMeasurementInformation    (3),
        navigationModel                    (4),
        timeModelGNSS-UTC                (5),
        timeModelGNSS-GNSS                (6),
        databitassistance                (7),
        ephemerisExtension                (8),
        ephemerisExtensionCheck            (9),
        addUTCmodel                        (10),
        auxiliaryInformation            (11)  } (SIZE (1..16))
    GANSSAdditionalAssistanceChoices

GANSSAdditionalAssistanceChoices

    GANSSAdditionalAssistanceChoices ::= SEQUENCE (SIZE(1..16)) OF GANSSAdditionalAssistanceChoicesForOneGANSS
    GANSSAdditionalAssistanceChoicesForOneGANSS

_0GANSSAdditionalAssistanceChoicesForOneGANSS

    INTEGER (0..7)     OPTIONAL

GANSSModelID

    GANSSModelID ::= BIT STRING {
        model1 (0),
        model2 (1),
        model3 (2),
        model4 (3),
        model5 (4),
        model6 (5),
        model7 (6),
        model8 (7) } (SIZE (1..8))
    -- indicates assistance data that may be needed by the MS
    -- These elements are coded as defined in TS 49.031 with the exceptions defined in section A.8.2.3
    AssistanceNeeded

PositionMethod

    ENUMERATED {
    eotd (0),
    gps (1),
    gpsOrEOTD (2)
    }
    -- Measurement request response time
    MeasureResponseTime

UseMultipleSets

    ENUMERATED {
    multipleSets (0),        -- multiple sets are allowed
    oneSet (1)                -- sending of multiple is not allowed
    }
    -- Environment characterization
    EnvironmentCharacter

EnvironmentCharacter

    ENUMERATED {
    badArea (0),        -- bad urban or suburban, heavy multipath and NLOS
    notBadArea (1),        -- light multipath and NLOS
    mixedArea (2),        -- not defined or mixed environment
    ...
    }
    -- E-OTD reference BTS for Assitance data IE
    ReferenceAssistData

TimeSlotScheme

    ENUMERATED {
    equalLength (0),
    variousLength (1)
    }
    -- Time slot (modulo)
    ModuloTimeSlot

ReferenceRelation

    ENUMERATED {
    secondBTSThirdSet (0),    -- 1st BTS related to 1st and 2nd sets
    secondBTSSecondSet (1),    -- 1st BTS related to 1st and 3rd sets
    firstBTSFirstSet (2)    -- 1st BTS related to 1st set
    }
    -- Reference BTS Identity, this element contains number of
    -- BTSs told nbrOfReferenceBTSs field in Multiple sets element)
    ReferenceIdentity

MpathIndic

    ENUMERATED {
    notMeasured (0),
    low (1),
    medium (2),
    high (3)
    }
    -- Location error IE
    LocationError

LocErrorReason

    ENUMERATED {
    unDefined (0),
    notEnoughBTSs (1),
    notEnoughSats (2),
    eotdLocCalAssDataMissing (3),
    eotdAssDataMissing (4),
    gpsLocCalAssDataMissing (5),
    gpsAssDataMissing (6),
    methodNotSupported (7),
    notProcessed (8),
    refBTSForGPSNotServingBTS (9),
    refBTSForEOTDNotServingBTS (10),
    ...,
    notEnoughGANSSSats (11),
     ganssAssDataMissing (12),
    refBTSForGANSSNotServingBTS (13)
    }
    -- exception handling:
    -- an unrecognized value shall be treated the same as value 0
    -- defines additional assistance data needed for any new location attempt
    -- MS shall retain any assistance data already received
    AdditionalAssistanceData

ErrorCodes

    ENUMERATED {
    unDefined (0),
    missingComponet (1),
    incorrectData (2),
    missingIEorComponentElement (3),
    messageTooShort (4),
    unknowReferenceNumber (5),
    ...
    }
    -- exception handling:
    -- an unrecognized value shall be treated the same as value 0
    -- GPS assistance data IE
    GPS-AssistData

MoreAssDataToBeSent

    ENUMERATED {
    noMoreMessages (0),            -- This is the only or last Assistance Data message used to deliver
    -- the entire set of assistance data.
    moreMessagesOnTheWay (1)    -- The SMLC will send more Assistance Data messages or a final RRLP
    -- Measure Position Request message to deliver the
    -- the entire set of assistance data.
    }
    -- Control header of the GPS assistance data
    ControlHeader

UlPseudoSegInd

    ENUMERATED {
    firstOfMany (0),
    secondOfMany(1)
    }
    Rel5-MsrPosition-Req-Extension

MsrPosition_Req

    MsrPosition-Req ::= SEQUENCE {
        positionInstruct        PositionInstruct,
        referenceAssistData        ReferenceAssistData        OPTIONAL,
        msrAssistData            MsrAssistData            OPTIONAL,
        systemInfoAssistData    SystemInfoAssistData    OPTIONAL,
        gps-AssistData            GPS-AssistData            OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release 98 extension element
    rel98-MsrPosition-Req-extension            Rel98-MsrPosition-Req-Extension            OPTIONAL,
        -- Release 5 extension element
    rel5-MsrPosition-Req-extension            Rel5-MsrPosition-Req-Extension            OPTIONAL,
        -- Release 7 extension element
    rel7-MsrPosition-Req-extension            Rel7-MsrPosition-Req-Extension            OPTIONAL
    }
    -- add this defintion to RRLP-Components module
    -- Measurement Position response component
    MsrPosition-Rsp

MsrPosition_Rsp

    MsrPosition-Rsp ::= SEQUENCE {
        multipleSets            MultipleSets            OPTIONAL,
        referenceIdentity        ReferenceIdentity        OPTIONAL,
        otd-MeasureInfo            OTD-MeasureInfo            OPTIONAL,
        locationInfo            LocationInfo            OPTIONAL,
        gps-MeasureInfo            GPS-MeasureInfo            OPTIONAL,
        locationError            LocationError            OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extension here
        rel-98-MsrPosition-Rsp-Extension
                                Rel-98-MsrPosition-Rsp-Extension        OPTIONAL,
        rel-5-MsrPosition-Rsp-Extension
                                Rel-5-MsrPosition-Rsp-Extension        OPTIONAL,
        -- When RRLP pseudo-segmentation is used, rel-5-MsrPosition-Rsp-Extension
        -- and other possible future extensions should be the ones included in
        -- the 2nd MsrPosition-Rsp component.
        rel-7-MsrPosition-Rsp-Extension
                                Rel-7-MsrPosition-Rsp-Extension        OPTIONAL
    }
    -- add this defintion to RRLP-Components module
    -- Assistance Data component
    AssistanceData

AssistanceData

    AssistanceData ::= SEQUENCE {
        referenceAssistData    ReferenceAssistData            OPTIONAL,
        msrAssistData            MsrAssistData            OPTIONAL,
        systemInfoAssistData    SystemInfoAssistData    OPTIONAL,
        gps-AssistData            GPS-AssistData            OPTIONAL,
        moreAssDataToBeSent        MoreAssDataToBeSent        OPTIONAL,    -- If not present, interpret as only
                                                                    -- Assistance Data component used to
                                                                    -- deliver entire set of assistance
                                                                    -- data.
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extension here
        rel98-AssistanceData-Extension    Rel98-AssistanceData-Extension    OPTIONAL,
        rel5-AssistanceData-Extension    Rel5-AssistanceData-Extension    OPTIONAL,
     rel7-AssistanceData-Extension Rel7-AssistanceData-Extension OPTIONAL
    }
    -- add this defintion to RRLP-Components module
    -- Protocol Error component
    ProtocolError

ProtocolError

    ProtocolError ::= SEQUENCE {
        errorCause                ErrorCodes,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        -- Release extensions here
        rel-5-ProtocolError-Extension Rel-5-ProtocolError-Extension        OPTIONAL
    }
    -- add this definition to RRLP-Components module
    -- Positioning Capability request component
    PosCapability-Req

PosCapability_Req

    PosCapability-Req ::= SEQUENCE {
        extended-reference            Extended-reference,
        gANSSPositionMethods        GANSSPositionMethods    OPTIONAL,
        extensionContainer            ExtensionContainer        OPTIONAL,
        ...
    }
    -- add this definition to RRLP-Components module
    -- Positioning Capability response component
    PosCapability-Rsp

PosCapability_Rsp

    PosCapability-Rsp ::= SEQUENCE {
        extended-reference        Extended-reference,
        posCapabilities            PosCapabilities,
    -- assistanceSupported shall be included if and only if any of the assistance data is supported
        assistanceSupported        AssistanceSupported        OPTIONAL,
        assistanceNeeded        AssistanceNeeded        OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...
    }
    -- add these defintions to RRLP-Components module
    -- Position instructions
    PositionInstruct

PositionInstruct

    PositionInstruct ::= SEQUENCE {
        -- Method type
        methodType                MethodType,
        positionMethod            PositionMethod,
        measureResponseTime        MeasureResponseTime,
        useMultipleSets            UseMultipleSets,
        environmentCharacter    EnvironmentCharacter    OPTIONAL
    }
    --
    MethodType

AccuracyOpt

    AccuracyOpt ::= SEQUENCE {
        accuracy        Accuracy    OPTIONAL
    }
    -- The values of this field are defined in 3GPP TS 23.032 (Uncertainty code)
    Accuracy

ReferenceAssistData

    ReferenceAssistData ::= SEQUENCE {
        bcchCarrier        BCCHCarrier,                        -- BCCH carrier
        bsic            BSIC,                                -- BSIC
        timeSlotScheme    TimeSlotScheme,                     -- Timeslot scheme
        btsPosition        BTSPosition            OPTIONAL
    }
    -- ellipsoid point and
    -- ellipsoid point with altitude and uncertainty ellipsoid shapes are supported
    BTSPosition

MsrAssistData

    MsrAssistData ::= SEQUENCE {
         msrAssistList SeqOfMsrAssistBTS
    }
    SeqOfMsrAssistBTS

MsrAssistBTS

    MsrAssistBTS ::= SEQUENCE {
        bcchCarrier            BCCHCarrier,        -- BCCH carrier
        bsic                BSIC,                -- BSIC
        multiFrameOffset    MultiFrameOffset,     -- multiframe offset
        timeSlotScheme        TimeSlotScheme,        -- Timeslot scheme
        roughRTD            RoughRTD,            -- rough RTD value
        -- Location Calculation Assistance data is moved here
        calcAssistanceBTS    CalcAssistanceBTS    OPTIONAL
    }
    -- Multiframe offset
    MultiFrameOffset

SystemInfoAssistData

    SystemInfoAssistData ::= SEQUENCE {
        systemInfoAssistList     SeqOfSystemInfoAssistBTS
    }
    SeqOfSystemInfoAssistBTS

AssistBTSData

    AssistBTSData ::= SEQUENCE {
        bsic                BSIC,                -- BSIC
        multiFrameOffset    MultiFrameOffset,    -- multiframe offset
        timeSlotScheme        TimeSlotScheme,        -- Timeslot scheme
        roughRTD            RoughRTD,            -- rough RTD value
        -- Location Calculation Assistance data
        calcAssistanceBTS    CalcAssistanceBTS    OPTIONAL
    }
    -- E-OTD Location calculation assistance data,
    -- CalcAssistanceBTS element is optional not subfields
    CalcAssistanceBTS

CalcAssistanceBTS

    CalcAssistanceBTS ::= SEQUENCE {
        fineRTD                FineRTD,        -- fine RTD value between base stations
        referenceWGS84        ReferenceWGS84    -- reference coordinates
    }
    -- Coordinates of neighbour BTS, WGS-84 ellipsoid
    ReferenceWGS84

ReferenceWGS84

    ReferenceWGS84 ::= SEQUENCE {
        relativeNorth    RelDistance,                -- relative distance (south negative)
        relativeEast    RelDistance,                -- relative distance (west negative)
        -- Relative Altitude is not always known
        relativeAlt        RelativeAlt        OPTIONAL    -- relative altitude
    }
    -- Fine RTD value between this BTS and the reference BTS
    FineRTD

MultipleSets

    MultipleSets ::= SEQUENCE {
        -- number of reference sets
        nbrOfSets            INTEGER (2..3),
        -- This field actually tells the number of reference BTSs
        nbrOfReferenceBTSs    INTEGER (1..3),
        -- This field is conditional and included optionally only if
        -- nbrOfSets is 3 and number of reference BTSs is 2.
        referenceRelation        ReferenceRelation        OPTIONAL
    }
    -- Relation between refence BTSs and sets
    ReferenceRelation

ReferenceIdentity

    ReferenceIdentity ::= SEQUENCE {
        -- Reference BTS list
        refBTSList        SeqOfReferenceIdentityType
    }
    SeqOfReferenceIdentityType

BSICAndCarrier

    BSICAndCarrier ::= SEQUENCE {
        carrier    BCCHCarrier,
        bsic        BSIC
    }
    RequestIndex

CellIDAndLAC

    CellIDAndLAC ::= SEQUENCE {
        referenceLAC    LAC,                -- Location area code
        referenceCI        CellID                -- Cell identity
    }
    CellID

OTD_MeasureInfo

    OTD-MeasureInfo ::= SEQUENCE {
        -- Measurement info elements, OTD-MsrElement is repeated number of times
        -- told in nbrOfReferenceBTSs in MultipleSets, default value is 1
        otdMsrFirstSets        OTD-MsrElementFirst,
        -- if more than one sets are present this element is repeated
        -- NumberOfSets - 1 (-1 = first set)
        otdMsrRestSets        SeqOfOTD-MsrElementRest        OPTIONAL
    }
    SeqOfOTD-MsrElementRest

OTD_MsrElementFirst

    OTD-MsrElementFirst ::= SEQUENCE {
        refFrameNumber            INTEGER (0..42431),                 -- Frame number modulo 42432
        referenceTimeSlot        ModuloTimeSlot,
        toaMeasurementsOfRef    TOA-MeasurementsOfRef    OPTIONAL,
        stdResolution            StdResolution,
        taCorrection            INTEGER (0..960)        OPTIONAL,    -- TA correction
        -- measured neighbors in OTD measurements
        otd-FirstSetMsrs         SeqOfOTD-FirstSetMsrs     OPTIONAL
    }
    SeqOfOTD-FirstSetMsrs

OTD_MsrElementRest

    OTD-MsrElementRest ::= SEQUENCE {
        refFrameNumber            INTEGER (0..42431),                     -- Frame number modulo 42432
        referenceTimeSlot        ModuloTimeSlot,
        toaMeasurementsOfRef    TOA-MeasurementsOfRef        OPTIONAL,
        stdResolution            StdResolution,
        taCorrection            INTEGER (0..960)            OPTIONAL,    -- TA correction
        -- measured neighbors in OTD measurements
        otd-MsrsOfOtherSets     SeqOfOTD-MsrsOfOtherSets    OPTIONAL
    }
    SeqOfOTD-MsrsOfOtherSets

TOA_MeasurementsOfRef

    TOA-MeasurementsOfRef ::= SEQUENCE {
        refQuality            RefQuality,
        numOfMeasurements    NumOfMeasurements
    }
    RefQuality

OTD_Measurement

    OTD-Measurement ::= SEQUENCE {
        nborTimeSlot    ModuloTimeSlot,
        eotdQuality        EOTDQuality,
        otdValue        OTDValue
    }
    -- This measurement contains the BTS identity and measurement
    OTD-MeasurementWithID

OTD_MeasurementWithID

    OTD-MeasurementWithID ::=SEQUENCE {
        neighborIdentity    NeighborIdentity,
        nborTimeSlot        ModuloTimeSlot,
        eotdQuality            EOTDQuality,
        otdValue            OTDValue
    }
    EOTDQuality

EOTDQuality

    EOTDQuality ::= SEQUENCE {
        nbrOfMeasurements    INTEGER    (0..7),
        stdOfEOTD            INTEGER (0..31)
    }
    NeighborIdentity

MultiFrameCarrier

    MultiFrameCarrier ::= SEQUENCE {
        bcchCarrier            BCCHCarrier,
        multiFrameOffset    MultiFrameOffset
    }
    -- OTD measurement value for neighbour
    OTDValue

LocationInfo

    LocationInfo ::= SEQUENCE {
        refFrame        INTEGER (0..65535),            -- Reference Frame number
        -- If refFrame is within (42432..65535), it shall be ignored by the receiver
        -- in that case the MS should provide GPS TOW if available
        gpsTOW            INTEGER (0..14399999)    OPTIONAL,    -- GPS TOW
        fixType            FixType,
        -- Note that applicable range for refFrame is 0 - 42431
        -- Possible shapes carried in posEstimate are
        -- ellipsoid point,
        -- ellipsoid point with uncertainty circle
        -- ellipsoid point with uncertainty ellipse
        -- ellipsoid point with altitude and uncertainty ellipsoid
        posEstimate        Ext-GeographicalInformation
    }
    FixType

GPS_MeasureInfo

    GPS-MeasureInfo ::= SEQUENCE {
        -- Measurement info elements
        -- user has to make sure that in this element is number of elements
        -- defined in reference BTS identity
        gpsMsrSetList    SeqOfGPS-MsrSetElement
    }
    SeqOfGPS-MsrSetElement

GPS_MsrSetElement

    GPS-MsrSetElement ::= SEQUENCE {
        refFrame        INTEGER (0..65535)    OPTIONAL,     -- Reference Frame number
        gpsTOW            GPSTOW24b,                        -- GPS TOW
        -- Note that applicable range for refFrame is 0 - 42431
    --N_SAT can be read from number of elements of gps-msrList
        gps-msrList        SeqOfGPS-MsrElement
    }
    -- 24 bit presentation for GPSTOW
    GPSTOW24b

GPS_MsrElement

    GPS-MsrElement ::= SEQUENCE {
        satelliteID        SatelliteID,                -- Satellite identifier
        cNo                INTEGER (0..63),            -- carrier noise ratio
        doppler            INTEGER (-32768..32767),     -- doppler, mulltiply by 0,2
        wholeChips        INTEGER (0..1022),            -- whole value of the code phase measurement
        fracChips        INTEGER (0..1024),            -- fractional value of the code phase measurement
                                                -- a value of 1024 shall not be encoded by the sender
                                                -- the receiver shall consider a value of 1024 to be
                                                -- invalid data
        mpathIndic        MpathIndic,                    -- multipath indicator
        pseuRangeRMSErr    INTEGER (0..63)                -- index
    }
    -- Multipath indicator
    MpathIndic

LocationError

    LocationError ::= SEQUENCE {
        locErrorReason                LocErrorReason,
        additionalAssistanceData    AdditionalAssistanceData    OPTIONAL,
        ...
    }
    LocErrorReason

AdditionalAssistanceData

    AdditionalAssistanceData ::= SEQUENCE {
        gpsAssistanceData        GPSAssistanceData        OPTIONAL,
        extensionContainer        ExtensionContainer        OPTIONAL,
        ...,
        ganssAssistanceData GANSSAssistanceData OPTIONAL
    }
    GPSAssistanceData

GPS_AssistData

    GPS-AssistData ::= SEQUENCE {
        controlHeader        ControlHeader
    }
    -- More Assistance Data To Be Sent IE
    -- More Assistance Data Components On the Way indication for delivery of an entire set of assistance
    -- data in multiple Assistance Data components.
    MoreAssDataToBeSent

ControlHeader

    ControlHeader ::= SEQUENCE {
        -- Field type Present information
        referenceTime        ReferenceTime        OPTIONAL,
        refLocation            RefLocation            OPTIONAL,
        dgpsCorrections        DGPSCorrections        OPTIONAL,
        navigationModel        NavigationModel        OPTIONAL,
        ionosphericModel    IonosphericModel    OPTIONAL,
        utcModel            UTCModel            OPTIONAL,
        almanac                Almanac                OPTIONAL,
        acquisAssist        AcquisAssist        OPTIONAL,
        realTimeIntegrity SeqOf-BadSatelliteSet OPTIONAL
    }
    ReferenceTime

ReferenceTime

    ReferenceTime ::= SEQUENCE {
        gpsTime                GPSTime,
        gsmTime                GSMTime                OPTIONAL,
        gpsTowAssist        GPSTOWAssist        OPTIONAL
    }
    -- GPS Time includes week number and time-of-week (TOW)
    GPSTime

GPSTime

    GPSTime ::= SEQUENCE {
        gpsTOW23b            GPSTOW23b,
        gpsWeek                GPSWeek
    }
    -- GPSTOW, range 0-604799,92, resolution 0,08 sec, 23-bit presentation
    GPSTOW23b

GPSTOWAssistElement

    GPSTOWAssistElement ::= SEQUENCE {
        satelliteID            SatelliteID,
        tlmWord                TLMWord,
        antiSpoof            AntiSpoofFlag,
        alert                AlertFlag,
        tlmRsvdBits            TLMReservedBits
    }
    -- TLM Word, 14 bits
    TLMWord

GSMTime

    GSMTime ::= SEQUENCE {
        bcchCarrier        BCCHCarrier,    -- BCCH carrier
        bsic            BSIC,            -- BSIC
        frameNumber        FrameNumber,
        timeSlot        TimeSlot,
        bitNumber        BitNumber
    }
    -- Frame number
    FrameNumber

RefLocation

    RefLocation ::= SEQUENCE {
        threeDLocation            Ext-GeographicalInformation
    }
    -- DGPS Corrections IE
    DGPSCorrections

DGPSCorrections

    DGPSCorrections ::= SEQUENCE {
        gpsTOW        INTEGER (0..604799),    -- DGPS reference time
        status        INTEGER (0..7),
        -- N_SAT can be read from number of elements of satList
        satList        SeqOfSatElement
    }
    SeqOfSatElement

SatElement

    SatElement ::= SEQUENCE {
        satelliteID        SatelliteID,
    --- Sequence number for ephemeris
        iode             INTEGER (0..239),
        -- User Differential Range Error
        udre            INTEGER (0..3),
        -- Pseudo Range Correction, range is
        -- -655,04 - +655,04,
        pseudoRangeCor    INTEGER (-2047..2047),
        -- Pseudo Range Rate Correction, range is
        -- -4,064 - +4,064,
        rangeRateCor    INTEGER (-127..127),
    -- Delta Pseudo Range Correction 2
        deltaPseudoRangeCor2     INTEGER (-127..127),    -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 2
        deltaRangeRateCor2        INTEGER (-7..7),        -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 3
        deltaPseudoRangeCor3     INTEGER (-127..127),    -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
        -- Delta Pseudo Range Correction 3
        deltaRangeRateCor3        INTEGER (-7..7)            -- This IE shall be ignored by the receiver and
                                                        -- set to zero by the sender
    }
    SatelliteID

NavigationModel

    NavigationModel ::= SEQUENCE {
        navModelList    SeqOfNavModelElement
    }
    -- navigation model satellite list
    SeqOfNavModelElement

NavModelElement

    NavModelElement ::= SEQUENCE {
        satelliteID        SatelliteID,
        satStatus        SatStatus        -- satellite status
    }
    -- the Status of the navigation model
    SatStatus

UncompressedEphemeris

    UncompressedEphemeris ::= SEQUENCE {
        ephemCodeOnL2    INTEGER (0..3),
        ephemURA        INTEGER (0..15),
        ephemSVhealth    INTEGER (0..63),
        ephemIODC        INTEGER    (0..1023),
        ephemL2Pflag    INTEGER (0..1),
        ephemSF1Rsvd    EphemerisSubframe1Reserved,
        ephemTgd        INTEGER (-128..127),
        ephemToc        INTEGER (0..37799),
        ephemAF2        INTEGER (-128..127),
        ephemAF1        INTEGER (-32768..32767),
        ephemAF0        INTEGER (-2097152..2097151),
        ephemCrs        INTEGER (-32768..32767),
        ephemDeltaN        INTEGER (-32768..32767),
        ephemM0            INTEGER (-2147483648..2147483647),
        ephemCuc        INTEGER (-32768..32767),
        ephemE            INTEGER (0..4294967295),
        ephemCus        INTEGER (-32768..32767),
        ephemAPowerHalf    INTEGER (0..4294967295),
        ephemToe        INTEGER (0..37799),
        ephemFitFlag    INTEGER (0..1),
        ephemAODA        INTEGER (0..31),
        ephemCic        INTEGER (-32768..32767),
        ephemOmegaA0    INTEGER (-2147483648..2147483647),
        ephemCis        INTEGER (-32768..32767),
        ephemI0            INTEGER (-2147483648..2147483647),
        ephemCrc        INTEGER (-32768..32767),
        ephemW            INTEGER (-2147483648..2147483647),
        ephemOmegaADot    INTEGER (-8388608..8388607),
        ephemIDot        INTEGER (-8192..8191)
    }
    -- Reserved bits in subframe 1 of navigation message
    EphemerisSubframe1Reserved

EphemerisSubframe1Reserved

    EphemerisSubframe1Reserved ::= SEQUENCE {
        reserved1        INTEGER (0..8388607),    -- 23-bit field
        reserved2        INTEGER (0..16777215),    -- 24-bit field
        reserved3        INTEGER (0..16777215),    -- 24-bit field
        reserved4        INTEGER (0..65535)        -- 16-bit field
    }
    -- Ionospheric Model IE
    IonosphericModel

IonosphericModel

    IonosphericModel ::= SEQUENCE {
        alfa0            INTEGER (-128..127),
        alfa1            INTEGER (-128..127),
        alfa2            INTEGER (-128..127),
        alfa3            INTEGER (-128..127),
        beta0            INTEGER (-128..127),
        beta1            INTEGER (-128..127),
        beta2            INTEGER (-128..127),
        beta3            INTEGER (-128..127)
    }
    -- Universal Time Coordinate Model
    UTCModel

UTCModel

    UTCModel ::= SEQUENCE {
        utcA1            INTEGER (-8388608..8388607),
        utcA0            INTEGER (-2147483648..2147483647),
        utcTot            INTEGER (0..255),
        utcWNt            INTEGER (0..255),
        utcDeltaTls        INTEGER (-128..127),
        utcWNlsf        INTEGER (0..255),
        utcDN            INTEGER (-128..127),
        utcDeltaTlsf    INTEGER (-128..127)
    }
    -- Almanac, Long term model
    -- NOTE: These are parameters are subset of the ephemeris
    -- NOTE: But with reduced resolution and accuracy
    Almanac

Almanac

    Almanac ::= SEQUENCE {
        alamanacWNa        INTEGER (0..255),    -- Once per message
        -- navigation model satellite list.
        -- The size of almanacList is actually Nums_Sats_Total field
        almanacList        SeqOfAlmanacElement
    }
    SeqOfAlmanacElement

AlmanacElement

    AlmanacElement ::= SEQUENCE {
        satelliteID            SatelliteID,
        almanacE            INTEGER (0..65535),
        alamanacToa            INTEGER (0..255),
        almanacKsii            INTEGER (-32768..32767),
        almanacOmegaDot        INTEGER (-32768..32767),
        almanacSVhealth        INTEGER (0..255),
        almanacAPowerHalf    INTEGER (0..16777215),
        almanacOmega0        INTEGER (-8388608..8388607),
        almanacW            INTEGER (-8388608..8388607),
        almanacM0            INTEGER (-8388608..8388607),
        almanacAF0            INTEGER (-1024..1023),
        almanacAF1            INTEGER (-1024..1023)
    }
    -- Acquisition Assistance
    AcquisAssist

AcquisAssist

    AcquisAssist ::= SEQUENCE {
        -- Number of Satellites can be read from acquistList
        timeRelation    TimeRelation,
        -- Acquisition assistance list
        -- The size of Number of Satellites is actually Number of Satellites field
        acquisList        SeqOfAcquisElement
    }
    SeqOfAcquisElement

TimeRelation

    TimeRelation ::= SEQUENCE {
        --
        gpsTOW        GPSTOW23b,        -- 23b presentation
        gsmTime        GSMTime        OPTIONAL
    }
    -- data occuring per number of satellites
    AcquisElement

AcquisElement

    AcquisElement ::= SEQUENCE {
        svid                    SatelliteID,
        -- Doppler 0th order term,
        -- -5120,0 - 5117,5 Hz (= -2048 - 2047 with 2,5 Hz resolution)
        doppler0                INTEGER (-2048..2047),
        addionalDoppler            AddionalDopplerFields    OPTIONAL,
        codePhase                INTEGER (0..1022),    -- Code Phase
        intCodePhase            INTEGER (0..19),    -- Integer Code Phase
        gpsBitNumber            INTEGER (0..3),     -- GPS bit number
        codePhaseSearchWindow    INTEGER (0..15),    -- Code Phase Search Window
        addionalAngle            AddionalAngleFields        OPTIONAL
    }
    AddionalDopplerFields

AddionalDopplerFields

    AddionalDopplerFields ::= SEQUENCE {
        -- Doppler 1st order term, -1,0 - +0,5 Hz/sec
     -- (= -42 + (0 to 63) with 1/42 Hz/sec. resolution)
        doppler1                INTEGER (0..63),
        dopplerUncertainty        INTEGER (0..7)
     -- a sender shall not encode any DopplerUncertainty value in the range 5 to 7
     -- a receiver shall ignore any value between 5 and 7.
    }
    AddionalAngleFields

AddionalAngleFields

    AddionalAngleFields    ::= SEQUENCE {
        -- azimuth angle, 0 - 348,75 deg (= 0 - 31 with 11,25 deg resolution)
        azimuth                    INTEGER (0..31),
        -- elevation angle, 0 - 78,75 deg (= 0 - 7 with 11,25 deg resolution)
        elevation                INTEGER (0..7)
    }
    -- Real-Time Integrity
    -- number of bad satellites can be read from this element
    SeqOf-BadSatelliteSet

Rel98_MsrPosition_Req_Extension

    Rel98-MsrPosition-Req-Extension ::= SEQUENCE {
        rel98-Ext-ExpOTD            Rel98-Ext-ExpOTD        OPTIONAL,    -- ExpectedOTD extension
        ...,
     gpsTimeAssistanceMeasurementRequest NULL OPTIONAL,
     gpsReferenceTimeUncertainty GPSReferenceTimeUncertainty OPTIONAL
    -- Further R98 extensions here
    }
    Rel98-AssistanceData-Extension

Rel98_AssistanceData_Extension

    Rel98-AssistanceData-Extension ::= SEQUENCE {
        rel98-Ext-ExpOTD            Rel98-Ext-ExpOTD        OPTIONAL,    -- ExpectedOTD extension
        ...,
     gpsTimeAssistanceMeasurementRequest NULL OPTIONAL,
     gpsReferenceTimeUncertainty GPSReferenceTimeUncertainty OPTIONAL
    -- Further R98 extensions here
    }
    -- Release 98 ExpOTD extension
    Rel98-Ext-ExpOTD

Rel98_Ext_ExpOTD

    Rel98-Ext-ExpOTD ::= SEQUENCE {
    -- If MsrAssistBTS is included in message, msrAssistData-R98-ExpOTD shall be included.
        msrAssistData-R98-ExpOTD            MsrAssistData-R98-ExpOTD            OPTIONAL,
    -- If SystemInfoAssistaData is included in message, systemInfoAssistData-R98-ExpOTD shall be
    -- included.
        systemInfoAssistData-R98-ExpOTD    SystemInfoAssistData-R98-ExpOTD    OPTIONAL
    }
    -- MsrAssistData R98 extension
    MsrAssistData-R98-ExpOTD

MsrAssistData_R98_ExpOTD

    MsrAssistData-R98-ExpOTD ::= SEQUENCE {
         msrAssistList-R98-ExpOTD             SeqOfMsrAssistBTS-R98-ExpOTD
    }
    -- Indexes in SeqOfMsrAssistBTS-R98-ExpOTD refer to SeqOfMsrAssistBTS
    -- If the index exceeds the SegOfMsrAssistBTS range or if there is other
    -- inconsistencies between the BTS indices, the MS shall apply protocol
    -- error cause incorrectData
    SeqOfMsrAssistBTS-R98-ExpOTD

MsrAssistBTS_R98_ExpOTD

    MsrAssistBTS-R98-ExpOTD ::= SEQUENCE {
        expectedOTD                ExpectedOTD,
        expOTDUncertainty        ExpOTDUncertainty
    }
    -- SystemInfoAssistData R98 extension
    SystemInfoAssistData-R98-ExpOTD

SystemInfoAssistData_R98_ExpOTD

    SystemInfoAssistData-R98-ExpOTD ::= SEQUENCE {
        systemInfoAssistListR98-ExpOTD     SeqOfSystemInfoAssistBTS-R98-ExpOTD
    }
    -- SeqOfSystemInfoAssistBTS-R98-ExpOTD index refer to SeqOfSystemInfoAssistBTS
    -- If the index exceeds the SegOfSystemInfoAssistBTS range or if there is other
    -- inconsistencies between the BTS indices, the MS shall apply protocol
    -- error cause incorrectData
    SeqOfSystemInfoAssistBTS-R98-ExpOTD

AssistBTSData_R98_ExpOTD

    AssistBTSData-R98-ExpOTD ::= SEQUENCE {
        expectedOTD                ExpectedOTD,
        expOTDuncertainty        ExpOTDUncertainty    -- Uncertainty of expected OTD
    }
    -- Expected OTD value between nbor base station and reference BTS
    -- at MS's current estimated location.
    ExpectedOTD

GPSTimeAssistanceMeasurements

    GPSTimeAssistanceMeasurements ::= SEQUENCE {
     referenceFrameMSB INTEGER (0 .. 63)    OPTIONAL,         -- MSB of frame number
     gpsTowSubms INTEGER (0 .. 9999)         OPTIONAL,         -- in units of 100ns, for MS based AGPS
     deltaTow INTEGER (0 .. 127)             OPTIONAL,         -- for MS assisted AGPS
     gpsReferenceTimeUncertainty GPSReferenceTimeUncertainty OPTIONAL
    }
    Rel-98-MsrPosition-Rsp-Extension

Rel_98_MsrPosition_Rsp_Extension

    Rel-98-MsrPosition-Rsp-Extension ::= SEQUENCE {
        -- First extension to Release 98
        rel-98-Ext-MeasureInfo    SEQUENCE {
            otd-MeasureInfo-R98-Ext    OTD-MeasureInfo-R98-Ext        OPTIONAL
        },
        ...,
     timeAssistanceMeasurements GPSTimeAssistanceMeasurements OPTIONAL
     -- Further R98 extensions here
    }
    -- This is an addition to OTD-MeasureInfo element defined in original message,
    -- If OTD-MeasureInfo is absent, or if one or more OTD-MsrElementRest are present
    -- OTD-MeasureInfo-R98-Ext shall be absent.
    -- OTD-MeasureInfo-R98-Ext
    OTD-MeasureInfo-R98-Ext

_0Rel_98_MsrPosition_Rsp_Extension

    SEQUENCE {
    otd-MeasureInfo-R98-Ext    OTD-MeasureInfo-R98-Ext        OPTIONAL
    }

OTD_MeasureInfo_R98_Ext

    OTD-MeasureInfo-R98-Ext ::= SEQUENCE {
        -- Measurement info elements
        otdMsrFirstSets-R98-Ext        OTD-MsrElementFirst-R98-Ext
    }
    -- OTD measurement information Ext for the first set only
    OTD-MsrElementFirst-R98-Ext

OTD_MsrElementFirst_R98_Ext

    OTD-MsrElementFirst-R98-Ext ::= SEQUENCE {
        -- additional measured neighbors in OTD measurements
        otd-FirstSetMsrs-R98-Ext     SeqOfOTD-FirstSetMsrs-R98-Ext     OPTIONAL
    }
    SeqOfOTD-FirstSetMsrs-R98-Ext

Rel_5_MsrPosition_Rsp_Extension

    Rel-5-MsrPosition-Rsp-Extension ::= SEQUENCE {
        extended-reference    Extended-reference     OPTIONAL,
        -- The extended-reference shall be included by the MS if and only if previously
        -- received from the SMLC in a Measure Position Request. When included, the value sent
        -- by the MS shall equal the value received from the SMLC.
        -- extension to Release 5, for RRLP pseudo-segmentation here
        otd-MeasureInfo-5-Ext    OTD-MeasureInfo-5-Ext    OPTIONAL,
        ulPseudoSegInd            UlPseudoSegInd            OPTIONAL,    -- Included when uplink RRLP
        -- Pseudo-segmentation is used, not included when no uplink pseudo-segmentation is used
        ...
                        -- Possibly more extensions for Release 5 here later
    }
    Extended-reference

Extended_reference

    Extended-reference ::= SEQUENCE {
        smlc-code            INTEGER (0..63),
        transaction-ID        INTEGER (0..262143)
    }
    OTD-MeasureInfo-5-Ext

Rel5_MsrPosition_Req_Extension

    Rel5-MsrPosition-Req-Extension ::= SEQUENCE {
        extended-reference            Extended-reference,
        ...
        -- Possibly more extensions for Release 5 here later
    }
    Rel5-AssistanceData-Extension

Rel5_AssistanceData_Extension

    Rel5-AssistanceData-Extension ::= SEQUENCE {
        extended-reference            Extended-reference,
        ...
    -- Possibly more extensions for Release 5 here later
    }
    Rel-5-ProtocolError-Extension

Rel_5_ProtocolError_Extension

    Rel-5-ProtocolError-Extension::= SEQUENCE {
        extended-reference            Extended-reference     OPTIONAL,
        -- The extended-reference shall be included by the MS if and only if previously
        -- received from the SMLC.
        -- When included, the value sent by the MS shall equal the value received from the SMLC.
        ...
        -- Possibly more extensions for Release 5 here later
    }
    -- Release 7 Extensions here
    Rel7-MsrPosition-Req-Extension

Rel7_MsrPosition_Req_Extension

    Rel7-MsrPosition-Req-Extension ::= SEQUENCE {
        velocityRequested                                NULL                    OPTIONAL,
        ganssPositionMethod                                GANSSPositioningMethod    OPTIONAL,
        ganss-AssistData                                GANSS-AssistData        OPTIONAL,
        ganssCarrierPhaseMeasurementRequest                NULL                    OPTIONAL,
        ganssTODGSMTimeAssociationMeasurementRequest    NULL                    OPTIONAL,
        requiredResponseTime                            RequiredResponseTime    OPTIONAL,
        add-GPS-AssistData                                Add-GPS-AssistData        OPTIONAL,
        ganssMultiFreqMeasurementRequest                NULL                    OPTIONAL,
        ...
        -- Further Release 7 extentions here
    }
    -- additional satellite systems may be added in future versions of the protocol
    -- Bit 0 of GANSSPositioningMethod bit map shall not be the only one set to TRUE (‘1’)
    GANSSPositioningMethod

GANSS_AssistData

    GANSS-AssistData ::= SEQUENCE {
        ganss-controlHeader    GANSS-ControlHeader
    }
    GANSS-ControlHeader

GANSS_ControlHeader

    GANSS-ControlHeader ::= SEQUENCE {
     ganssCommonAssistData             GANSSCommonAssistData                 OPTIONAL,
     ganssGenericAssistDataList     SeqOfGANSSGenericAssistDataElement     OPTIONAL
    }
    -- GANSS Common Assistance Data Elements
    GANSSCommonAssistData

GANSSCommonAssistData

    GANSSCommonAssistData ::= SEQUENCE {
        ganssReferenceTime             GANSSReferenceTime             OPTIONAL,
        ganssRefLocation            GANSSRefLocation             OPTIONAL,
        ganssIonosphericModel        GANSSIonosphericModel         OPTIONAL,
        ... ,
        ganssAddIonosphericModel    GANSSAddIonosphericModel    OPTIONAL,
        ganssEarthOrientParam        GANSSEarthOrientParam        OPTIONAL,
        -- If GANSSReferenceTime is included, GANSSReferenceTime-R10-Ext shall also be included.
        ganssReferenceTime-R10-Ext    GANSSReferenceTime-R10-Ext    OPTIONAL
    }
    -- List of GANSS Generic Assistance Data Elements, up to 8 GANSS
    SeqOfGANSSGenericAssistDataElement

GANSSGenericAssistDataElement

    GANSSGenericAssistDataElement ::= SEQUENCE {
        ganssID     INTEGER (0..7)    OPTIONAL, -- Coding according to Annex
        ganssTimeModel    SeqOfGANSSTimeModel    OPTIONAL,
        ganssDiffCorrections    GANSSDiffCorrections    OPTIONAL,
        ganssNavigationModel    GANSSNavModel    OPTIONAL,
        ganssRealTimeIntegrity    GANSSRealTimeIntegrity    OPTIONAL,
        ganssDataBitAssist    GANSSDataBitAssist    OPTIONAL,
        ganssRefMeasurementAssist    GANSSRefMeasurementAssist     OPTIONAL,
        ganssAlmanacModel    GANSSAlmanacModel    OPTIONAL,
        ganssUTCModel    GANSSUTCModel    OPTIONAL,
        ganssEphemerisExtension    GANSSEphemerisExtension    OPTIONAL,
        ganssEphemerisExtCheck    GANSSEphemerisExtensionCheck    OPTIONAL,
        ... ,
        sbasID    INTEGER (0..7)     OPTIONAL, -- Coding according to Annex
        ganssAddUTCModel    GANSSAddUTCModel    OPTIONAL,
        ganssAuxiliaryInfo    GANSSAuxiliaryInformation    OPTIONAL,
        ganssDiffCorrectionsValidityPeriod    GANSSDiffCorrectionsValidityPeriod    OPTIONAL,
        -- If SeqOfGANSSTimeModel is included, SeqOfGANSSTimeModel-R10-Ext shall also be included.
        ganssTimeModel-R10-Ext    SeqOfGANSSTimeModel-R10-Ext    OPTIONAL,
        -- If GANSSRefMeasurementAssist is included, GANSSRefMeasurementAssist-R10-Ext shall also be
        -- included.
        ganssRefMeasurementAssist-R10-Ext    GANSSRefMeasurementAssist-R10-Ext    OPTIONAL,
        -- If GANSSAlmanacModel is included, GANSSAlmanacModel-R10-Ext shall also be included.
        ganssAlmanacModel-R10-Ext    GANSSAlmanacModel-R10-Ext     OPTIONAL
    }
    -- GANSS COMMON ASSISTANCE DATA ELEMENTS
    -- GANSS Reference Time IE
    GANSSReferenceTime

GANSSReferenceTime

    GANSSReferenceTime ::= SEQUENCE {
        ganssRefTimeInfo                GANSSRefTimeInfo,
        ganssTOD-GSMTimeAssociation     GANSSTOD-GSMTimeAssociation OPTIONAL
    }
    -- GANSS Reference Time includes GANSS TOD, GANSS Day, uncertainty
    GANSSRefTimeInfo

GANSSRefTimeInfo

    GANSSRefTimeInfo ::= SEQUENCE {
        -- ganssDay shall be present in this version of the protocol
        ganssDay             INTEGER(0 .. 8191)      OPTIONAL,
         ganssTOD             GANSSTOD,
        ganssTODUncertainty     GANSSTODUncertainty     OPTIONAL,
         ganssTimeID          INTEGER (0 .. 7)          OPTIONAL
    }
    -- GANSS TOD integer seconds
    GANSSTOD

GANSSReferenceTime_R10_Ext

    GANSSReferenceTime-R10-Ext ::= SEQUENCE {
        ganssDayCycleNumber        INTEGER(0..7)     -- coding according to annex
    }
    -- GANSS TOD-GSM Time association
    GANSSTOD-GSMTimeAssociation

GANSSTOD_GSMTimeAssociation

    GANSSTOD-GSMTimeAssociation ::= SEQUENCE {
        bcchCarrier        BCCHCarrier,    -- BCCH carrier
        bsic            BSIC,            -- BSIC
        frameNumber        FrameNumber,
        timeSlot        TimeSlot,
        bitNumber        BitNumber,
         frameDrift         FrameDrift             OPTIONAL
    }
    -- Frame drift
    FrameDrift

GANSSRefLocation

    GANSSRefLocation ::= SEQUENCE {
        threeDLocation            Ext-GeographicalInformation
    }
    -- GANSS Ionospheric Model IE
    -- GANSS Ionospheric Model consists of NeQuick model parameters and storm flags
    GANSSIonosphericModel

GANSSIonosphericModel

    GANSSIonosphericModel ::= SEQUENCE {
         ganssIonoModel             GANSSIonosphereModel,
         ganssIonoStormFlags     GANSSIonoStormFlags             OPTIONAL,
         ...
    }
    -- GANSS ionosphere model. Coding according to Annex
    GANSSIonosphereModel

GANSSIonosphereModel

    GANSSIonosphereModel ::= SEQUENCE {
         ai0 INTEGER (0 .. 4095),
         ai1 INTEGER (0 .. 4095),
         ai2 INTEGER (0 .. 4095)
    }
    -- GANSS ionosphere storm flags
    GANSSIonoStormFlags

GANSSIonoStormFlags

    GANSSIonoStormFlags ::= SEQUENCE {
        ionoStormFlag1    INTEGER (0 .. 1),
        ionoStormFlag2    INTEGER (0 .. 1),
        ionoStormFlag3    INTEGER (0 .. 1),
        ionoStormFlag4    INTEGER (0 .. 1),
        ionoStormFlag5    INTEGER (0 .. 1)
    }
    -- GANSS Additional Ionospheric Model IE
    -- GANSS Additional Ionospheric Model consists of Klobuchar model parameters
    GANSSAddIonosphericModel

GANSSAddIonosphericModel

    GANSSAddIonosphericModel ::= SEQUENCE {
        dataID        BIT STRING (SIZE (2)),      -- Coding according to Annex
        ionoModel    IonosphericModel
    }
    -- GANSS Earth Orientation Paramaters IE
    GANSSEarthOrientParam

GANSSEarthOrientParam

    GANSSEarthOrientParam ::= SEQUENCE {
        teop                INTEGER (0..65535),
        pmX                    INTEGER (-1048576..1048575),
        pmXdot                INTEGER (-16384..16383),
        pmY                    INTEGER (-1048576..1048575),
        pmYdot                INTEGER (-16384..16383),
        deltaUT1            INTEGER (-1073741824..1073741823),
        deltaUT1dot            INTEGER (-262144..262143)
    }
    -- GANSS GENERIC ASSISTANCE DATA ELEMENTS
    -- GANSS Time Model IE consists of time offset and first and second order parameters to relate GNSS
    -- specific system time to selected time reference
    SeqOfGANSSTimeModel

GANSSTimeModelElement

    GANSSTimeModelElement ::= SEQUENCE {
        ganssTimeModelRefTime        INTEGER(0 .. 65535),
        tA0                             TA0,
        tA1                             TA1                     OPTIONAL,
        tA2                             TA2                     OPTIONAL,
         gnssTOID                     INTEGER (0 .. 7),         -- coding according to annex
         weekNumber                     INTEGER (0 .. 8191)     OPTIONAL
    }
    -- GANSS time model parameter A0
    TA0

GANSSTimeModelElement_R10_Ext

    GANSSTimeModelElement-R10-Ext ::= SEQUENCE {
        gnssTOID         INTEGER (0 .. 7),         -- coding according to annex
         deltaT             INTEGER (-128..127)
    }
    -- DGANSS Corrections IE
    GANSSDiffCorrections

GANSSDiffCorrections

    GANSSDiffCorrections ::= SEQUENCE {
        dganssRefTime        INTEGER (0 .. 119),     -- DGANSS reference time
        -- N_SGN_TYPE can be read from number of elements of sgnTypeList
        sgnTypeList         SeqOfSgnTypeElement
    }
    SeqOfSgnTypeElement

SgnTypeElement

    SgnTypeElement ::= SEQUENCE {
        ganssSignalID         GANSSSignalID, -- signal type identity
         ganssStatusHealth     INTEGER (0 .. 7),
        -- N_SAT can be read from number of elements of dganssSgnList
         dganssSgnList         SeqOfDGANSSSgnElement
    }
    GANSSSignalID

DGANSSSgnElement

    DGANSSSgnElement ::= SEQUENCE {
        svID             SVID, -- Satellite identity
    --- Sequence number for GANSS Navigation Model that matches the DGANSS correction set
        iod             INTEGER (0 .. 1023),
        -- User Differential Range Error
        udre            INTEGER (0..3),
        -- Pseudo Range Correction, range is
        -- -655,04 - +655,04,
        pseudoRangeCor    INTEGER (-2047..2047),
        -- Pseudo Range Rate Correction, range is
        -- -4,064 - +4,064,
        rangeRateCor    INTEGER (-127..127)
    }
    SVID

GANSSNavModel

    GANSSNavModel ::= SEQUENCE {
         nonBroadcastIndFlag     INTEGER (0 .. 1),
        ganssSatelliteList         SeqOfGANSSSatelliteElement
    }
    SeqOfGANSSSatelliteElement

GANSSSatelliteElement

    GANSSSatelliteElement ::= SEQUENCE {
     svID                 SVID,
     svHealth             BIT STRING (SIZE(5)),     -- Coding according to Annex
     iod                 INTEGER (0 .. 1023),     -- Coding according to Annex
     ganssClockModel     GANSSClockModel,
     ganssOrbitModel     GANSSOrbitModel,
     ...,
     svHealthMSB        BIT STRING (SIZE(1))     OPTIONAL, -- Coding according to Annex
     iodMSB                INTEGER (0 .. 1)         OPTIONAL  -- Coding according to Annex
    }
    -- GANSS orbit model for the GNSS satellite according to the choice
    GANSSOrbitModel

NavModel_KeplerianSet

    NavModel-KeplerianSet ::= SEQUENCE {
        keplerToe          INTEGER (0 .. 16383),
        keplerW             INTEGER (-2147483648..2147483647),
        keplerDeltaN     INTEGER (-32768..32767),
        keplerM0         INTEGER (-2147483648..2147483647),
        keplerOmegaDot     INTEGER (-8388608..8388607),
        keplerE           INTEGER (0..4294967295),
        keplerIDot         INTEGER (-8192..8191),
        keplerAPowerHalf INTEGER (0.. 4294967295),
        keplerI0         INTEGER (-2147483648..2147483647),
        keplerOmega0      INTEGER (-2147483648..2147483647),
        keplerCrs         INTEGER (-32768..32767),
        keplerCis         INTEGER (-32768..32767),
        keplerCus         INTEGER (-32768..32767),
        keplerCrc         INTEGER (-32768..32767),
        keplerCic         INTEGER (-32768..32767),
        keplerCuc         INTEGER (-32768..32767)
    }
    NavModel-NAVKeplerianSet

NavModel_NAVKeplerianSet

    NavModel-NAVKeplerianSet ::= SEQUENCE {
        navURA            INTEGER (0..15),
        navFitFlag        INTEGER (0..1),
        navToe            INTEGER (0..37799),
        navOmega        INTEGER (-2147483648..2147483647),
        navDeltaN        INTEGER (-32768..32767),
        navM0            INTEGER (-2147483648..2147483647),
        navOmegaADot    INTEGER (-8388608..8388607),
        navE            INTEGER (0..4294967295),
        navIDot            INTEGER (-8192..8191),
        navAPowerHalf    INTEGER (0..4294967295),
        navI0            INTEGER (-2147483648..2147483647),
        navOmegaA0        INTEGER (-2147483648..2147483647),
        navCrs            INTEGER (-32768..32767),
        navCis            INTEGER (-32768..32767),
        navCus            INTEGER (-32768..32767),
        navCrc            INTEGER (-32768..32767),
        navCic            INTEGER (-32768..32767),
        navCuc            INTEGER (-32768..32767)
    }
    NavModel-CNAVKeplerianSet

NavModel_CNAVKeplerianSet

    NavModel-CNAVKeplerianSet ::= SEQUENCE {
        cnavTop                INTEGER (0..2015),
        cnavURAindex        INTEGER (-16..15),
        cnavDeltaA            INTEGER (-33554432..33554431),
        cnavAdot            INTEGER (-16777216..16777215),
        cnavDeltaNo            INTEGER (-65536..65535),
        cnavDeltaNoDot        INTEGER (-4194304..4194303),
        cnavMo                INTEGER (-4294967296..4294967295),
        cnavE                INTEGER (0..8589934591),
        cnavOmega            INTEGER (-4294967296..4294967295),
        cnavOMEGA0            INTEGER (-4294967296..4294967295),
        cnavDeltaOmegaDot    INTEGER (-65536..65535),
        cnavIo                INTEGER (-4294967296..4294967295),
        cnavIoDot            INTEGER (-16384..16383),
        cnavCis                INTEGER (-32768..32767),
        cnavCic                INTEGER (-32768..32767),
        cnavCrs                INTEGER (-8388608..8388607),
        cnavCrc                INTEGER (-8388608..8388607),
        cnavCus                INTEGER (-1048576..1048575),
        cnavCuc                INTEGER (-1048576..1048575)
    }
    NavModel-GLONASSecef

NavModel_GLONASSecef

    NavModel-GLONASSecef ::= SEQUENCE {
        gloEn                INTEGER (0..31),
        gloP1                BIT STRING (SIZE(2)),
        gloP2                BOOLEAN,
        gloM                INTEGER (0..3),
        gloX                INTEGER (-67108864..67108863),
        gloXdot                INTEGER (-8388608..8388607),
        gloXdotdot            INTEGER (-16..15),
        gloY                INTEGER (-67108864..67108863),
        gloYdot                INTEGER (-8388608..8388607),
        gloYdotdot            INTEGER (-16..15),
        gloZ                INTEGER (-67108864..67108863),
        gloZdot                INTEGER (-8388608..8388607),
        gloZdotdot            INTEGER (-16..15)
    }
    NavModel-SBASecef

NavModel_SBASecef

    NavModel-SBASecef ::= SEQUENCE {
        sbasTo                INTEGER (0..5399)                     OPTIONAL,
        sbasAccuracy        BIT STRING (SIZE(4)),
        sbasXg                INTEGER (-536870912..536870911),
        sbasYg                INTEGER (-536870912..536870911),
        sbasZg                INTEGER (-16777216..16777215),
        sbasXgDot            INTEGER (-65536..65535),
        sbasYgDot            INTEGER (-65536..65535),
        sbasZgDot            INTEGER (-131072..131071),
        sbasXgDotDot        INTEGER (-512..511),
        sbagYgDotDot        INTEGER (-512..511),
        sbasZgDotDot        INTEGER (-512..511)
    }
    -- GANSS clock model for the GNSS satellite according to the choice
    GANSSClockModel

StandardClockModelElement

    StandardClockModelElement ::= SEQUENCE {
         stanClockToc     INTEGER (0 .. 16383),
         stanClockAF2     INTEGER (-2048 .. 2047),
         stanClockAF1     INTEGER (-131072 .. 131071),
         stanClockAF0     INTEGER (-134217728 .. 134217727),
         stanClockTgd     INTEGER (-512 .. 511)                 OPTIONAL,
         stanModelID     INTEGER (0 .. 1)                     OPTIONAL,
         ...
    }
    NAVclockModel

NAVclockModel

    NAVclockModel ::= SEQUENCE {
        navToc            INTEGER (0.. 37799),
        navaf2            INTEGER (-128..127),
        navaf1            INTEGER (-32768..32767),
        navaf0            INTEGER (-2097152..2097151),
        navTgd            INTEGER (-128..127)
    }
    CNAVclockModel

CNAVclockModel

    CNAVclockModel ::= SEQUENCE {
        cnavToc            INTEGER (0..2015),
        cnavTop            INTEGER (0..2015),
        cnavURA0        INTEGER (-16..15),
        cnavURA1        INTEGER (0..7),
        cnavURA2        INTEGER (0..7),
        cnavAf2            INTEGER (-512..511),
        cnavAf1            INTEGER (-524288..524287),
        cnavAf0            INTEGER (-33554432..33554431),
        cnavTgd            INTEGER (-4096..4095),
        cnavISCl1cp        INTEGER (-4096..4095)             OPTIONAL,
        cnavISCl1cd        INTEGER (-4096..4095)             OPTIONAL,
        cnavISCl1ca        INTEGER (-4096..4095)             OPTIONAL,
        cnavISCl2c        INTEGER (-4096..4095)             OPTIONAL,
        cnavISCl5i5        INTEGER (-4096..4095)             OPTIONAL,
        cnavISCl5q5        INTEGER (-4096..4095)             OPTIONAL
    }
    GLONASSclockModel

GLONASSclockModel

    GLONASSclockModel ::= SEQUENCE {
        gloTau            INTEGER (-2097152..2097151),
        gloGamma        INTEGER (-1024..1023),
        gloDeltaTau        INTEGER (-16..15)                 OPTIONAL
    }
    SBASclockModel

SBASclockModel

    SBASclockModel ::= SEQUENCE {
        sbasTo            INTEGER (0..5399),
        sbasAgfo        INTEGER (-2048..2047),
        sbasAgf1        INTEGER (-128..127)
    }
    -- GANSS Real-Time Integrity IE
    GANSSRealTimeIntegrity

GANSSRealTimeIntegrity

    GANSSRealTimeIntegrity ::= SEQUENCE {
     -- list of satellites with bad signals
     -- NBS can be read from number of elements in SeqOf-BadSignalSet
         ganssBadSignalList         SeqOfBadSignalElement
    }
    SeqOfBadSignalElement

BadSignalElement

    BadSignalElement ::= SEQUENCE {
         badSVID         SVID,                          -- Coding according to Annex
         badSignalID     GANSSSignals     OPTIONAL     -- Coding according to Annex
    }
    -- GANSS Data Bit Assistance IE
    GANSSDataBitAssist

GANSSDataBitAssist

    GANSSDataBitAssist ::= SEQUENCE {
        ganssTOD                     INTEGER (0 .. 59),
        -- N_SAT can be read from number of elements in SeqOfGanssDataBitsElement
        ganssDataBitsSatList        SeqOfGanssDataBitsElement,
        ...
    }
    SeqOfGanssDataBitsElement

GanssDataBitsElement

    GanssDataBitsElement ::= SEQUENCE {
        svID                    SVID,
        -- N_SGN can be read from number of elements in Seq-OfGANSSDataBitsSgn
        ganssDataBitsSgnList    Seq-OfGANSSDataBitsSgn,
        ...
    }
    Seq-OfGANSSDataBitsSgn

GANSSDataBitsSgnElement

    GANSSDataBitsSgnElement ::= SEQUENCE {
        ganssSignalType        GANSSSignalID,
        -- N_BIT can be read from number of elements in SeqOf-DataBits
        ganssDataBits        SeqOf-GANSSDataBits,
        ...
    }
    SeqOf-GANSSDataBits

GANSSRefMeasurementAssist

    GANSSRefMeasurementAssist ::= SEQUENCE {
        ganssSignalID            GANSSSignalID,    -- Coding according to Annex
        ganssRefMeasAssistList    SeqOfGANSSRefMeasurementElement
    }
    SeqOfGANSSRefMeasurementElement

GANSSRefMeasurementElement

    GANSSRefMeasurementElement ::= SEQUENCE {
        svID                    SVID,
        -- Doppler 0th order term,
        -- -1024 m/s to 1023,5 m/s with 0,5 m/s resolution)
        doppler0                INTEGER (-2048 .. 2047),                    -- Coding according to Annex
        additionalDoppler        AdditionalDopplerFields            OPTIONAL,
        codePhase                INTEGER (0 .. 1022),                        -- Code Phase in ms
        intCodePhase            INTEGER (0 .. 127),                            -- Integer Code Phase in ms
        codePhaseSearchWindow    INTEGER (0 .. 31),                -- Code Phase Search Window, see Annex
        additionalAngle            AddionalAngleFields                 OPTIONAL,
        ...
    }
    AdditionalDopplerFields

AdditionalDopplerFields

    AdditionalDopplerFields ::= SEQUENCE {
        -- Doppler 1st order term, -0,2 - +0,1 m/s2
        -- ( = -42 + (0 to 63) with 1/210 m/s2 resolution)
        doppler1                INTEGER (0..63),
        dopplerUncertainty        INTEGER (0..4)
    }
    -- GANSS Reference Measurement Rel-10 Extension:
    -- GANSSRefMeasurementAssist-R10-Ext shall contain the same number of elements as the
    -- SeqOfGANSSRefMeasurementElement included in GANSSRefMeasurementAssist IE
    GANSSRefMeasurementAssist-R10-Ext

GANSSRefMeasurement_R10_Ext_Element

    GANSSRefMeasurement-R10-Ext-Element ::= SEQUENCE {
        svID                SVID,
        azimuthLSB            INTEGER(0..15),
        elevationLSB        INTEGER(0..15)
    }
    -- GANSS Almanac Model IE
    GANSSAlmanacModel

GANSSAlmanacModel

    GANSSAlmanacModel ::= SEQUENCE {
         weekNumber             INTEGER (0 .. 255),
        toa                 INTEGER (0 .. 255)     OPTIONAL,
        ioda                 INTEGER (0 .. 3)     OPTIONAL,
        ganssAlmanacList     SeqOfGANSSAlmanacElement
    }
    SeqOfGANSSAlmanacElement

Almanac_KeplerianSet

    Almanac-KeplerianSet ::= SEQUENCE {
        svID                    SVID,
         kepAlmanacE                 INTEGER (0 .. 2047),
        kepAlmanacDeltaI        INTEGER (-1024 .. 1023),
        kepAlmanacOmegaDot        INTEGER (-1024 .. 1023),
         kepSVHealth             INTEGER (0 .. 15),              -- Coding according to Annex
        kepAlmanacAPowerHalf    INTEGER (-65536 .. 65535),
        kepAlmanacOmega0        INTEGER (-32768 .. 32767),
        kepAlmanacW                 INTEGER (-32768 .. 32767),
        kepAlmanacM0            INTEGER (-32768 .. 32767),
        kepAlmanacAF0            INTEGER (-8192 .. 8191),
        kepAlmanacAF1            INTEGER (-1024..1023)
    }
    Almanac-NAVKeplerianSet

Almanac_NAVKeplerianSet

    Almanac-NAVKeplerianSet ::= SEQUENCE {
        svID                    SVID,
        navAlmE                    INTEGER (0..65535),
        navAlmDeltaI            INTEGER (-32768..32767),
        navAlmOMEGADOT            INTEGER (-32768..32767),
        navAlmSVHealth            INTEGER (0..255),
        navAlmSqrtA                INTEGER (0..16777215),
        navAlmOMEGAo            INTEGER (-8388608..8388607),
        navAlmOmega                INTEGER (-8388608..8388607),
        navAlmMo                INTEGER (-8388608..8388607),
        navAlmaf0                INTEGER (-1024..1023),
        navAlmaf1                INTEGER (-1024..1023)
    }
    Almanac-ReducedKeplerianSet

Almanac_ReducedKeplerianSet

    Almanac-ReducedKeplerianSet ::= SEQUENCE {
        svID                    SVID,
        redAlmDeltaA            INTEGER (-128..127),
        redAlmOmega0            INTEGER (-64..63),
        redAlmPhi0                INTEGER (-64..63),
        redAlmL1Health            BOOLEAN,
        redAlmL2Health            BOOLEAN,
        redAlmL5Health            BOOLEAN
    }
    Almanac-MidiAlmanacSet

Almanac_MidiAlmanacSet

    Almanac-MidiAlmanacSet ::= SEQUENCE {
        svID                    SVID,
        midiAlmE                INTEGER (0..2047),
        midiAlmDeltaI            INTEGER (-1024..1023),
        midiAlmOmegaDot            INTEGER (-1024..1023),
        midiAlmSqrtA            INTEGER (0..131071),
        midiAlmOmega0            INTEGER (-32768..32767),
        midiAlmOmega            INTEGER (-32768..32767),
        midiAlmMo                INTEGER (-32768..32767),
        midiAlmaf0                INTEGER (-1024..1023),
        midiAlmaf1                INTEGER (-512..511),
        midiAlmL1Health            BOOLEAN,
        midiAlmL2Health            BOOLEAN,
        midiAlmL5Health            BOOLEAN
    }
    Almanac-GlonassAlmanacSet

Almanac_GlonassAlmanacSet

    Almanac-GlonassAlmanacSet ::= SEQUENCE {
        gloAlmNA                INTEGER (1..1461),
        gloAlmnA                INTEGER (1..24),
        gloAlmHA                INTEGER (0..31),
        gloAlmLambdaA            INTEGER (-1048576..1048575),
        gloAlmtlambdaA            INTEGER (0..2097151),
        gloAlmDeltaIa            INTEGER (-131072..131071),
        gloAlmDeltaTA            INTEGER (-2097152..2097151),
        gloAlmDeltaTdotA        INTEGER (-64..63),
        gloAlmEpsilonA            INTEGER (0..32767),
        gloAlmOmegaA            INTEGER (-32768..32767),
        gloAlmTauA                INTEGER (-512..511),
        gloAlmCA                INTEGER (0..1),
        gloAlmMA                BIT STRING (SIZE(2))             OPTIONAL
    }
    Almanac-ECEFsbasAlmanacSet

Almanac_ECEFsbasAlmanacSet

    Almanac-ECEFsbasAlmanacSet ::= SEQUENCE {
        sbasAlmDataID            INTEGER (0..3),
        svID                    SVID,
        sbasAlmHealth            BIT STRING (SIZE(8)),
        sbasAlmXg                INTEGER (-16384..16383),
        sbasAlmYg                INTEGER (-16384..16383),
        sbasAlmZg                INTEGER (-256..255),
        sbasAlmXgdot            INTEGER (-4..3),
        sbasAlmYgDot            INTEGER (-4..3),
        sbasAlmZgDot            INTEGER (-8..7),
        sbasAlmTo                INTEGER (0..2047)
    }
    -- GANSS Almanac Model Rel-10 Extension
    GANSSAlmanacModel-R10-Ext

GANSSAlmanacModel_R10_Ext

    GANSSAlmanacModel-R10-Ext ::= SEQUENCE {
        completeAlmanacProvided        BOOLEAN    -- TRUE means that complete Almanac is provided
    }
    -- GANSS Universal Time Coordinate Model (Model-1)
    GANSSUTCModel

GANSSUTCModel

    GANSSUTCModel ::= SEQUENCE {
        ganssUtcA1            INTEGER (-8388608..8388607),
        ganssUtcA0            INTEGER (-2147483648..2147483647),
        ganssUtcTot            INTEGER (0..255),
        ganssUtcWNt            INTEGER (0..255),
        ganssUtcDeltaTls    INTEGER (-128..127),
        ganssUtcWNlsf        INTEGER (0..255),
        ganssUtcDN            INTEGER (-128..127),
        ganssUtcDeltaTlsf    INTEGER (-128..127)
    }
    --GANSS Ephemeris Extension
    GANSSEphemerisExtension

GANSSEphemerisExtension

    GANSSEphemerisExtension ::= SEQUENCE {
        ganssEphemerisHeader            GANSSEphemerisExtensionHeader            OPTIONAL,
        ganssReferenceSet                SeqOfGANSSRefOrbit                        OPTIONAL,
        ganssephemerisDeltasMatrix        GANSSEphemerisDeltaMatrix                OPTIONAL,
    ...
    }
    -- The ganssEphemerisHeader and the ganssReferenceSet are mandatory only once in the delivery of the
    -- GANSS Ephemeris Extension.  The ganssReferenceSet shall include all healthy satellite vehicles
    -- at the time of message construction.
    GANSSEphemerisExtensionHeader

GANSSEphemerisExtensionHeader

    GANSSEphemerisExtensionHeader ::= SEQUENCE {
        timeAtEstimation            GANSSEphemerisExtensionTime,
        validityPeriod                INTEGER(1..8),
    -- The validity period, represented in hours, is the validity period of each individual ephemeris
    -- delta payload
        ephemerisExtensionDuration    INTEGER(1..512),
    -- If the ephemerisExtensionDuration does not match the request duration made by the MS, the MS
    -- should regard the provided ephemerisExtensionDuration as the limit of the SMLC ephemeris
    -- extension capability at this time.
    ...
    }
    GANSSEphemerisExtensionTime

GANSSEphemerisExtensionTime

    GANSSEphemerisExtensionTime ::= SEQUENCE {
        ganssEphExtDay        INTEGER(0..8191),
        ganssEphExtTOD        GANSSTOD,
    ...
    }
    -- Reference Nav Model for Ephepmeris Extension
    ReferenceNavModel

ReferenceNavModel

    ReferenceNavModel ::= SEQUENCE {
         keplerToe            INTEGER (0..37799),
        keplerW                INTEGER (-2147483648..2147483647),
        keplerDeltaN        INTEGER (-32768..32767),
        keplerM0            INTEGER (-2147483648..2147483647),
        keplerOmegaDot        INTEGER (-8388608..8388607),
        keplerE                INTEGER (0..4294967295),
        keplerIDot            INTEGER (-8192..8191),
        keplerAPowerHalf    INTEGER (0.. 4294967295),
        keplerI0            INTEGER (-2147483648..2147483647),
        keplerOmega0        INTEGER (-2147483648..2147483647),
        keplerCrs            INTEGER (-32768..32767),
        keplerCis            INTEGER (-32768..32767),
        keplerCus            INTEGER (-32768..32767),
        keplerCrc            INTEGER (-32768..32767),
        keplerCic            INTEGER (-32768..32767),
        keplerCuc            INTEGER (-32768..32767)
    }
    SeqOfGANSSRefOrbit

GANSSReferenceOrbit

    GANSSReferenceOrbit ::= SEQUENCE {
        svID                SVID,
        ganssOrbitModel        ReferenceNavModel,
        ganssClockModel        GANSSClockModel,
    ...
    }
    GANSSEphemerisDeltaMatrix

GANSSEphemerisDeltaEpoch

    GANSSEphemerisDeltaEpoch ::= SEQUENCE {
        ganssDeltaEpochHeader        GANSSDeltaEpochHeader                OPTIONAL,
        ganssDeltaElementList        GANSSDeltaElementList,
    ...
    }
    -- Each GANSSDeltaEpoch element contains a header and the delta values for a particular time window
    -- for all PRN’s.
    GANSSDeltaEpochHeader

GANSSDeltaEpochHeader

    GANSSDeltaEpochHeader ::= SEQUENCE {
        validityPeriod                INTEGER(1..8)                    OPTIONAL,
        ephemerisDeltaSizes            GANSSEphemerisDeltaBitSizes        OPTIONAL,
        ephemerisDeltaScales        GANSSEphemerisDeltaScales        OPTIONAL,
    ...
    }
    -- In each of the GANSSDeltaEpochs, if the optional element, validityPeriod is not included, the
    -- value in GANSSEphemerisExtensionHeader shall be used.  If the optional elements
    -- ephemerisDeltaSizes or ephemerisDeltaScales are not included, then the default ephemeris delta
    -- sizes and scales shall be used.  The default sizes and scales are found in the annex in the
    -- table 55.11.
    GANSSDeltaElementList

GANSSEphemerisDeltaBitSizes

    GANSSEphemerisDeltaBitSizes ::= SEQUENCE {
    -- This structure defines the order and sizes of the fields in the GANSSDeltaEpoch octet string
    -- seqNum and svID are the first two elements of each GANSS Ephemeris Delta Element Structure
    -- seqNum is always 7 bits, and svID is always 6 bits long and are thus not included in
    -- the GANSSEphemerisDeltaBitSizes table.  The value of seqNum indicates the GANSSDeltaEpoch number
    -- The Ephemeris delta element payload mimics the bitsize table, but also includes the svID and
    -- seqNum as the first two elements (in that order),in each block.
        bitsize-delta-omega            INTEGER(1..32),
        bitsize-delta-deltaN        INTEGER(1..16),
        bitsize-delta-m0            INTEGER(1..32),
        bitsize-delta-omegadot        INTEGER(1..24),
        bitsize-delta-e                INTEGER(1..32),
        bitsize-delta-idot            INTEGER(1..14),
        bitsize-delta-sqrtA            INTEGER(1..32),
        bitsize-delta-i0            INTEGER(1..32),
        bitsize-delta-omega0        INTEGER(1..32),
        bitsize-delta-crs            INTEGER(1..16),
        bitsize-delta-cis            INTEGER(1..16),
        bitsize-delta-cus            INTEGER(1..16),
        bitsize-delta-crc            INTEGER(1..16),
        bitsize-delta-cic            INTEGER(1..16),
        bitsize-delta-cuc            INTEGER(1..16),
        bitsize-delta-tgd1            INTEGER(1..10),
        bitsize-delta-tgd2            INTEGER(1..10),
    ...
    }
    GANSSEphemerisDeltaScales

GANSSEphemerisDeltaScales

    GANSSEphemerisDeltaScales ::= SEQUENCE {
        scale-delta-omega            INTEGER(-16..15),
        scale-delta-deltaN            INTEGER(-16..15),
        scale-delta-m0                INTEGER(-16..15),
        scale-delta-omegadot        INTEGER(-16..15),
        scale-delta-e                INTEGER(-16..15),
        scale-delta-idot            INTEGER(-16..15),
        scale-delta-sqrtA            INTEGER(-16..15),
        scale-delta-i0                INTEGER(-16..15),
        scale-delta-omega0            INTEGER(-16..15),
        scale-delta-crs                INTEGER(-16..15),
        scale-delta-cis                INTEGER(-16..15),
        scale-delta-cus                INTEGER(-16..15),
        scale-delta-crc                INTEGER(-16..15),
        scale-delta-cic                INTEGER(-16..15),
        scale-delta-cuc                INTEGER(-16..15),
        scale-delta-tgd1            INTEGER(-16..15),
        scale-delta-tgd2            INTEGER(-16..15),
    ...
    }
    -- GANSS Ephemeris Extension Check
    GANSSEphemerisExtensionCheck

GANSSEphemerisExtensionCheck

    GANSSEphemerisExtensionCheck ::= SEQUENCE {
        ganssBeginTime            GANSSEphemerisExtensionTime,
        ganssEndTime            GANSSEphemerisExtensionTime,
        ganssSatEventsInfo        GANSSSatEventsInfo,
    ...
    }
    GANSSSatEventsInfo

GANSSSatEventsInfo

    GANSSSatEventsInfo ::= SEQUENCE {
        eventOccured        BIT STRING (SIZE (64)),
        futureEventNoted    BIT STRING (SIZE (64)),
    ...
    }
    -- If a bit is clear in the eventOccured field it indicates that no known errors have occured
    -- between the current time and the ganssBeginTime nor is a maneuver planned for the next sixty
    -- minutes.
    -- If a bit is set in the futureEventNoted field it indicates that a maneuver is planned during the
    -- time period between current time plus sixty minutes and the ganssEndTime
    -- GANSS Additional Universal Time Coordinate Model
    GANSSAddUTCModel

UTCmodelSet2

    UTCmodelSet2 ::= SEQUENCE {
        utcA0                INTEGER (-32768..32767),
        utcA1                INTEGER (-4096.. 4095),
        utcA2                INTEGER (-64..63),
        utcDeltaTls            INTEGER (-128.. 127),
        utcTot                INTEGER (0..65535),
        utcWNot                INTEGER (0..8191),
        utcWNlsf            INTEGER (0..255),
        utcDN                BIT STRING (SIZE(4)),
        utcDeltaTlsf        INTEGER (-128..127)
    }
    UTCmodelSet3

UTCmodelSet3

    UTCmodelSet3 ::= SEQUENCE {
        nA                    INTEGER (1..1461),
        tauC                INTEGER (-2147483648..2147483647),
        b1                    INTEGER (-1024..1023)                     OPTIONAL,
        b2                    INTEGER (-512..511)                     OPTIONAL,
        kp                    BIT STRING (SIZE(2))                     OPTIONAL
    }
    UTCmodelSet4

UTCmodelSet4

    UTCmodelSet4 ::= SEQUENCE {
        utcA1wnt            INTEGER (-8388608..8388607),
        utcA0wnt            INTEGER (-2147483648..2147483647),
        utcTot                INTEGER (0..255),
        utcWNt                INTEGER (0..255),
        utcDeltaTls            INTEGER (-128..127),
        utcWNlsf            INTEGER (0..255),
        utcDN                INTEGER (-128..127),
        utcDeltaTlsf        INTEGER (-128..127),
        utcStandardID        INTEGER (0..7)             -- coding according to annex
    }
    -- GANSS Auxiliary Information
    GANSSAuxiliaryInformation

GANSS_ID1_element

    GANSS-ID1-element ::= SEQUENCE {
        svID                SVID,
        signalsAvailable    GANSSSignals,
        ...
    }
    GANSS-ID3

GANSS_ID3_element

    GANSS-ID3-element  ::= SEQUENCE {
        svID                SVID,
        signalsAvailable    GANSSSignals,
        channelNumber        INTEGER (-7..13),
        ...
    }
    -- DGANSS Corrections Validity Period:
    -- This element may only be included if GANSSDiffCorrections IE is included in
    -- GANSSGenericAssistDataElement element.
    -- GANSSDiffCorrectionsValidityPeriod shall contain the same number of elements as the
    -- SeqOfSgnTypeElement included in GANSSDiffCorrections IE
    GANSSDiffCorrectionsValidityPeriod

DGANSSExtensionSgnTypeElement

    DGANSSExtensionSgnTypeElement ::= SEQUENCE {
        ganssSignalID                 GANSSSignalID, -- signal type identity
        dganssExtensionSgnList        SeqOfDGANSSExtensionSgnElement
    }
    -- SeqOfDGANSSExtensionSgnElement shall contain the same number of elements as the
    -- SeqOfDGANSSSgnElement included in GANSSDiffCorrections IE
    SeqOfDGANSSExtensionSgnElement

DGANSSExtensionSgnElement

    DGANSSExtensionSgnElement ::= SEQUENCE {
        svID                SVID,             -- Satellite identity
        udreGrowthRate        INTEGER(0..7),     -- coding according to annex
        udreValidityTime    INTEGER(0..7),     -- coding according to annex
        ...
    }
    --Required Measurement Request Response Time, range is 1 to 128 seconds.
    RequiredResponseTime

Add_GPS_AssistData

    Add-GPS-AssistData ::= SEQUENCE {
        add-GPS-controlHeader    Add-GPS-ControlHeader
    }
    Add-GPS-ControlHeader

Add_GPS_ControlHeader

    Add-GPS-ControlHeader ::= SEQUENCE {
        gpsEphemerisExtension            GPSEphemerisExtension            OPTIONAL,
        gpsEphemerisExtensionCheck        GPSEphemerisExtensionCheck        OPTIONAL,
        ... ,
        dgpsCorrectionsValidityPeriod    DGPSCorrectionsValidityPeriod    OPTIONAL,
        -- If ReferenceTime is included in ControlHeader, GPSReferenceTime-R10-Ext
        -- shall also be included.
        gpsReferenceTime-R10-Ext        GPSReferenceTime-R10-Ext        OPTIONAL,
        -- If AcquisAssist is included in ControlHeader, GPSAcquisAssist-R10-Ext
        -- shall also be included.
        gpsAcquisAssist-R10-Ext            GPSAcquisAssist-R10-Ext            OPTIONAL,
        -- If Almanac is included in ControlHeader, GPSAlmanac-R10-Ext
        -- shall also be included.
        gpsAlmanac-R10-Ext                GPSAlmanac-R10-Ext                OPTIONAL
    }
    GPSClockModel

GPSClockModel

    GPSClockModel ::= SEQUENCE {
        af2        INTEGER (-128..127),
        af1        INTEGER (-32768..32767),
        af0        INTEGER (-2097152..2097151),
        tgd        INTEGER (-128..127)
    }
    --GPS Ephemeris Extension
    GPSEphemerisExtension

GPSEphemerisExtension

    GPSEphemerisExtension ::= SEQUENCE {
        gpsEphemerisHeader            GPSEphemerisExtensionHeader                OPTIONAL,
        gpsReferenceSet                SeqOfGPSRefOrbit                        OPTIONAL,
        gpsephemerisDeltaMatrix        GPSEphemerisDeltaMatrix                    OPTIONAL,
    ...
    }
    -- The gpsEphemerisHeader and the gpsReferenceSet are mandatory only once in the delivery of the
    -- GPS Ephemeris Extension.  The gpsReferenceSet shall include all healthy satellite vehicles at the
    -- time of message construction
    -- The SMLC is required to deliver the gpsReferenceSet for all healthy satellite vehicles
    -- at the time of message construction.
    GPSEphemerisExtensionHeader

GPSEphemerisExtensionHeader

    GPSEphemerisExtensionHeader ::= SEQUENCE {
        timeofEstimation            GPSEphemerisExtensionTime,
        validityPeriod                INTEGER(1..8),
    -- The validity period, represented in hours is the validity period of each individual ephemeris
    -- delta payload
        ephemerisExtensionDuration    INTEGER(1..512),
    -- If the ephemerisExtensionDuration does not match the request duration made by the MS, the MS
    -- should regard the provided ephemerisExtensionDuration as the limit of the SMLC ephemeris
    -- extension capability at this time.
    ...
    }
    GPSEphemerisExtensionTime

GPSEphemerisExtensionTime

    GPSEphemerisExtensionTime ::= SEQUENCE {
        gpsWeek                GPSWeek,
        gpsTOW                INTEGER (0..604799),
    ...
    }
    SeqOfGPSRefOrbit

GPSReferenceOrbit

    GPSReferenceOrbit ::= SEQUENCE {
        svID                SVID,
        gpsOrbitModel        ReferenceNavModel,
        gpsClockModel        GPSClockModel,
    ...
    }
    GPSEphemerisDeltaMatrix

GPSEphemerisDeltaEpoch

    GPSEphemerisDeltaEpoch ::= SEQUENCE {
        gpsDeltaEpochHeader        GPSDeltaEpochHeader                OPTIONAL,
        gpsDeltaElementList        GPSDeltaElementList,
    ...
    }
    -- Each GPSDeltaEpoch element contains a header and the delta values for a particular time window
    -- for all PRN’s.
    GPSDeltaEpochHeader

GPSDeltaEpochHeader

    GPSDeltaEpochHeader ::= SEQUENCE {
        validityPeriod                INTEGER(1..8)                OPTIONAL,
        ephemerisDeltaSizes            GPSEphemerisDeltaBitSizes    OPTIONAL,
        ephemerisDeltaScales        GPSEphemerisDeltaScales    OPTIONAL,
    ...
    }
    -- In each of the GPSDeltaEpochs, if the optional element validityPeriod is not included,
    -- the value in GPSEphemerisExtensionHeader shall be used.  if the optional elements
    -- ephemerisDeltaSizes or ephemerisDeltaScales are not included, then the default ephemeris delta
    -- sizes and scales shall be used.  The default sizes and scales are found in the annex in section
    -- A.29.m
    GPSDeltaElementList

GPSEphemerisDeltaBitSizes

    GPSEphemerisDeltaBitSizes ::= SEQUENCE {
    -- This structure defines the order and sizes of the fields in the GPSsDeltaEpoch octet string
    -- seqNum and svID are the first two elements of each GPS Ephemeris Delta Element Structure
    -- seqNum is always 7 bits, and svID is always 5 bits long and are thus not included in
    -- the GPSEphemerisDeltaBitSizes table. seqNum indicates the GPSDeltaEpoch number.
    -- The Ephemeris delta element payload mimics the bitsize table, but also includes the svID and
    -- seqNum as the first two elements (in that order),in each block.
        bitsize-delta-omega            INTEGER(1..32),
        bitsize-delta-deltaN        INTEGER(1..16),
        bitsize-delta-m0            INTEGER(1..32),
        bitsize-delta-omegadot        INTEGER(1..24),
        bitsize-delta-e                INTEGER(1..32),
        bitsize-delta-idot            INTEGER(1..14),
        bitsize-delta-sqrtA            INTEGER(1..32),
        bitsize-delta-i0            INTEGER(1..32),
        bitsize-delta-omega0        INTEGER(1..32),
        bitsize-delta-crs            INTEGER(1..16),
        bitsize-delta-cis            INTEGER(1..16),
        bitsize-delta-cus            INTEGER(1..16),
        bitsize-delta-crc            INTEGER(1..16),
        bitsize-delta-cic            INTEGER(1..16),
        bitsize-delta-cuc            INTEGER(1..16),
        bitsize-delta-tgd            INTEGER(1..10),
    ...
    }
    GPSEphemerisDeltaScales

GPSEphemerisDeltaScales

    GPSEphemerisDeltaScales ::= SEQUENCE {
        scale-delta-omega            INTEGER(-16..15),
        scale-delta-deltaN            INTEGER(-16..15),
        scale-delta-m0                INTEGER(-16..15),
        scale-delta-omegadot        INTEGER(-16..15),
        scale-delta-e                INTEGER(-16..15),
        scale-delta-idot            INTEGER(-16..15),
        scale-delta-sqrtA            INTEGER(-16..15),
        scale-delta-i0                INTEGER(-16..15),
        scale-delta-omega0            INTEGER(-16..15),
        scale-delta-crs                INTEGER(-16..15),
        scale-delta-cis                INTEGER(-16..15),
        scale-delta-cus                INTEGER(-16..15),
        scale-delta-crc                INTEGER(-16..15),
        scale-delta-cic                INTEGER(-16..15),
        scale-delta-cuc                INTEGER(-16..15),
        scale-delta-tgd                INTEGER(-16..15),
    ...
    }
    GPSEphemerisExtensionCheck

GPSEphemerisExtensionCheck

    GPSEphemerisExtensionCheck ::= SEQUENCE {
        gpsBeginTime            GPSEphemerisExtensionTime,
        gpsEndTime                GPSEphemerisExtensionTime,
        gpsSatEventsInfo        GPSSatEventsInfo,
    ...
    }
    GPSSatEventsInfo

GPSSatEventsInfo

    GPSSatEventsInfo ::= SEQUENCE {
        eventOccured        BIT STRING (SIZE (32)),
        futureEventNoted    BIT STRING (SIZE (32)),
    ...
    }
    -- If a bit is clear in the eventOccured field it indicates that no known errors have occured since
    -- the gpsBeginTime nor is a maneuver planned for the next sixty minutes.
    -- If a bit is set in the futureEventNoted field it indicates that a maneuver is planned during the
    -- time period between current time plus sixty minutes and gpsEndTime
    -- DGPS Corrections Validity Period:
    -- This element may only be included if DGPSCorrections IE is included in ControlHeader element.
    -- DGPSCorrectionsValidityPeriod shall contain the same number of elements as the SeqOfSatElement
    -- included in DGPSCorrections IE
    DGPSCorrectionsValidityPeriod

DGPSExtensionSatElement

    DGPSExtensionSatElement ::= SEQUENCE {
        satelliteID            SatelliteID,
        udreGrowthRate        INTEGER(0..7),     -- coding according to annex
        udreValidityTime    INTEGER(0..7),     -- coding according to annex
        ...
    }
    -- GPS Reference Time Rel-10 Extension:
    GPSReferenceTime-R10-Ext

GPSReferenceTime_R10_Ext

    GPSReferenceTime-R10-Ext ::= SEQUENCE {
        gpsWeekCycleNumber    INTEGER(0..7)     -- coding according to annex
    }
    -- GPS Acquisition Assistance Rel-10 Extension:
    -- GPSAcquisAssist-R10-Ext shall contain the same number of elements as the SeqOfAcquisElement
    -- included in AcquisAssist IE
    GPSAcquisAssist-R10-Ext

GPSAcquisAssist_R10_Ext_Element

    GPSAcquisAssist-R10-Ext-Element::= SEQUENCE {
        satelliteID            SatelliteID,
        azimuthLSB            INTEGER(0..15),
        elevationLSB        INTEGER(0..15)
    }
    -- GPS Almanac Rel-10 Extension:
    GPSAlmanac-R10-Ext

GPSAlmanac_R10_Ext

    GPSAlmanac-R10-Ext ::= SEQUENCE {
        completeAlmanacProvided        BOOLEAN    -- TRUE means that complete Almanac is provided
    }
    Rel-7-MsrPosition-Rsp-Extension

Rel_7_MsrPosition_Rsp_Extension

    Rel-7-MsrPosition-Rsp-Extension ::= SEQUENCE {
        velEstimate     VelocityEstimate OPTIONAL,
     -- Horizontal Velocity
     -- Horizontal with Vertical Velocity
     -- Horizontal Velocity with Uncertainty
     -- Horizontal with Vertical Velocity and Uncertainty
     ganssLocationInfo GANSSLocationInfo OPTIONAL,
     ganssMeasureInfo GANSSMeasureInfo OPTIONAL,
        ...
    -- Further Release 7 extensions here
    }
    -- GANSS Location Information contains location estimate, time stamp with uncertainty
    -- and optionally Reference Frame field
    GANSSLocationInfo

GANSSLocationInfo

    GANSSLocationInfo ::= SEQUENCE {
         referenceFrame                 ReferenceFrame             OPTIONAL, -- Reference Frame Number
         ganssTODm                     GANSSTODm                 OPTIONAL, -- GNSS TOD modulo
         ganssTODFrac                 INTEGER (0 .. 16384)     OPTIONAL, -- Coding according to Annex
        -- a value of 16384 shall not be encoded by the sender
        -- the receiver shall consider a value of 16384 to be invalid data
        ganssTODUncertainty         GANSSTODUncertainty     OPTIONAL, -- Coding according to Annex
         ganssTimeID                 INTEGER (0 .. 7)         OPTIONAL, -- Coding according to Annex
        fixType                         FixType,
         posData                     PositionData,
         stationaryIndication         INTEGER(0 .. 1)         OPTIONAL, -- ‘0’ if moving or motion not
                                                                      -- known
        -- Possible shapes carried in posEstimate are
        -- ellipsoid point,
        -- ellipsoid point with uncertainty circle
        -- ellipsoid point with uncertainty ellipse
        -- ellipsoid point with altitude and uncertainty ellipsoid
        posEstimate                     Ext-GeographicalInformation,
         ...
    }
    PositionData

ReferenceFrame

    ReferenceFrame ::= SEQUENCE {
     referenceFN INTEGER (0 .. 65535),
        -- Note that applicable range for referenceFN is 0 - 42431
     referenceFNMSB INTEGER (0 .. 63) OPTIONAL -- MSB of Reference Frame Number
    }
    -- GANSS Measurement Information
    GANSSMeasureInfo

GANSSMeasureInfo

    GANSSMeasureInfo ::= SEQUENCE {
        -- Measurement info elements
    ganssMsrSetList SeqOfGANSS-MsrSetElement
    }
    SeqOfGANSS-MsrSetElement

GANSS_MsrSetElement

    GANSS-MsrSetElement ::= SEQUENCE {
        referenceFrame             ReferenceFrame         OPTIONAL, -- Reference Frame Number
        -- if ganssTODm is included, it is the GNSS specific system time of the GANSS reported
        -- first in ganss-SgnTypeList. If GPS Measurement Information element is not included in
        -- a Measure Position Response component, this field shall be present.
        ganssTODm                 GANSSTODm             OPTIONAL, -- GANSS TOD modulo 1 hour
        deltaGANSSTOD             INTEGER (0 .. 127)     OPTIONAL,
        ganssTODUncertainty     GANSSTODUncertainty    OPTIONAL, -- Coding according to Annex
        --N_GANSS can be read from number of elements of SeqOfGANSS-MsrElement
        ganss-MsrElementList    SeqOfGANSS-MsrElement
    }
    SeqOfGANSS-MsrElement

GANSS_MsrElement

    GANSS-MsrElement ::= SEQUENCE {
        ganssID        INTEGER (0..7)     OPTIONAL, --Absence means Galileo
        ganss-SgnTypeList         SeqOfGANSS-SgnTypeElement
    }
    -- Measurements can be returned up to 8 different signal types
    -- N_SGN_TYPE can be read from number of elements of SeqOfGANSS-SgnTypeElement
    -- Reporting of multiple signal types as defined in A.2.2.4g
    SeqOfGANSS-SgnTypeElement

GANSS_SgnTypeElement

    GANSS-SgnTypeElement ::= SEQUENCE {
        ganssSignalID            GANSSSignalID, -- Coding according to Annex
        ganssCodePhaseAmbiguity    INTEGER (0 .. 127)                OPTIONAL,
         --N_SGN can be read from number of elements of SeqOfGANSS-SgnElement
         ganss-SgnList SeqOfGANSS-SgnElement,
         ...
    }
    -- Up to 16 Measurements can be returned per signal type
    SeqOfGANSS-SgnElement

GANSS_SgnElement

    GANSS-SgnElement ::= SEQUENCE {
         svID                 SVID,
        cNo                 INTEGER (0 .. 63),
        mpathDet             MpathIndic,                                  -- Coding according to Annex
        carrierQualityInd     INTEGER (0 .. 3)             OPTIONAL,      -- Coding according to Annex
        codePhase             INTEGER (0 .. 2097151),
        integerCodePhase     INTEGER (0 .. 127)             OPTIONAL,
        codePhaseRMSError     INTEGER (0..63),                          -- Coding according to Annex
        doppler             INTEGER (-32768 .. 32767)     OPTIONAL,
        adr                 INTEGER (0 .. 33554431)     OPTIONAL
    }
    Rel7-AssistanceData-Extension

Rel7_AssistanceData_Extension

    Rel7-AssistanceData-Extension ::= SEQUENCE {
        ganss-AssistData                                GANSS-AssistData    OPTIONAL,
        ganssCarrierPhaseMeasurementRequest                NULL                OPTIONAL,
        ganssTODGSMTimeAssociationMeasurementRequest    NULL                OPTIONAL,
         add-GPS-AssistData                                Add-GPS-AssistData    OPTIONAL,
        ...
    -- Possibly more extensions for Release 7 here
    }
    -- Rel-7 Positioning Capability parameters here
    PosCapabilities

PosCapabilities

    PosCapabilities ::= SEQUENCE {
    -- nonGANSSpositionMethods shall be included if and only if any
    -- of the non-GANSS methods is supported.
        nonGANSSpositionMethods        NonGANSSPositionMethods    OPTIONAL,
    -- gANSSpositionMethods shall be included if and only if any of the GANSS methods is supported.
        gANSSPositionMethods        GANSSPositionMethods    OPTIONAL,
    -- multipleMeasurementSets shall be present if and only if 'multiple sets' is supported
    -- for any of the positioning methods
        multipleMeasurementSets        MultipleMeasurementSets    OPTIONAL,
        ...
    }
    NonGANSSPositionMethods

GANSSPositionMethod

    GANSSPositionMethod ::= SEQUENCE {
        ganssID                         INTEGER (0..7)                 OPTIONAL, --Absence means Galileo
    -- gANSSPositioningMethodTypes may be present for PosCapability-Req
    -- and shall be present for PosCapability-Rsp
        gANSSPositioningMethodTypes        GANSSPositioningMethodTypes OPTIONAL,
        gANSSSignals                    GANSSSignals,
        ... ,
    -- sbasID shall be present if and only if ganssID indicates SBAS
        sbasID                            SBASID                        OPTIONAL
    }
    GANSSPositioningMethodTypes

AssistanceSupported

    AssistanceSupported ::= SEQUENCE {
        gpsAssistance                        GPSAssistance                        OPTIONAL,
        gANSSAssistanceSet                    GANSSAssistanceSet                    OPTIONAL,
        ... ,
    -- gANSSAdditionalAssistanceChoices shall be present if the MS supports other than native models
        gANSSAdditionalAssistanceChoices    GANSSAdditionalAssistanceChoices    OPTIONAL
    }
    -- GPS assistance data supported
    GPSAssistance

GANSSAssistanceSet

    GANSSAssistanceSet ::= SEQUENCE {
        commonGANSSAssistance        CommonGANSSAssistance,
        specificGANSSAssistance        SpecificGANSSAssistance,
        ...
    }
    -- Common GANSS assistance data supported
    CommonGANSSAssistance

GANSSAssistanceForOneGANSS

    GANSSAssistanceForOneGANSS ::= SEQUENCE {
        ganssID                    INTEGER (0..7)     OPTIONAL, --Absence means Galileo
        gANSSAssistance            GANSSAssistance,
        ...
    }
    -- specific GANSS assistance data supported
    GANSSAssistance

GANSSAdditionalAssistanceChoicesForOneGANSS

    GANSSAdditionalAssistanceChoicesForOneGANSS ::= SEQUENCE {
        ganssID                            INTEGER (0..7)     OPTIONAL, --Absence means Galileo
        ganssClockModelChoice            GANSSModelID     OPTIONAL,
        gannsOrbitModelChoice            GANSSModelID     OPTIONAL,
        ganssAlmanacModelChoice            GANSSModelID     OPTIONAL,
        ganssAdditionalUTCModelChoice    GANSSModelID     OPTIONAL,
        ...
    }
    GANSSModelID

AssistanceNeeded

    AssistanceNeeded ::= SEQUENCE {
        gpsAssistanceData        GPSAssistanceData        OPTIONAL,
        ganssAssistanceData        GANSSAssistanceData        OPTIONAL,
        ...
    }
    END

MethodType

    MethodType ::= CHOICE {
        msAssisted        AccuracyOpt,    -- accuracy is optional
        msBased            Accuracy,        -- accuracy is mandatory
        msBasedPref        Accuracy,        -- accuracy is mandatory
        msAssistedPref    Accuracy         -- accuracy is mandatory
    }
    -- Accuracy of the location estimation
    AccuracyOpt

SystemInfoAssistBTS

    SystemInfoAssistBTS ::= CHOICE {
        notPresent        NULL,
        present            AssistBTSData
    }
    -- Actual assistance data for system information base station
    AssistBTSData

ReferenceIdentityType

    ReferenceIdentityType ::= CHOICE {
        bsicAndCarrier    BSICAndCarrier,        -- BSIC and Carrier
        ci                CellID,                -- Cell ID, LAC not needed
        requestIndex    RequestIndex,        -- Index to Requested Neighbor List
        systemInfoIndex    SystemInfoIndex,    -- Index to System info list, this type of ref. identity
                                            -- shall not be used by the MS unless it has received
                                            -- the SystemInfoAssistData from the SMLC for this cell.
        ciAndLAC        CellIDAndLAC        -- CI and LAC
    }
    BSICAndCarrier

OTD_MsrsOfOtherSets

    OTD-MsrsOfOtherSets ::= CHOICE {
        identityNotPresent    OTD-Measurement,
        identityPresent        OTD-MeasurementWithID
    }
    -- For this OTD measurement identity is same as the identity of BTS
    -- in the first set with same sequence number
    OTD-Measurement

NeighborIdentity

    NeighborIdentity ::= CHOICE {
        bsicAndCarrier        BSICAndCarrier,        -- BSIC and Carrier
        ci                    CellID,                -- Cell ID, LAC not needed
        multiFrameCarrier    MultiFrameCarrier,     -- MultiFrameOffest and BSIC
        requestIndex        RequestIndex,        -- Index to Requested Neighbor List
        systemInfoIndex        SystemInfoIndex,    -- Index to System info list, this type of neighbour
                                                -- identity shall not be used by the MS unless it has
                                                -- received the SystemInfoAssistData from the SMLC for
                                                -- this cell.
        ciAndLAC            CellIDAndLAC        -- CI and LAC
    }
    -- Multiframe and carrier
    MultiFrameCarrier

SatStatus

    SatStatus ::= CHOICE {
        -- New satellite, new Navigation Model
        newSatelliteAndModelUC    UncompressedEphemeris,
        -- Existing satellite, Existing Navigation Model
        oldSatelliteAndModel    NULL,
        -- Existing satellite, new Navigation Model
        newNaviModelUC            UncompressedEphemeris,
        ...
    }
    -- Uncompressed satellite emhemeris and clock corrections
    UncompressedEphemeris

SystemInfoAssistBTS_R98_ExpOTD

    SystemInfoAssistBTS-R98-ExpOTD ::= CHOICE {
        notPresent        NULL,
        present            AssistBTSData-R98-ExpOTD
    }
    -- This element completes AssistBTSData IE
    AssistBTSData-R98-ExpOTD

GANSSOrbitModel

    GANSSOrbitModel ::= CHOICE {
        keplerianSet         NavModel-KeplerianSet,        -- Model-1
        ... ,
        navKeplerianSet         NavModel-NAVKeplerianSet,     -- Model-2
        cnavKeplerianSet    NavModel-CNAVKeplerianSet,     -- Model-3
        glonassECEF            NavModel-GLONASSecef,         -- Model-4
        sbasECEF            NavModel-SBASecef            -- Model-5
    }
    -- Navigation model in Keplerian parameters
    NavModel-KeplerianSet

GANSSClockModel

    GANSSClockModel ::= CHOICE {
        standardClockModelList     SeqOfStandardClockModelElement,    -- Model-1
        ... ,
        navClockModel             NAVclockModel,                     -- Model-2
        cnavClockModel             CNAVclockModel,                     -- Model-3
        glonassClockModel         GLONASSclockModel,                 -- Model-4
        sbasClockModel             SBASclockModel                        -- Model-5
    }
    SeqOfStandardClockModelElement

GANSSAlmanacElement

    GANSSAlmanacElement ::= CHOICE {
        keplerianAlmanacSet         Almanac-KeplerianSet,            -- Model-1
         ...,
        keplerianNAVAlmanac         Almanac-NAVKeplerianSet,         -- Model-2
        keplerianReducedAlmanac    Almanac-ReducedKeplerianSet,     -- Model-3
        keplerianMidiAlmanac    Almanac-MidiAlmanacSet,         -- Model-4
        keplerianGLONASS        Almanac-GlonassAlmanacSet,         -- Model-5
        ecefSBASAlmanac            Almanac-ECEFsbasAlmanacSet        -- Model-6
    }
    -- Almanac parameters according to Keplerian parameters
    Almanac-KeplerianSet

GANSSAddUTCModel

    GANSSAddUTCModel ::= CHOICE {
        utcModel2            UTCmodelSet2,
        utcModel3            UTCmodelSet3,
        utcModel4            UTCmodelSet4,
        ...
    }
    UTCmodelSet2

GANSSAuxiliaryInformation

    GANSSAuxiliaryInformation ::= CHOICE{
        ganssID1    GANSS-ID1,     -- This choice may only be present if GANSS ID indicates Modernized GPS
        ganssID3    GANSS-ID3,     -- This choice may only be present if GANSS ID indicates GLONASS
        ...
    }
    GANSS-ID1

FixType_twoDFix_

    const FixType twoDFix (0)

FixType_threeDFix_

    const FixType threeDFix (1)

maxGPSAssistanceData

    const integer maxGPSAssistanceData    INTEGER ::= 40
    GANSSAssistanceData

maxGANSSAssistanceData

    const integer maxGANSSAssistanceData    INTEGER ::= 40
    -- Protocol Error Causes
    ErrorCodes

GANSSPositioningMethod_gps_

    const GANSSPositioningMethod gps                (0)

GANSSPositioningMethod_glonass_

    const GANSSPositioningMethod glonass           (5)

GANSSPositioningMethod_modernizedGPS_

    const GANSSPositioningMethod modernizedGPS      (3)

GANSSPositioningMethod_qzss_

    const GANSSPositioningMethod qzss                (4)

GANSSPositioningMethod_galileo_

    const GANSSPositioningMethod galileo           (1)

GANSSPositioningMethod_sbas_

    const GANSSPositioningMethod sbas                (2)

PositionData_gps_

    const PositionData gps                (1)

PositionData_e_otd_

    const PositionData e-otd               (0)

PositionData_glonass_

    const PositionData glonass           (6)

PositionData_qzss_

    const PositionData qzss                (5)

PositionData_galileo_

    const PositionData galileo           (2)

PositionData_modernizedGPS_

    const PositionData modernizedGPS      (4)

PositionData_sbas_

    const PositionData sbas                (3)

NonGANSSPositionMethods_msBasedGPS_

    const NonGANSSPositionMethods msBasedGPS          (3)

NonGANSSPositionMethods_msAssistedGPS_

    const NonGANSSPositionMethods msAssistedGPS     (2)

NonGANSSPositionMethods_msBasedEOTD_

    const NonGANSSPositionMethods msBasedEOTD          (1)

NonGANSSPositionMethods_standaloneGPS_

    const NonGANSSPositionMethods standaloneGPS     (4)

NonGANSSPositionMethods_msAssistedEOTD_

    const NonGANSSPositionMethods msAssistedEOTD     (0)

GANSSPositioningMethodTypes_msAssisted_

    const GANSSPositioningMethodTypes msAssisted    (0)

GANSSPositioningMethodTypes_msBased_

    const GANSSPositioningMethodTypes msBased         (1)

GANSSPositioningMethodTypes_standalone_

    const GANSSPositioningMethodTypes standalone    (2)

GANSSSignals_signal6_

    const GANSSSignals signal6 (5)

GANSSSignals_signal5_

    const GANSSSignals signal5 (4)

GANSSSignals_signal7_

    const GANSSSignals signal7 (6)

GANSSSignals_signal8_

    const GANSSSignals signal8 (7)

GANSSSignals_signal3_

    const GANSSSignals signal3 (2)

GANSSSignals_signal1_

    const GANSSSignals signal1 (0)

GANSSSignals_signal2_

    const GANSSSignals signal2 (1)

GANSSSignals_signal4_

    const GANSSSignals signal4 (3)

SBASID_waas_

    const SBASID waas      (0)

SBASID_gagan_

    const SBASID gagan      (3)

SBASID_masas_

    const SBASID masas      (2)

SBASID_egnos_

    const SBASID egnos      (1)

MultipleMeasurementSets_gps_

    const MultipleMeasurementSets gps          (1)

MultipleMeasurementSets_eotd_

    const MultipleMeasurementSets eotd     (0)

MultipleMeasurementSets_ganss_

    const MultipleMeasurementSets ganss     (2)

GPSAssistance_ephemerisExtension_

    const GPSAssistance ephemerisExtension        (9)

GPSAssistance_realTimeIntegrity_

    const GPSAssistance realTimeIntegrity        (8)

GPSAssistance_acquisitionAssistance_

    const GPSAssistance acquisitionAssistance    (7)

GPSAssistance_dGPScorrections_

    const GPSAssistance dGPScorrections            (4)

GPSAssistance_navigationmodel_

    const GPSAssistance navigationmodel            (3)

GPSAssistance_referenceTime_

    const GPSAssistance referenceTime            (6)

GPSAssistance_ionosphericModel_

    const GPSAssistance ionosphericModel        (2)

GPSAssistance_uTCmodel_

    const GPSAssistance uTCmodel                (1)

GPSAssistance_ephemerisExtensionCheck_

    const GPSAssistance ephemerisExtensionCheck    (10)

GPSAssistance_referenceLocation_

    const GPSAssistance referenceLocation        (5)

GPSAssistance_almanac_

    const GPSAssistance almanac                    (0)

CommonGANSSAssistance_ionosphericModel_

    const CommonGANSSAssistance ionosphericModel         (3)

CommonGANSSAssistance_referenceLocation_

    const CommonGANSSAssistance referenceLocation         (1)

CommonGANSSAssistance_earthOrientationParam_

    const CommonGANSSAssistance earthOrientationParam     (5)

CommonGANSSAssistance_referenceTime_

    const CommonGANSSAssistance referenceTime             (0)

CommonGANSSAssistance_addIonosphericModel_

    const CommonGANSSAssistance addIonosphericModel         (4)

GANSSAssistance_differentialCorrections_

    const GANSSAssistance differentialCorrections            (1)

GANSSAssistance_timeModelGNSS_GNSS_

    const GANSSAssistance timeModelGNSS-GNSS                (6)

GANSSAssistance_auxiliaryInformation_

    const GANSSAssistance auxiliaryInformation            (11)

GANSSAssistance_realTimeIntegrity_

    const GANSSAssistance realTimeIntegrity                (0)

GANSSAssistance_almanac_

    const GANSSAssistance almanac                            (2)

GANSSAssistance_addUTCmodel_

    const GANSSAssistance addUTCmodel                        (10)

GANSSAssistance_referenceMeasurementInformation_

    const GANSSAssistance referenceMeasurementInformation    (3)

GANSSAssistance_ephemerisExtensionCheck_

    const GANSSAssistance ephemerisExtensionCheck            (9)

GANSSAssistance_timeModelGNSS_UTC_

    const GANSSAssistance timeModelGNSS-UTC                (5)

GANSSAssistance_ephemerisExtension_

    const GANSSAssistance ephemerisExtension                (8)

GANSSAssistance_databitassistance_

    const GANSSAssistance databitassistance                (7)

GANSSAssistance_navigationModel_

    const GANSSAssistance navigationModel                    (4)

GANSSModelID_model6_

    const GANSSModelID model6 (5)

GANSSModelID_model1_

    const GANSSModelID model1 (0)

GANSSModelID_model4_

    const GANSSModelID model4 (3)

GANSSModelID_model3_

    const GANSSModelID model3 (2)

GANSSModelID_model5_

    const GANSSModelID model5 (4)

GANSSModelID_model7_

    const GANSSModelID model7 (6)

GANSSModelID_model8_

    const GANSSModelID model8 (7)

GANSSModelID_model2_

    const GANSSModelID model2 (1)

© Copyright Testing Technologies IST GmbH 2012