OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_14x

Declared in module SUPL_V2_SET_INITIATED_Tests
Subgroups: TC_140, TC_141, TC_142

Test cases Summary
TC_140_1 |
TC_140_2 | To test SET correctly actions timer UT1 - Test 2: Triggered Session
TC_141_1 |
TC_141_2 | To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
TC_141_3 | To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
TC_141_4 | To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
TC_142_1 |
TC_142_2 | To test SET correctly actions timer UT3 - Test 2: Triggered Session
TC_143 | To test SET correctly actions timer UT7

## Details

TC_140_1

    testcase TC_140_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
Runs On: SUPLComponent
System: SystemInterfaces

TC_140_2

    testcase TC_140_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
To test SET correctly actions timer UT1 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-140-2 TP version: Test Case Id : SUPL-2.0-con-140 Test Object : Client Test Case Description : To test SET correctly actions timer UT1 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 2: Triggered session [Includes Optional Features] 6. Start a SI Periodic Triggered Location Session, or a SI Area Event Triggered Location session if Periodic Location sessions are not supported in the SET. 7. The SET sends SUPL TRIGGERED START 8. Do not respond 9. After timer UT1 expires (depending on ixit_timer_UT1) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 10. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : 1. At step 4 and step 9 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 5 and step 10 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_1

    testcase TC_141_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_2

    testcase TC_141_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-2 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 8. Start a SI Periodic Triggered Location Session 9. The SET sends SUPL TRIGGERED START 10. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 11. When the first periodic trigger occurs the SET sends SUPL POS INIT 12. Do not respond 13. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the SUPL POS session) Note that the SET may release the secure connection at this time. 14. When the second periodic trigger occurs the SET sends SUPL POS INIT 15. A SUPL POS session takes place 16. Send SUPL REPORT 17. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_3

    testcase TC_141_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
Purpose: SUPL-2.0-con-141-3 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Test Procedure : Test 3: No SUPL POS session (Immediate session) 18. Start a SI Location Session 19. The SET sends SUPL START 20. Send SUPL RESPONSE with: Positioning Method set to Enhanced Cell/sector 21. The SET sends SUPL POS INIT 22. Do not respond 23. After timer UT2 expires (depending on ixit_timer_UT2) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 24. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : Test 1 and Test 3: 1. At step 6 and step 23 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 7 and step 24 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_4

    testcase TC_141_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-4 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 4: No SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any triggered service. This test case has been written for a Periodic Triggered Location Session. The case where Periodic Location sessions is not supported in the SET is FFS 25. Start a SI Periodic Triggered Location Session 26. The SET sends SUPL TRIGGERED START 27. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to Enhanced Cell/sector 28. When the first periodic trigger occurs the SET sends SUPL POS INIT 29. Do not respond 30. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the individual location session) 31. When the second periodic trigger occurs the SET sends SUPL POS INIT 32. Send SUPL REPORT 33. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_142_1

    testcase TC_142_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
Runs On: SUPLComponent
System: SystemInterfaces

TC_142_2

    testcase TC_142_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
To test SET correctly actions timer UT3 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-142-2 TP version: Test Case Id : SUPL-2.0-con-142 Test Object : Client Test Case Description : To test SET correctly actions timer UT3 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: Triggered session Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 9. Start a SI Periodic Triggered Location Session 10. The SET sends SUPL TRIGGERED START 11. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 12. When the first periodic trigger occurs the SET sends SUPL POS INIT 13. A SUPL POS session takes place 14. After the SET sends the final SUPL POS do not respond 15. (After timer UT3 expires (depending on ixit_timer_UT3) the SET will continue to the next trigger in the session) Note that the SET may release the secure connection at this time. 16. When the second periodic trigger occurs the SET sends SUPL POS INIT 17. A SUPL POS session takes place 18. Send SUPL REPORT 19. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2: 3. At step 16 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_143

    testcase TC_143() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x
To test SET correctly actions timer UT7
Purpose: SUPL-2.0-con-143 TP version: Test Case Id : SUPL-2.0-con-143 Test Object : Client Test Case Description : To test SET correctly actions timer UT7 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ((ics_periodic_SET_initiated OR ics_event_SET_initiated) AND NOT (ics_periodic_Network_initiated OR ics_event_Network_initiated)) AND ixit_timer_UT7 Test Procedure : 1. Start a SI Periodic Triggered Location Session, or a SI Area Event Triggered Location session if Periodic Location sessions are not supported in the SET. 2. Allow the first trigger to occur (either periodic or area event) and the first location session to complete 3. From the SET stop the Triggered Location Session 4. The SET sends SUPL TRIGGERED STOP 5 Do not respond 6. After timer UT7 expires (depending on ixit_timer_UT7) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 7. The Triggered Location Session ends and the SET releases the secure IP connection. Pass-Criteria : 1. At step 6 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 7 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012