OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_14x.TC_141

Declared in module SUPL_V2_SET_INITIATED_Tests

Test cases Summary
TC_141_1 |
TC_141_2 | To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
TC_141_3 | To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
TC_141_4 | To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)

## Details

TC_141_1

    testcase TC_141_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_2

    testcase TC_141_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-2 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 8. Start a SI Periodic Triggered Location Session 9. The SET sends SUPL TRIGGERED START 10. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 11. When the first periodic trigger occurs the SET sends SUPL POS INIT 12. Do not respond 13. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the SUPL POS session) Note that the SET may release the secure connection at this time. 14. When the second periodic trigger occurs the SET sends SUPL POS INIT 15. A SUPL POS session takes place 16. Send SUPL REPORT 17. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_3

    testcase TC_141_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
Purpose: SUPL-2.0-con-141-3 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Test Procedure : Test 3: No SUPL POS session (Immediate session) 18. Start a SI Location Session 19. The SET sends SUPL START 20. Send SUPL RESPONSE with: Positioning Method set to Enhanced Cell/sector 21. The SET sends SUPL POS INIT 22. Do not respond 23. After timer UT2 expires (depending on ixit_timer_UT2) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 24. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : Test 1 and Test 3: 1. At step 6 and step 23 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 7 and step 24 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_4

    testcase TC_141_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-4 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 4: No SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any triggered service. This test case has been written for a Periodic Triggered Location Session. The case where Periodic Location sessions is not supported in the SET is FFS 25. Start a SI Periodic Triggered Location Session 26. The SET sends SUPL TRIGGERED START 27. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to Enhanced Cell/sector 28. When the first periodic trigger occurs the SET sends SUPL POS INIT 29. Do not respond 30. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the individual location session) 31. When the second periodic trigger occurs the SET sends SUPL POS INIT 32. Send SUPL REPORT 33. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012