OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group suplMessagesParameterGroup

Declared in module SUPL_V2_Templates

Constants Summary
c_GNSSPosTechnologyGloneASS |
c_GNSSPosTechnologyGalileoGloneASS |
c_GNSSPosTechnologyGalileo |
c_GNSSPosTechnologyGalileoGloneASSiXIT |
c_geographicTargetAreaCircularIn |
c_geographicTargetAreaCircularOut |

Templates Summary
m_ver2SuplInitExtensionGnssPosTechnology |
m_ver2SuplInitExtensionTriggerType |
m_ver2SuplInitMinimumMajorVersion |
m_ver2SuplInitProtectionLevel |
m_ver2SuplInitESlpAddress |
m_triggerParamsPeriodic |
m_triggerParamsAreaEvent |
m_reportingModeBatch |
m_reportingModeQuasiReal |
m_batchRepConditionsByInterval |
m_batchRepConditionsByMinutes |
m_batchRepConditionsByEndofsession |
m_batchRepType |
mw_posTechICS |
mw_posTechICSV1 |
mw_posTech |
mw_posTechV1 |
m_areaIdList |
mw_setCapabilities |
mw_setCapabilitiesExt |
m_methodType_msAssistedV5 | TODO: Add description
m_methodType_msAssistedV10 | TODO: Add description
m_methodType_msAssitedPrefV5 | MS-AssistedPref Method Type
m_methodType_msAssitedPrefV10 | MS-AssistedPref Method Type
m_accuracyOpt_omittedV5 | TODO: Add description
m_accuracyOpt_omittedV10 | TODO: Add description
m_methodType_msBasedV5 |
m_methodType_msBasedV10 |
m_methodType_msBasedPrefV5 | MS-BasedPref Method Type
m_methodType_msBasedPrefV10 | MS-BasedPref Method Type
m_areaIdLists_one_areaId | TODO: Add description
m_areaId_gsm_cellId | Builds an Area Id message instance from a GSM cell ID
m_areaId_wcdma_cellId | Builds an Area Id message instance from a WCDMA cell ID
m_areaId_lte_cellId | Builds an Area Id message instance from a LTE cell ID
m_areaId_cdma_cellId | Builds an Area Id message instance from a CDMA cell ID
m_areaId_hrpd_cellId | Builds an Area Id message instance from a hRPD cell ID
m_gsmAreaId_cellId | GSM area ID from cell ID
m_wcdmaAreaId_cellId | WCDMA Area ID from cell ID
m_lteAreaId_cellId | LTE Area ID from cell ID
m_cdmaAreaId_cellId | CDMA Area ID from cell ID
m_hrpdAreaId_cellId | hRPD Area ID from cell ID
m_BasicProtectionLevel | basic ProtectionLevel from SUPL INIT
m_ProtectionParamsDefault |
m_ProtectionLevel |
m_keyIdentifier |
m_keyIdentifier_incorrect |
m_basicReplayCounter |
m_basicMAC |
m_basicMAC_zero |
m_SLPAddressFQDN |
m_ESLPAddressIP |
m_notificationEmergency |
m_setTriggerServiceSupported |
m_setEventTriggerCap |

## Details

c_GNSSPosTechnologyGloneASS

    const GNSSPosTechnology c_GNSSPosTechnologyGloneASS :=
    {
        gps := false,
        galileo := false,
        sbas := false,
        modernized_gps := false,
        qzss := false,
        glonass := true
    }

Declared in group suplMessagesParameterGroup

c_GNSSPosTechnologyGalileoGloneASS

    const GNSSPosTechnology c_GNSSPosTechnologyGalileoGloneASS :=
    {
        gps := false,
        galileo := true,
        sbas := false,
        modernized_gps := false,
        qzss := false,
        glonass := true
    }

Declared in group suplMessagesParameterGroup

c_GNSSPosTechnologyGalileo

    const GNSSPosTechnology c_GNSSPosTechnologyGalileo :=
    {
        gps := false,
        galileo := true,
        sbas := false,
        modernized_gps := false,
        qzss := false,
        glonass := false
    }

Declared in group suplMessagesParameterGroup

c_GNSSPosTechnologyGalileoGloneASSiXIT

    const GNSSPosTechnology c_GNSSPosTechnologyGalileoGloneASSiXIT :=
    {
    gps := false,
    galileo := ixit_gANSS.galileo,
    sbas := false,
    modernized_gps := false,
    qzss := false,
    glonass := ixit_gANSS.gloneass
    }

Declared in group suplMessagesParameterGroup

c_geographicTargetAreaCircularIn

    const GeographicTargetArea c_geographicTargetAreaCircularIn :=
    {
        circularArea := {
            coordinate := {
                latitudeSign := north,
                latitude := fx_GadLatitude(35.666667),
                longitude := fx_GadLongitude(139.75)
            },
            radius := 1000,
            radius_min := omit,
            radius_max := omit
        }
    }

Declared in group suplMessagesParameterGroup

c_geographicTargetAreaCircularOut

    const GeographicTargetArea c_geographicTargetAreaCircularOut :=
    {
        circularArea := {
            coordinate := {
                latitudeSign := north,
                latitude := fx_GadLatitude(35.666667),
                longitude := fx_GadLongitude(139.77)
            },
            radius := 1000,
            radius_min := omit,
            radius_max := omit
        }
    }

Declared in group suplMessagesParameterGroup

m_ver2SuplInitExtensionGnssPosTechnology

    template Ver2_SUPL_INIT_extension
    m_ver2SuplInitExtensionGnssPosTechnology(template GNSSPosTechnology
                                                 p_gnssPosTechnology) := {
        notificationMode := omit,
        supportedNetworkInformation := omit,
        triggerType := omit,
        e_SLPAddress := omit,
        historicReporting := omit,
        protectionLevel := omit,
        gnssPosTechnology := p_gnssPosTechnology,
        minimumMajorVersion := omit
    }

Declared in group suplMessagesParameterGroup
Returns: Ver2_SUPL_INIT_extension -
Parameters:

- p_gnssPosTechnology -

m_ver2SuplInitExtensionTriggerType

    template Ver2_SUPL_INIT_extension
    m_ver2SuplInitExtensionTriggerType(template TriggerType p_triggerType)
    := {
        notificationMode := omit,
        supportedNetworkInformation := omit,
        triggerType := p_triggerType,
        e_SLPAddress := omit,
        historicReporting := omit,
        protectionLevel := omit,
        gnssPosTechnology := omit,
        minimumMajorVersion := omit
    }

Declared in group suplMessagesParameterGroup
Returns: Ver2_SUPL_INIT_extension -
Parameters:

- p_triggerType -

m_ver2SuplInitMinimumMajorVersion

    template Ver2_SUPL_INIT_extension
    m_ver2SuplInitMinimumMajorVersion(template integer p_minimumMajorVersion)
    := {
    notificationMode := omit,
    supportedNetworkInformation := omit,
    triggerType := omit,
    e_SLPAddress := omit,
    historicReporting := omit,
    protectionLevel := omit,
    gnssPosTechnology := omit,
    minimumMajorVersion := p_minimumMajorVersion
    }

Declared in group suplMessagesParameterGroup
Returns: Ver2_SUPL_INIT_extension -
Parameters:

- p_minimumMajorVersion -

m_ver2SuplInitProtectionLevel

    template Ver2_SUPL_INIT_extension
    m_ver2SuplInitProtectionLevel(template  ProtectionLevel p_protectionLevel)
    := {
    notificationMode := omit,
    supportedNetworkInformation := omit,
    triggerType := omit,
    e_SLPAddress := omit,
    historicReporting := omit,
    protectionLevel := p_protectionLevel,
    gnssPosTechnology := omit,
    minimumMajorVersion := omit
    }

Declared in group suplMessagesParameterGroup
Returns: Ver2_SUPL_INIT_extension -
Parameters:

- p_protectionLevel -

m_ver2SuplInitESlpAddress

    template Ver2_SUPL_INIT_extension
    m_ver2SuplInitESlpAddress(template SLPAddress p_sLPAddress)
    := {
    notificationMode := omit,
    supportedNetworkInformation := omit,
    triggerType := omit,
    e_SLPAddress := p_sLPAddress,
    historicReporting := omit,
    protectionLevel := omit,
    gnssPosTechnology := omit,
    minimumMajorVersion := omit
    }

Declared in group suplMessagesParameterGroup
Returns: Ver2_SUPL_INIT_extension -
Parameters:

- p_sLPAddress -

m_triggerParamsPeriodic

    template TriggerParams
    m_triggerParamsPeriodic(_0PeriodicParams p_number, _0PeriodicParams0 p_interval,
    _0PeriodicParams1 p_start) := {
        periodicParams := {
            numberOfFixes := p_number,
            intervalBetweenFixes := p_interval,
            startTime := p_start
        }
    }

Declared in group suplMessagesParameterGroup
Returns: TriggerParams -
Parameters:

- p_number -
- p_interval -
- p_start -

m_triggerParamsAreaEvent

    template TriggerParams
    m_triggerParamsAreaEvent(template(present) AreaEventType p_areaEventType,
                             template(present) boolean p_locationEstimate,
                             template RepeatedReportingParams
                                 p_repeatedReportingParams,
                             template _0AreaEventParams p_start,
                             template _0AreaEventParams0 p_stop,
                             template GeographicTargetAreaList
                                 p_geographicTargetAreaList,
                             template _0AreaEventParams1 p_areaIdLists) := {
        areaEventParams := {
            areaEventType := p_areaEventType,
            locationEstimate := p_locationEstimate,
            repeatedReportingParams := p_repeatedReportingParams,
            startTime := p_start,
            stopTime := p_stop,
            geographicTargetAreaList := p_geographicTargetAreaList,
            areaIdLists := p_areaIdLists
        }
    }

Declared in group suplMessagesParameterGroup
Returns: TriggerParams -
Parameters:

- p_areaEventType -
- p_locationEstimate -
- p_repeatedReportingParams -
- p_start -
- p_stop -
- p_geographicTargetAreaList -
- p_areaIdLists -

m_reportingModeBatch

    template ReportingMode m_reportingModeBatch(template BatchRepConditions p_batchRepConditions,
                                                template BatchRepType p_batchRepType ) :={
        repMode := batch,
        batchRepConditions := p_batchRepConditions,
        batchRepType:= p_batchRepType
    }

Declared in group suplMessagesParameterGroup
Returns: ReportingMode -
Parameters:

- p_batchRepConditions -
- p_batchRepType -

m_reportingModeQuasiReal

    template ReportingMode m_reportingModeQuasiReal(template BatchRepConditions p_batchRepConditions,
                                       template BatchRepType p_batchRepType ) :={
       repMode := quasirealtime,
       batchRepConditions := p_batchRepConditions,
       batchRepType:= p_batchRepType
       }

Declared in group suplMessagesParameterGroup
Returns: ReportingMode -
Parameters:

- p_batchRepConditions -
- p_batchRepType -

m_batchRepConditionsByInterval

    template BatchRepConditions m_batchRepConditionsByInterval(template _0BatchRepConditions p_num_interval)
                              := {
    num_interval := p_num_interval
    }

Declared in group suplMessagesParameterGroup
Returns: BatchRepConditions -
Parameters:

- p_num_interval -

m_batchRepConditionsByMinutes

    template BatchRepConditions m_batchRepConditionsByMinutes(template _0BatchRepConditions p_num_minutes)
                                     := {
    num_minutes := p_num_minutes
    }

Declared in group suplMessagesParameterGroup
Returns: BatchRepConditions -
Parameters:

- p_num_minutes -

m_batchRepConditionsByEndofsession

    template BatchRepConditions m_batchRepConditionsByEndofsession() := {
    endofsession := NULL
    }

Declared in group suplMessagesParameterGroup
Returns: BatchRepConditions -

m_batchRepType

    template BatchRepType m_batchRepType(template boolean p_reportPosition,
                 template boolean p_reportMeasurements,
                                                template boolean p_intermediateReports,
                                                template boolean p_discardOldest) := {
    reportPosition := p_reportPosition,
    reportMeasurements := p_reportMeasurements,
    intermediateReports := p_intermediateReports,
    discardOldest := p_discardOldest
    }

Declared in group suplMessagesParameterGroup
Returns: BatchRepType -
Parameters:

- p_reportPosition -
- p_reportMeasurements -
- p_intermediateReports -
- p_discardOldest -

mw_posTechICS

    template PosTechnology mw_posTechICS := mw_posTech(
    ics_AGPSSETassisted_Network_initiated,
    ics_AGPSSETbased_Network_initiated,
    ics_autonomousGPS_Network_initiated,
    ics_aFLT,
    ics_eCID_Network_initiated,
    ics_eOTD,
    ics_oTDOA,
    ics_AGANSSSETassisted_GLONASS_Network_initiated,
    ics_AGANSSSETbased_GLONASS_Network_initiated,
    ics_autonomousGANSS_Network_initiated);

Declared in group suplMessagesParameterGroup

mw_posTechICSV1

    template PosTechnology mw_posTechICSV1 := mw_posTechV1(
    ics_AGPSSETassisted_Network_initiated,
    ics_AGPSSETbased_Network_initiated,
    ics_autonomousGPS_Network_initiated,
    ics_aFLT,
    ics_eCID_Network_initiated,
    ics_eOTD,
    ics_oTDOA);

Declared in group suplMessagesParameterGroup

mw_posTech

    template PosTechnology
    mw_posTech(template boolean p_agpsSETassisted,
               template boolean p_agpsSETBased,
               template boolean p_autonomousGPS, template boolean p_aFLT,
               template boolean p_eCID, template boolean p_eOTD,
               template boolean p_oTDOA,
               template boolean p_agnssSETassisted,
               template boolean p_agnssSETbased,
               template boolean p_autonomousGNSS) := {
        agpsSETassisted := p_agpsSETassisted,
        agpsSETBased := p_agpsSETBased,
        autonomousGPS := p_autonomousGPS,
        aFLT := p_aFLT,
        eCID := p_eCID,
        eOTD := p_eOTD,
        oTDOA := p_oTDOA,
        ver2_PosTechnology_extension := {
            gANSSPositionMethods := {
                {
                    ganssId := ?,
                    ganssSBASid := omit,
                    gANSSPositioningMethodTypes := {
                        setAssisted := p_agnssSETassisted,
                        setBased := p_agnssSETbased,
                        autonomous := p_autonomousGNSS
                    },
                    gANSSSignals := ?
                }
            }
        }ifpresent
    }

Declared in group suplMessagesParameterGroup
Returns: PosTechnology -
Parameters:

- p_agpsSETassisted -
- p_agpsSETBased -
- p_autonomousGPS -
- p_aFLT -
- p_eCID -
- p_eOTD -
- p_oTDOA -
- p_agnssSETassisted -
- p_agnssSETbased -
- p_autonomousGNSS -

mw_posTechV1

    template PosTechnology
    mw_posTechV1(template boolean p_agpsSETassisted,
       template boolean p_agpsSETBased,
       template boolean p_autonomousGPS, template boolean p_aFLT,
       template boolean p_eCID, template boolean p_eOTD,
       template boolean p_oTDOA) := {
    agpsSETassisted := p_agpsSETassisted,
    agpsSETBased := p_agpsSETBased,
    autonomousGPS := p_autonomousGPS,
    aFLT := p_aFLT,
    eCID := p_eCID,
    eOTD := p_eOTD,
    oTDOA := p_oTDOA,
    ver2_PosTechnology_extension := omit
    }

Declared in group suplMessagesParameterGroup
Returns: PosTechnology -
Parameters:

- p_agpsSETassisted -
- p_agpsSETBased -
- p_autonomousGPS -
- p_aFLT -
- p_eCID -
- p_eOTD -
- p_oTDOA -

m_areaIdList

    template AreaIdList m_areaIdList(template AreaId p_areaId) := {
        areaIdSet := {p_areaId},
        areaIdSetType := omit,
        geoAreaMappingList := omit
    }

Declared in group suplMessagesParameterGroup
Returns: AreaIdList -
Parameters:

- p_areaId -

mw_setCapabilities

    template SETCapabilities
    mw_setCapabilities(template ReportingCap p_reportingCap) := {
        posTechnology := mw_posTechICS,
        prefMethod := ?,
        posProtocol := ?,
        ver2_SETCapabilities_extension := {
            serviceCapabilities :=
                {
                    servicesSupported := ?,
                    reportingCapabilities := p_reportingCap,
                    eventTriggerCapabilities := *,
                    sessionCapabilities := ?
                }
                 ifpresent
        }
    }

Declared in group suplMessagesParameterGroup
Returns: SETCapabilities -
Parameters:

- p_reportingCap -

mw_setCapabilitiesExt

    template SETCapabilities
    mw_setCapabilitiesExt(
    template ServicesSupported p_serviceSupported,
    template ReportingCap p_reportingCap,
    template EventTriggerCapabilities p_eventTriggerCap) := {
     posTechnology := mw_posTechICS,
     prefMethod := ?,
     posProtocol := ?,
     ver2_SETCapabilities_extension := {
     serviceCapabilities :=
     {
     servicesSupported := p_serviceSupported,
     reportingCapabilities := p_reportingCap,
     eventTriggerCapabilities := p_eventTriggerCap,
     sessionCapabilities := ?
     }
      }
    }

Declared in group suplMessagesParameterGroup
Returns: SETCapabilities -
Parameters:

- p_serviceSupported -
- p_reportingCap -
- p_eventTriggerCap -

m_methodType_msAssistedV5

    template RRLP_CommonTypes.MethodType
    m_methodType_msAssistedV5(template RRLP_CommonTypes.AccuracyOpt p_msAssisted) := {
    methodTypeV5 :={
    msAssisted := p_msAssisted.accuracyOptV5
    }
    }

Declared in group suplMessagesParameterGroup
TODO: Add description
Returns: MethodType -
Parameters:

- p_msAssisted -

m_methodType_msAssistedV10

    template RRLP_CommonTypes.MethodType
    m_methodType_msAssistedV10(template RRLP_CommonTypes.AccuracyOpt p_msAssisted) := {
    methodTypeV10 :={
    msAssisted := p_msAssisted.accuracyOptV10
    }
    }

Declared in group suplMessagesParameterGroup
TODO: Add description
Returns: MethodType -
Parameters:

- p_msAssisted -

m_methodType_msAssitedPrefV5

    template RRLP_CommonTypes.MethodType
    m_methodType_msAssitedPrefV5(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV5 :={
    msAssistedPref := p_accuracy.accuracyV5
    }
    }

Declared in group suplMessagesParameterGroup
MS-AssistedPref Method Type
Returns: MethodType -
Parameters:

- p_accuracy -

m_methodType_msAssitedPrefV10

    template RRLP_CommonTypes.MethodType
    m_methodType_msAssitedPrefV10(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV10 :={
    msAssistedPref := p_accuracy.accuracyV10
    }
    }

Declared in group suplMessagesParameterGroup
MS-AssistedPref Method Type
Returns: MethodType -
Parameters:

- p_accuracy -

m_accuracyOpt_omittedV5

    template RRLP_CommonTypes.AccuracyOpt m_accuracyOpt_omittedV5 := {
    accuracyOptV5 :={
    accuracy := omit
    }
    }

Declared in group suplMessagesParameterGroup
TODO: Add description

m_accuracyOpt_omittedV10

    template RRLP_CommonTypes.AccuracyOpt m_accuracyOpt_omittedV10 := {
    accuracyOptV10 :={
    accuracy := omit
    }
    }

Declared in group suplMessagesParameterGroup
TODO: Add description

m_methodType_msBasedV5

    template RRLP_CommonTypes.MethodType
    m_methodType_msBasedV5(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV5 := {
    msBased := p_accuracy.accuracyV5
    }
    }

Declared in group suplMessagesParameterGroup
Returns: MethodType -
Parameters:

- p_accuracy -

m_methodType_msBasedV10

    template RRLP_CommonTypes.MethodType
    m_methodType_msBasedV10(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV10 := {
    msBased := p_accuracy.accuracyV10
    }
    }

Declared in group suplMessagesParameterGroup
Returns: MethodType -
Parameters:

- p_accuracy -

m_methodType_msBasedPrefV5

    template RRLP_CommonTypes.MethodType
    m_methodType_msBasedPrefV5(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV5 := {
     msBasedPref := p_accuracy.accuracyV5
    }
    }

Declared in group suplMessagesParameterGroup
MS-BasedPref Method Type
Returns: MethodType -
Parameters:

- p_accuracy -

m_methodType_msBasedPrefV10

    template RRLP_CommonTypes.MethodType
    m_methodType_msBasedPrefV10(template(present) RRLP_CommonTypes.Accuracy p_accuracy) := {
    methodTypeV10 := {
     msBasedPref := p_accuracy.accuracyV10
    }
    }

Declared in group suplMessagesParameterGroup
MS-BasedPref Method Type
Returns: MethodType -
Parameters:

- p_accuracy -

m_areaIdLists_one_areaId

    template _0AreaEventParams1
    m_areaIdLists_one_areaId(template(present) AreaId p_areaId) := {
    m_areaIdList(p_areaId)
    }

Declared in group suplMessagesParameterGroup
TODO: Add description
Returns: _0AreaEventParams1 -
Parameters:

- p_areaId -

m_areaId_gsm_cellId

    template AreaId m_areaId_gsm_cellId(template _0GSMAreaId0 p_cellId) := {
        gSMAreaId := m_gsmAreaId_cellId(p_cellId)
    }

Declared in group suplMessagesParameterGroup
Builds an Area Id message instance from a GSM cell ID
Returns: AreaId -
Parameters:

- p_cellId -

m_areaId_wcdma_cellId

    template AreaId m_areaId_wcdma_cellId(template _0WCDMAAreaId0 p_cellId) := {
        wCDMAAreaId := m_wcdmaAreaId_cellId(p_cellId)
    }

Declared in group suplMessagesParameterGroup
Builds an Area Id message instance from a WCDMA cell ID
Returns: AreaId -
Parameters:

- p_cellId -

m_areaId_lte_cellId

    template AreaId m_areaId_lte_cellId(template _0LTEAreaId1 p_cellId) := {
    lTEAreaId := m_lteAreaId_cellId(p_cellId)
    }

Declared in group suplMessagesParameterGroup
Builds an Area Id message instance from a LTE cell ID
Returns: AreaId -
Parameters:

- p_cellId -

m_areaId_cdma_cellId

    template AreaId m_areaId_cdma_cellId(template _0CDMAAreaId1 p_cellId) := {
    cDMAAreaId :=m_cdmaAreaId_cellId (p_cellId)
    }

Declared in group suplMessagesParameterGroup
Builds an Area Id message instance from a CDMA cell ID
Returns: AreaId -
Parameters:

- p_cellId -

m_areaId_hrpd_cellId

    template AreaId m_areaId_hrpd_cellId(template _0HRPDAreaId p_cellId) := {
    hRPDAreaId := m_hrpdAreaId_cellId(p_cellId)
    }

Declared in group suplMessagesParameterGroup
Builds an Area Id message instance from a hRPD cell ID
Returns: AreaId -
Parameters:

- p_cellId -

m_gsmAreaId_cellId

    template GSMAreaId m_gsmAreaId_cellId(template _0GSMAreaId2 p_cellId) := {
        refMCC := omit, refMNC := omit, refLAC := omit, refCI := p_cellId
    }

Declared in group suplMessagesParameterGroup
GSM area ID from cell ID
Returns: GSMAreaId -
Parameters:

- p_cellId -

m_wcdmaAreaId_cellId

    template WCDMAAreaId m_wcdmaAreaId_cellId(template _0WCDMAAreaId2 p_cellId) := {
        refMCC := omit, refMNC := omit, refLAC := omit, refUC := p_cellId
    }

Declared in group suplMessagesParameterGroup
WCDMA Area ID from cell ID
Returns: WCDMAAreaId -
Parameters:

- p_cellId -

m_lteAreaId_cellId

    template LTEAreaId m_lteAreaId_cellId(template _0LTEAreaId1 p_cellId) := {
    refMCC := omit, refMNC := omit, refCI := p_cellId
    }

Declared in group suplMessagesParameterGroup
LTE Area ID from cell ID
Returns: LTEAreaId -
Parameters:

- p_cellId -

m_cdmaAreaId_cellId

    template CDMAAreaId m_cdmaAreaId_cellId(template _0CDMAAreaId1 p_cellId) := {
    refSID := omit, refNID := omit, refBASEID := p_cellId
    }

Declared in group suplMessagesParameterGroup
CDMA Area ID from cell ID
Returns: CDMAAreaId -
Parameters:

- p_cellId -

m_hrpdAreaId_cellId

    template HRPDAreaId m_hrpdAreaId_cellId(template _0HRPDAreaId p_cellId) := {
    refSECTORID := p_cellId
    }

Declared in group suplMessagesParameterGroup
hRPD Area ID from cell ID
Returns: HRPDAreaId -
Parameters:

- p_cellId -

m_BasicProtectionLevel

    template ProtectionLevel m_BasicProtectionLevel(_0BasicProtectionParams p_keyIdentifier, _0BasicProtectionParams0 p_basicReplyCounter, _0BasicProtectionParams1 p_basicMAC) := {
    protlevel := basicProtection,
    basicProtectionParams := {p_keyIdentifier, p_basicReplyCounter, p_basicMAC}
    }

Declared in group suplMessagesParameterGroup
basic ProtectionLevel from SUPL INIT
Returns: ProtectionLevel -
Parameters:

- p_keyIdentifier -
- p_basicReplyCounter -
- p_basicMAC -

m_ProtectionParamsDefault

    template BasicProtectionParams m_ProtectionParamsDefault := {
    keyIdentifier := m_keyIdentifier,
    basicReplayCounter := m_basicReplayCounter,
    basicMAC := m_basicMAC_zero
    }

Declared in group suplMessagesParameterGroup

m_ProtectionLevel

    template ProtectionLevel m_ProtectionLevel(ProtLevel p_protectionLevel, template BasicProtectionParams p_basicProtectionParams) := {
    protlevel := p_protectionLevel,
    basicProtectionParams := p_basicProtectionParams
    }

Declared in group suplMessagesParameterGroup
Returns: ProtectionLevel -
Parameters:

- p_protectionLevel -
- p_basicProtectionParams -

m_keyIdentifier

    template _0BasicProtectionParams m_keyIdentifier := '0001020304050607'O;

Declared in group suplMessagesParameterGroup

m_keyIdentifier_incorrect

    template _0BasicProtectionParams m_keyIdentifier_incorrect := '0000000000000000'O;

Declared in group suplMessagesParameterGroup

m_basicReplayCounter

    template _0BasicProtectionParams0 m_basicReplayCounter := 1;

Declared in group suplMessagesParameterGroup

m_basicMAC

    template _0BasicProtectionParams1 m_basicMAC := '01010101010101010101010101010101'B;

Declared in group suplMessagesParameterGroup

m_basicMAC_zero

    template _0BasicProtectionParams1 m_basicMAC_zero := '00000000000000000000000000000000'B;

Declared in group suplMessagesParameterGroup

m_SLPAddressFQDN

    template SLPAddress m_SLPAddressFQDN (FQDN p_fQDN) := {
      fQDN:= p_fQDN
    }

Declared in group suplMessagesParameterGroup
Returns: SLPAddress -
Parameters:

- p_fQDN -

m_ESLPAddressIP

    template SLPAddress m_ESLPAddressIP := {
      iPAddress:= f_SLPAddressIP()
    }

Declared in group suplMessagesParameterGroup

m_notificationEmergency

    template Notification m_notificationEmergency(NotificationType p_type) := {
    notificationType := p_type,
    encodingType := omit,
    requestorId := omit,
    requestorIdType := omit,
    clientName := omit,
    clientNameType := omit,
    ver2_Notification_extension := {emergencyCallLocation := NULL}
    }

Declared in group suplMessagesParameterGroup
Returns: Notification -
Parameters:

- p_type -

m_setTriggerServiceSupported

    template ServicesSupported m_setTriggerServiceSupported(template boolean p_PeriodicTrigger, template boolean p_AreaEventTrigger ) := {
    periodicTrigger := p_PeriodicTrigger,
    areaEventTrigger := p_AreaEventTrigger
    }

Declared in group suplMessagesParameterGroup
Returns: ServicesSupported -
Parameters:

- p_PeriodicTrigger -
- p_AreaEventTrigger -

m_setEventTriggerCap

    template EventTriggerCapabilities m_setEventTriggerCap(template boolean p_EllipticalArea, template boolean p_PolygonArea, template _0EventTriggerCapabilities p_MaxNumGeoSp, template _0EventTriggerCapabilities0 p_MaxAreaIdListSp, template _0EventTriggerCapabilities1 p_MaxAreaIdPerList ) := {
    geoAreaShapesSupported:=
    {
          ellipticalArea := p_EllipticalArea,
    polygonArea := p_PolygonArea
    },
    maxNumGeoAreaSupported    := p_MaxNumGeoSp,
    maxAreaIdListSupported    := p_MaxAreaIdListSp,
    maxAreaIdSupportedPerList    := p_MaxAreaIdPerList
    }

Declared in group suplMessagesParameterGroup
Returns: EventTriggerCapabilities -
Parameters:

- p_EllipticalArea -
- p_PolygonArea -
- p_MaxNumGeoSp -
- p_MaxAreaIdListSp -
- p_MaxAreaIdPerList -

© Copyright Testing Technologies IST GmbH 2012