OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module SUPL_Parameters

Import Declarations:

- SUPL_CommonSteps
  all
- SUPL_TypeDefinitions
  all
- BSF_XML_TypeDefinitions
  all
- SUPL_Configuration
  all
- LibCommon_DataStrings
  all
- SUPLTypes
  all

Groups:

- SUPL_IXIT_Items

- SLP
- TransportSMS
- PositioningMethods
- Timer
- Securtiy
- SIM
- Auth
- SET
- notificatioin

Modulepars Summary
ics_TestAutomation | (boolean) If set, Tester sends MMI commands over MMI port
ixit_GpsDataAutomation | (GPSAutomationType) Tester sends GPS commands to MMI or Automation Interface
ics_NetworkInitiated |
ics_SETInitiated |
ixit_H_SLP_IP_TYPE | (slpSessionIdFormat) IP address type for SLP
ixit_H_SLP_FQDN | (charstring) FQDN for SLP
ixit_H_SLP_IPv4 | (charstring) IPv4 address for SLP
ixit_H_SLP_IPv6 | (charstring) IPv6 address for SLP
ixit_BSF_FQDN | (charstring) BSF FQDN
ixit_BSF_enabled | (boolean) enables BSF simulation.
ics_MT_SMS |
ics_WapPush |
ixit_MTTransport | (MTTransport) Transport channel for SUPL INIT message
ixit_PositioningProtocol | (PositioningProtocol) Positioning Protocol to be used
ixit_LPP_Version | (LPP_Version_Enum) LPP version to be used
ixit_RRLP_Version | (RRLP_Version_Enum) RRLP version to be used
ics_AGPSSETassisted_SET_initiated | (boolean) UE supports A-GPS SET assited Positioning Method (SET initiated)
ics_AGPSSETassisted_Network_initiated | UE supports A-GPS SET assited Positioning Method (Network initiated)
ics_AGPSSETbased_SET_initiated | (boolean) UE supports A-GPS SET based Positioning Method (SET initiated)
ics_AGPSSETbased_Network_initiated | (boolean) UE supports A-GPS SET based Positioning Method (Network initiated)
ics_autonomousGPS_SET_initiated |
ics_autonomousGPS_Network_initiated | (boolean) UE supports autonomous GPS Positioning Method in Network initiated session
ics_aFLT | (boolean) UE supports aFLT Positioning Method
ics_eCID_SET_initiated |
ics_eCID_Network_initiated | (boolean) UE supports eCID Positioning Method (Network initiated
ics_eOTD | (boolean) UE supports eOTD Positioning Method
ics_oTDOA | (boolean) UE supports oTDOA Positioning Method
ixit_timer_UT1 | (integer) value of Timer UT1, default = 10s
ixit_timer_UT2 | (integer) value of Timer UT2, default = 10s
ixit_timer_UT3 | (integer) value of Timer UT3, default = 10s
ixit_timer_UT4 |
ixit_timer_UT5 |
ixit_verification_timeout |
ixit_TLS_Version | (TlsVersionConfig) used TLS Version.
ixit_CipherSuite | (CipherSuites) used cipher suite
ixit_CertificationVersion | (CertificateVersions) used certificate version
ics_PSK_TLS | (bollean) SET supports TLS/PSK
ixit_PSK_remote_IP | (cahrstring) SET PSK Remote IP
ixit_OrganizationOctet | (octetstring) sed for PSK generation in Value NAF_Id
ixit_GBA_mode | (GBAType) Specifies the supperted GBA algorithm in the DUT
ixit_VER_HMACHash | (HMACHash) used HMAC hash function for calculating VER.
ixit_IMPI_ISIM | (charstring) IMPI for I-SIM
ixit_IMPI_USIM | (charstring) IMPI for U-SIM
ixit_usedSIM | (Sims) SET has following SIM
ixit_AuthAMF | (Bit16) Authentication Management Field (16 bits)
ixit_AuthK | (Bit128) Authentication Key (128 bits)
ixit_AuthN | (integer) min 31, max 127 (TS 34_108 cl 8_1_2) default = 127
ixit_AuthRAND | (Bit128) Authentication / Random challenge (128 bits)
ics_SET_supportSLPInitPosReq |
ics_notification |
ics_notification_currentLocation |
ics_UE_support_formatIndicator_logicalName |
ics_UE_support_formatIndicator_eMailAddress |
ics_UE_support_formatIndicator_MSISDN |
ics_UE_support_formatIndicator_URL |
ics_UE_support_formatIndicator_SIPURL |
ics_UE_support_formatIndicator_MIN |
ics_UE_support_formatIndicator_MDN |
ics_UE_support_formatIndicator_IMSPublicIdentity |
ics_charEncoding_UCS2 |
ics_charEncoding_UTF8 |
ics_charEncoding_GSM |

## Details

ics_TestAutomation

    boolean ics_TestAutomation := false

Declared in group SUPL_IXIT_Items
(boolean) If set, Tester sends MMI commands over MMI port

ixit_GpsDataAutomation

    GPSAutomationType ixit_GpsDataAutomation := OFF

Declared in group SUPL_IXIT_Items
(GPSAutomationType) Tester sends GPS commands to MMI or Automation Interface

ics_NetworkInitiated

    boolean ics_NetworkInitiated := true

Declared in group SUPL_IXIT_Items

ics_SETInitiated

    boolean ics_SETInitiated := true

Declared in group SUPL_IXIT_Items

ixit_H_SLP_IP_TYPE

    slpSessionIdFormat ixit_H_SLP_IP_TYPE := slpSessionIdIPv4

Declared in group SUPL_IXIT_Items.SLP
(slpSessionIdFormat) IP address type for SLP

ixit_H_SLP_FQDN

    charstring ixit_H_SLP_FQDN := "www.openmobilealliance.com"

Declared in group SUPL_IXIT_Items.SLP
(charstring) FQDN for SLP

ixit_H_SLP_IPv4

    charstring ixit_H_SLP_IPv4 := "192.168.0.35"

Declared in group SUPL_IXIT_Items.SLP
(charstring) IPv4 address for SLP

ixit_H_SLP_IPv6

    charstring ixit_H_SLP_IPv6 := "fd00:0:20:1:0:0:0:4"

Declared in group SUPL_IXIT_Items.SLP
(charstring) IPv6 address for SLP

ixit_BSF_FQDN

    charstring ixit_BSF_FQDN := "bsf.mnc001.mcc001.pub.3gppnetwork.org"

Declared in group SUPL_IXIT_Items.SLP
(charstring) BSF FQDN

ixit_BSF_enabled

    boolean ixit_BSF_enabled := false

Declared in group SUPL_IXIT_Items.SLP
(boolean) enables BSF simulation.

ics_MT_SMS

    boolean ics_MT_SMS := true

Declared in group SUPL_IXIT_Items.TransportSMS

ics_WapPush

    boolean ics_WapPush := true

Declared in group SUPL_IXIT_Items.TransportSMS

ixit_MTTransport

    MTTransport ixit_MTTransport := MT_SMS

Declared in group SUPL_IXIT_Items.TransportSMS
(MTTransport) Transport channel for SUPL INIT message

ixit_PositioningProtocol

    PositioningProtocol ixit_PositioningProtocol := RRLP

Declared in group SUPL_IXIT_Items.PositioningMethods
(PositioningProtocol) Positioning Protocol to be used

ixit_LPP_Version

    LPP_Version_Enum ixit_LPP_Version := e_LPP_V10

Declared in group SUPL_IXIT_Items.PositioningMethods
(LPP_Version_Enum) LPP version to be used

ixit_RRLP_Version

    RRLP_Version_Enum ixit_RRLP_Version := e_RRLP_V5

Declared in group SUPL_IXIT_Items.PositioningMethods
(RRLP_Version_Enum) RRLP version to be used

ics_AGPSSETassisted_SET_initiated

    boolean ics_AGPSSETassisted_SET_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports A-GPS SET assited Positioning Method (SET initiated)

ics_AGPSSETassisted_Network_initiated

    boolean ics_AGPSSETassisted_Network_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
UE supports A-GPS SET assited Positioning Method (Network initiated)

ics_AGPSSETbased_SET_initiated

    boolean ics_AGPSSETbased_SET_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports A-GPS SET based Positioning Method (SET initiated)

ics_AGPSSETbased_Network_initiated

    boolean ics_AGPSSETbased_Network_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports A-GPS SET based Positioning Method (Network initiated)

ics_autonomousGPS_SET_initiated

    boolean ics_autonomousGPS_SET_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods

ics_autonomousGPS_Network_initiated

    boolean ics_autonomousGPS_Network_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports autonomous GPS Positioning Method in Network initiated session

ics_aFLT

    boolean ics_aFLT := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports aFLT Positioning Method

ics_eCID_SET_initiated

    boolean ics_eCID_SET_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods

ics_eCID_Network_initiated

    boolean ics_eCID_Network_initiated := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports eCID Positioning Method (Network initiated

ics_eOTD

    boolean ics_eOTD := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports eOTD Positioning Method

ics_oTDOA

    boolean ics_oTDOA := true

Declared in group SUPL_IXIT_Items.PositioningMethods
(boolean) UE supports oTDOA Positioning Method

ixit_timer_UT1

    integer ixit_timer_UT1 := 10

Declared in group SUPL_IXIT_Items.Timer
(integer) value of Timer UT1, default = 10s

ixit_timer_UT2

    integer ixit_timer_UT2 := 10

Declared in group SUPL_IXIT_Items.Timer
(integer) value of Timer UT2, default = 10s

ixit_timer_UT3

    integer ixit_timer_UT3 := 10

Declared in group SUPL_IXIT_Items.Timer
(integer) value of Timer UT3, default = 10s

ixit_timer_UT4

    integer ixit_timer_UT4 := 10

Declared in group SUPL_IXIT_Items.Timer

ixit_timer_UT5

    integer ixit_timer_UT5 := 10

Declared in group SUPL_IXIT_Items.Timer

ixit_verification_timeout

    integer ixit_verification_timeout := 40

Declared in group SUPL_IXIT_Items.Timer

ixit_TLS_Version

    TlsVersionConfig ixit_TLS_Version := TLS1_1

Declared in group SUPL_IXIT_Items.Securtiy
(TlsVersionConfig) used TLS Version. For Compliance with SUPL 2.0 TS, this ixit MUST be set to TLS 1.1

ixit_CipherSuite

    CipherSuites ixit_CipherSuite := TLS_RSA_WITH_AES_128_CBC_SHA

Declared in group SUPL_IXIT_Items.Securtiy
(CipherSuites) used cipher suite

ixit_CertificationVersion

    CertificateVersions ixit_CertificationVersion := X509v1

Declared in group SUPL_IXIT_Items.Securtiy
(CertificateVersions) used certificate version

ics_PSK_TLS

    boolean ics_PSK_TLS := false

Declared in group SUPL_IXIT_Items.Securtiy
(bollean) SET supports TLS/PSK

ixit_PSK_remote_IP

    charstring ixit_PSK_remote_IP := "127.0.0.1"

Declared in group SUPL_IXIT_Items.Securtiy
(cahrstring) SET PSK Remote IP

ixit_OrganizationOctet

    octetstring ixit_OrganizationOctet := '01'O

Declared in group SUPL_IXIT_Items.Securtiy
(octetstring) sed for PSK generation in Value NAF_Id

ixit_GBA_mode

    GBAType ixit_GBA_mode := e_gba_u

Declared in group SUPL_IXIT_Items.Securtiy
(GBAType) Specifies the supperted GBA algorithm in the DUT

ixit_VER_HMACHash

    HMACHash ixit_VER_HMACHash := SHA256

Declared in group SUPL_IXIT_Items.Securtiy
(HMACHash) used HMAC hash function for calculating VER. For Compliance with SUPL 2.0 TS, this ixit MUST be set to SHA256

ixit_IMPI_ISIM

    charstring ixit_IMPI_ISIM := "user1-private@operator.com"

Declared in group SUPL_IXIT_Items.SIM
(charstring) IMPI for I-SIM

ixit_IMPI_USIM

    charstring ixit_IMPI_USIM := "001010123456063@ims.mnc001.mcc001.pub.3gppnetwork.org"

Declared in group SUPL_IXIT_Items.SIM
(charstring) IMPI for U-SIM

ixit_usedSIM

    Sims ixit_usedSIM := USIM

Declared in group SUPL_IXIT_Items.SIM
(Sims) SET has following SIM

ixit_AuthAMF

    Bit16 ixit_AuthAMF := '0000000000000000'B

Declared in group SUPL_IXIT_Items.Auth
(Bit16) Authentication Management Field (16 bits)

ixit_AuthK

    Bit128 ixit_AuthK :=
    '00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111'B

Declared in group SUPL_IXIT_Items.Auth
(Bit128) Authentication Key (128 bits)

ixit_AuthN

    integer ixit_AuthN := 127

Declared in group SUPL_IXIT_Items.Auth
(integer) min 31, max 127 (TS 34_108 cl 8_1_2) default = 127

ixit_AuthRAND

    Bit128 ixit_AuthRAND :=
    '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B

Declared in group SUPL_IXIT_Items.Auth
(Bit128) Authentication / Random challenge (128 bits)

ics_SET_supportSLPInitPosReq

    boolean ics_SET_supportSLPInitPosReq := true

Declared in group SUPL_IXIT_Items.SET

ics_notification

    boolean ics_notification := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_notification_currentLocation

    boolean ics_notification_currentLocation := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_logicalName

    boolean ics_UE_support_formatIndicator_logicalName := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_eMailAddress

    boolean ics_UE_support_formatIndicator_eMailAddress := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_MSISDN

    boolean ics_UE_support_formatIndicator_MSISDN := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_URL

    boolean ics_UE_support_formatIndicator_URL := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_SIPURL

    boolean ics_UE_support_formatIndicator_SIPURL := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_MIN

    boolean ics_UE_support_formatIndicator_MIN := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_MDN

    boolean ics_UE_support_formatIndicator_MDN := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_UE_support_formatIndicator_IMSPublicIdentity

    boolean ics_UE_support_formatIndicator_IMSPublicIdentity := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_charEncoding_UCS2

    boolean ics_charEncoding_UCS2 := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_charEncoding_UTF8

    boolean ics_charEncoding_UTF8 := true

Declared in group SUPL_IXIT_Items.notificatioin

ics_charEncoding_GSM

    boolean ics_charEncoding_GSM := true

Declared in group SUPL_IXIT_Items.notificatioin

© Copyright Testing Technologies IST GmbH 2012