OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_11x

Declared in module SUPL_V2_SET_INITIATED_Tests
Subgroups: TC_110

Test cases Summary
TC_110_1 |
TC_110_2 |
TC_110_3 |
TC_110_4 |
TC_110_5 |
TC_110_7 | To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_110_9 | To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
TC_110_10 | To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
TC_110_11_1 | To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_11_2 | To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_12_1 | To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_12_2 | To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_13 | To test SET correctly actions single session Positioning method - Test 13: OTDOA

## Details

TC_110_1

    testcase TC_110_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_2

    testcase TC_110_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_3

    testcase TC_110_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_4

    testcase TC_110_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_5

    testcase TC_110_5() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_7

    testcase TC_110_7() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
Purpose: SUPL-2.0-con-110-7 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGANSSSETassisted_GLONASS_SET_initiated Test Procedure : Test 7: A-GANSS SET assisted –GLONASS [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: A-GNSS SET assisted only GNSS Positioning Technology set to: GLONASS 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 5. Do nothing (only Test 4 and Test 5) 6. A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. 7. Do nothing (only Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2) 8. send SUPL END with: Position set to a realistic position for the SET. 9. The SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_9

    testcase TC_110_9() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
Purpose: SUPL-2.0-con-110-9 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGANSSSETbased_GLONASS_SET_initiated Test Procedure : Test 9: A-GANSS SET based –GLONASS [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. 7. Test 9: send SUPL END 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_10

    testcase TC_110_10() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
Purpose: SUPL-2.0-con-110-10 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_autonomousGANSS_SET_initiated AND ixit_gANSS Test Procedure : Test 10: Autonomous GANSS [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_11_1

    testcase TC_110_11_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only. Otherwise A-GANSS SET based only
Purpose: SUPL-2.0-con-110-11_1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGNSSSETassisted_preferred AND ixit_gANSS Test Procedure : Test 11: SET declares A-GNSS SET-assisted Preferred method [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. Test 11: If A-GPS is supported by the SET then A-GPS SET based shall be used. Otherwise A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_11_2

    testcase TC_110_11_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only. Otherwise A-GANSS SET based only
Purpose: SUPL-2.0-con-110-11_1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGNSSSETassisted_preferred AND ixit_gANSS Test Procedure : Test 11: SET declares A-GNSS SET-assisted Preferred method [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. Test 11: If A-GPS is supported by the SET then A-GPS SET based shall be used. Otherwise A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_12_1

    testcase TC_110_12_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
Purpose: SUPL-2.0-con-110-12-1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ( (ics_AGANSSSETassisted_Galileo_SET_initiated AND ics_AGANSSSETbased_Galileo_SET_initiated) OR (ics_AGANSSSETassisted_GLONASS_SET_initiated AND ics_AGANSSSETbased_GLONASS_SET_initiated)) AND (ixit_gANSS.galileo or ixit_gANSS.gloneass) Test Procedure : Test 12: A-GANSS Preferred methods [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 1: A-GANSS SET assisted is used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 1: A-GANSS SET assisted shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_12_2

    testcase TC_110_12_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
Purpose: SUPL-2.0-con-110-12-2 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ( (ics_AGANSSSETassisted_Galileo_SET_initiated AND ics_AGANSSSETbased_Galileo_SET_initiated) OR (ics_AGANSSSETassisted_GLONASS_SET_initiated AND ics_AGANSSSETbased_GLONASS_SET_initiated)) AND ixit_gANSS Test Procedure : Test 12: A-GANSS Preferred methods [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based is used, where in both cases the GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_13

    testcase TC_110_13() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 13: OTDOA
Purpose: SUPL-2.0-con-110-13 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O, ULP-PRO-C-020 Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_OTDOA_SET_initiated Test Procedure : Test 13: OTDOA [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based is used, where in both cases the GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 8. Test 1, Test 6, Test 7, Test 12 and Test 13: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. Test 13: OTDOA shall be used.
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012