OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_14x.TC_140

Declared in module SUPL_V2_SET_INITIATED_Tests

Test cases Summary
TC_140_1 |
TC_140_2 | To test SET correctly actions timer UT1 - Test 2: Triggered Session

## Details

TC_140_1

    testcase TC_140_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
Runs On: SUPLComponent
System: SystemInterfaces

TC_140_2

    testcase TC_140_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
To test SET correctly actions timer UT1 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-140-2 TP version: Test Case Id : SUPL-2.0-con-140 Test Object : Client Test Case Description : To test SET correctly actions timer UT1 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 2: Triggered session [Includes Optional Features] 6. Start a SI Periodic Triggered Location Session, or a SI Area Event Triggered Location session if Periodic Location sessions are not supported in the SET. 7. The SET sends SUPL TRIGGERED START 8. Do not respond 9. After timer UT1 expires (depending on ixit_timer_UT1) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 10. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : 1. At step 4 and step 9 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 5 and step 10 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012