OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group externalFunctionGroup

Declared in module SUPL_V2_CommonSteps

Functions Summary
fx_gpsPositionCalculation | calculates a Position value based on the last received SUPL POS
fx_positionIsIn | calculation if a Position estimate value is located within the geographic area
fx_GadLatitude | convertion of latitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
fx_GadLongitude | convertion of logitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]

## Details

fx_gpsPositionCalculation

    external function fx_gpsPositionCalculation(in ULP_PDU p_supl_pos, in integer p_gpsTOW, in GNSSScenario p_GNSSScenario, in integer p_rrlpVersion, out SUPLTypes.PositionEstimate p_PositionEstimate) return boolean;

Declared in group externalFunctionGroup
calculates a Position value based on the last received SUPL POS
Returns: boolean - Position of SET
Parameters:

- p_supl_pos -
- p_gpsTOW -
- p_GNSSScenario -
- p_rrlpVersion -
- p_PositionEstimate -

fx_positionIsIn

    external function fx_positionIsIn(in SUPLTypes.PositionEstimate p_positionEstimate,
    in GeographicTargetArea p_geographicTargetArea) return boolean;

Declared in group externalFunctionGroup
calculation if a Position estimate value is located within the geographic area
Returns: boolean - true if estimate is in the area
Parameters:

- p_positionEstimate -
- p_geographicTargetArea -

fx_GadLatitude

    external function fx_GadLatitude(float coordinate) return integer;

Declared in group externalFunctionGroup
convertion of latitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
Returns: integer - integer
Parameters:

- coordinate -

fx_GadLongitude

    external function fx_GadLongitude(float coordinate) return integer;

Declared in group externalFunctionGroup
convertion of logitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
Returns: integer - integer
Parameters:

- coordinate -

© Copyright Testing Technologies IST GmbH 2012