OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test Cases Modules

INDEX

A B C D E F G H I J K L M N O P Q R S T U V W X Y Z _

T61String | type declared in ASNAUX
T_BCSM_CAMEL_TDP_Criteria | type declared in MAP_MS_DataTypes_V10
T_BCSM_CAMEL_TDP_CriteriaList | type declared in MAP_MS_DataTypes_V10
T_BcsmCamelTDPData | type declared in MAP_MS_DataTypes_V10
T_BcsmCamelTDPDataList | type declared in MAP_MS_DataTypes_V10
T_BcsmTriggerDetectionPoint | type declared in MAP_MS_DataTypes_V10
T_CauseValueCriteria | type declared in MAP_MS_DataTypes_V10
T_CSI | type declared in MAP_MS_DataTypes_V10
t_locErrorReason_V10 | template declared in RRLP_Templates
t_locErrorReason_V5 | template declared in RRLP_Templates
t_r_posTech | template declared in SUPL_Templates
t_r_sessionId | template declared in SUPL_Templates
t_r_setCaps | template declared in SUPL_Templates
t_r_ulpSuplEnd | template declared in SUPL_Templates
t_r_ulpSuplNotiRep | template declared in SUPL_Templates
t_r_ulpSuplPosInit | template declared in SUPL_Templates
t_r_ulpSuplPosInitV1 | template declared in SUPL_Templates
t_r_ulpSuplStart | template declared in SUPL_Templates
t_s_complementSetSessionId | template declared in SUPL_Templates
t_s_emptySessionId | template declared in SUPL_Templates
t_s_notification | template declared in SUPL_Templates
t_s_notificationTypeOnly | template declared in SUPL_Templates
t_s_plausibleSetSessionId | template declared in SUPL_Templates
TA0 | type declared in RRLP_Components_V10
TA1 | type declared in RRLP_Components_V10
TA2 | type declared in RRLP_Components_V10
TAResolution | type declared in SUPLTypes
TargetAreaCell | type declared in SUPL_V2_TypeDefinitions
TargetCellOutsideGCA_Param | type declared in MAP_ER_DataTypes_V10
TBCD_STRING | type declared in MAP_CommonDataTypes_V10
TC_000_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_000_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports SUPL INIT delivery using OMA Push and, if supported, MT SMS and, or SIP Push Test 4: ics_UDP
TC_001 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_002 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_003 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_004_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_005 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_006 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_007_1 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_2 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_3 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_4 | testcase declared in SUPL_V2_COMMON_Tests
TC_007_5 | testcase declared in SUPL_V2_COMMON_Tests
TC_008_1 | testcase declared in SUPL_V2_COMMON_Tests
TC_008_2 | testcase declared in SUPL_V2_COMMON_Tests To test SET correctly uses optional ciphering suites Test 2: ics_PSKTLS_add_cipher
TC_009_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 1: Correct support
TC_009_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 2: Correct discard procedure � incorrect Protection Level
TC_009_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 3: Correct discard procedure � incorrect Key Identity
TC_009_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly supports Basic SUPL INIT protection Case 4: Correct discard procedure � incorrect Basic Replay Counter
TC_010_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL message - Test 1: Support for higher versions of SUPL 2_X_X
TC_010_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accept compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
TC_010_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accept compatible Version numbers in SUPL messages - Test 3: Correct support with SLP supporting SUPL V3_0 and V2_0
TC_010_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL message - Test 4: Correct support with SLP supporting SUPL V1_0 only, SUPL V1_0 supported by SET
TC_011_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects unsupported Version number in SUPL messages - Test1: Higher version not supported
TC_011_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects unsupported Version number in SUPL messages - Test 2: Lower Version not supportet, SUPL V1_0 not supported by SET
TC_012 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly rejects incorrect UDP message content
TC_020 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_021 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_5 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_022_6 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_023 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_024_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_025_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_025_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_10 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 10: Autonomous GNSS
TC_030_11 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_12_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS Preferred methods
TC_030_12_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS Preferred methods
TC_030_13 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 13: OTDOA
TC_030_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_5 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_030_7 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_030_9 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based only - GLONASS
TC_031 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_033_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 1: E-SLP address sent in SUPL INIT
TC_033_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 2: Use of provisioned H-SLP address
TC_033_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions Emergency Services Location Requests Case 3: Use of default E-SLP address
TC_034_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions an Emergency Services Location Request when a normal SUPL session is also active Case 1: Normal SUPL session already in progress before Emergency SUPL session
TC_034_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions an Emergency Services Location Request when a normal SUPL session is also active Case 2: Normal SUPL session attempted during Emergency SUPL session
TC_040_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Real Time Periodic reporting - Test 1: A-GPS SET assisted
TC_040_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Real Time Periodic reporting - Test 2: A-GPS SET based
TC_041_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs basic Quasi Real Time Periodic reporting Test 2: A-GPS SET based
TC_042_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_042_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_042_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_050_1_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_050_1_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_050_1_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_050_1_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_050_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
TC_050_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
TC_050_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
TC_050_2_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Geographic Target Area - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_051_1_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_051_1_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_051_1_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_051_1_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_051_2_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 1: Entering event type
TC_051_2_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 2: Inside event type
TC_051_2_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 3: Outside event type
TC_051_2_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_061 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions when the Network cancels a Triggered Location Request
TC_065_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_065_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session).
TC_070_3 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_070_4 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session).
TC_071_1 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_071_2 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET coorectly actions timer UT3 - Test 2: Triggered session.
TC_072 | testcase declared in SUPL_V2_SLP_INITIATED_Tests
TC_073 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT7
TC_074 | testcase declared in SUPL_V2_SLP_INITIATED_Tests To test SET correctly actions timer UT8
TC_100_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_100_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_100_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_101 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_102 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_103_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
TC_103_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
TC_110_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_10 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
TC_110_11_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_11_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_12_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_12_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_13 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 13: OTDOA
TC_110_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_5 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_110_7 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_110_9 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
TC_130_1_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_130_1_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_130_1_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_130_1_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_130_2_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
TC_130_2_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
TC_130_2_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
TC_130_2_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Leaving event type
TC_131_1_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_131_1_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_131_1_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_131_1_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_131_2_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
TC_131_2_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
TC_131_2_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
TC_131_2_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_140_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_140_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT1 - Test 2: Triggered Session
TC_141_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_141_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
TC_141_3 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
TC_141_4 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
TC_142_1 | testcase declared in SUPL_V2_SET_INITIATED_Tests
TC_142_2 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT3 - Test 2: Triggered Session
TC_143 | testcase declared in SUPL_V2_SET_INITIATED_Tests To test SET correctly actions timer UT7
TCPInfo | type declared in SUPL_TypeDefinitions
tcpInfoEstablishedConnection | template declared in SUPL_Templates
TCPInfoMessage | type declared in SUPL_TypeDefinitions
tcpInfoReleaseConnection | template declared in SUPL_Templates
TEID | type declared in MAP_MS_DataTypes_V10
telephony | const declared in MAP_TS_Code_V10
TeleserviceCode | type declared in MAP_TS_Code_V10
TeleserviceList | type declared in MAP_MS_DataTypes_V10
TeleservNotProvParam | type declared in MAP_ER_DataTypes_V10
TeletexString | type declared in ASNAUX
TerminationCause | type declared in MAP_LCS_DataTypes_V10
TGSN | type declared in SUPLTypes
ThirdParty | type declared in SUPLTypes
ThirdPartyID | type declared in SUPLTypes
Time | type declared in MAP_CommonDataTypes_V10
TimeRelation | type declared in RRLP_Components_V10
TimeRelation | type declared in RRLPV5Types
TimeSlot | type declared in RRLP_Components_V10
TimeSlot | type declared in RRLPV5Types
TimeslotISCP | type declared in SUPLTypes
TimeslotISCP_List | type declared in SUPLTypes
TimeSlotScheme | type declared in RRLP_Components_V10
TimeSlotScheme | type declared in RRLPV5Types
Timestamp | type declared in LibSip_SIPTypesAndValues
TimeStamp | type declared in SUPLTypes
TimeValue | type declared in LibSip_SIPTypesAndValues
TimeWindow | type declared in SUPLTypes
TimingAdvance | type declared in SUPLTypes
TLMReservedBits | type declared in RRLP_Components_V10
TLMReservedBits | type declared in RRLPV5Types
TLMWord | type declared in RRLP_Components_V10
TLMWord | type declared in RRLPV5Types
TLSNotify | type declared in SUPL_Configuration
TlsVersionConfig | type declared in SUPL_Configuration
TMSI | type declared in MAP_CommonDataTypes_V10
To | type declared in LibSip_SIPTypesAndValues
TOA_MeasurementsOfRef | type declared in RRLP_Components_V10
TOA_MeasurementsOfRef | type declared in RRLPV5Types
Tokyo_Steps |
Tokyo_Templates_LPP |
Tokyo_Templates_RRLP |
Tokyo_TypesDefinitions |
TokyoAlmanacM0 | const declared in Tokyo_TypesDefinitions
TokyoAlmanacOmega0 | const declared in Tokyo_TypesDefinitions
TokyoAlmanacWNa | const declared in Tokyo_TypesDefinitions
TokyoAltitude | const declared in Tokyo_TypesDefinitions
TokyoClockModel_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoConfidence | const declared in Tokyo_TypesDefinitions
TokyoEphemM0 | const declared in Tokyo_TypesDefinitions
TokyoEphemOmegaA0 | const declared in Tokyo_TypesDefinitions
TokyoGNSS_AlmanacElement_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoGNSS_ReferenceLocation_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoGNSS_ReferenceTime_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoIonosphericModel_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoIonosphericModelV10 | template declared in Tokyo_Templates_RRLP
TokyoIonosphericModelV5 | template declared in Tokyo_Templates_RRLP
TokyoLatitude | const declared in Tokyo_TypesDefinitions
TokyoLongitude | const declared in Tokyo_TypesDefinitions
TokyoNavModelSatelliteElement_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoOrbitModel_LPP_AGPS | template declared in Tokyo_Templates_LPP
tokyoReferenceTimeOnlyV10 | template declared in Tokyo_Templates_RRLP
tokyoReferenceTimeOnlyV5 | template declared in Tokyo_Templates_RRLP
TokyoStartTOW | const declared in Tokyo_TypesDefinitions
TokyoUncertaintyAltitude | const declared in Tokyo_TypesDefinitions
TokyoUncertaintySemiMajor | const declared in Tokyo_TypesDefinitions
TokyoUncertaintySemiMinor | const declared in Tokyo_TypesDefinitions
TokyoUTCModel_LPP_AGPS | template declared in Tokyo_Templates_LPP
TokyoUTCModelV10 | template declared in Tokyo_Templates_RRLP
TokyoUTCModelV5 | template declared in Tokyo_Templates_RRLP
TokyoWeek | const declared in Tokyo_TypesDefinitions
TPDU_TypeCriterion | type declared in MAP_MS_DataTypes_V10
TraceDepth | type declared in MAP_OM_DataTypes_V10
TraceDepthList | type declared in MAP_OM_DataTypes_V10
TraceEventList | type declared in MAP_OM_DataTypes_V10
TraceInterfaceList | type declared in MAP_OM_DataTypes_V10
TraceNE_TypeList | type declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_bm_sc_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_eNB_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_ggsn_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_mgw_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_mme_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_msc_s_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_pgw_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_rnc_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_sgsn_ | const declared in MAP_OM_DataTypes_V10
TraceNE_TypeList_sgw_ | const declared in MAP_OM_DataTypes_V10
TracePropagationList | type declared in MAP_OM_DataTypes_V10
TraceRecordingSessionReference | type declared in MAP_OM_DataTypes_V10
TraceReference | type declared in MAP_OM_DataTypes_V10
TraceReference2 | type declared in MAP_OM_DataTypes_V10
TraceType | type declared in MAP_OM_DataTypes_V10
TracingBufferFullParam | type declared in MAP_ER_DataTypes_V10
TrackingAreaCode | type declared in SUPLTypes
trafficAndPublicTransportationInfo | const declared in MAP_CommonDataTypes_V10
trafficCongestionReporting | const declared in MAP_CommonDataTypes_V10
TransactionId | type declared in MAP_MS_DataTypes_V10
TransactionNumber | type declared in LPP_PDU_Definitions
transferToThirdParty | const declared in MAP_SS_Code_V10
TriggeredReportingCriteria | type declared in LPP_PDU_Definitions
TriggerParams | type declared in SUPLTypes
TriggerType | type declared in SUPLTypes
TripletList | type declared in MAP_MS_DataTypes_V10
ts_AuthenticationInit | function declared in SUPL_CommonSteps
ts_AuthenticationInitForGbaU | function declared in SUPL_CommonSteps
ts_AuthResponseCheck | function declared in SUPL_HTTP_Steps
ts_Build_DNS_A_Response | function declared in SUPL_DHCP_DNS_Steps
ts_Build_DNS_AAAA_Response | function declared in SUPL_DHCP_DNS_Steps
ts_calculateRspauth | function declared in SUPL_HTTP_Steps
ts_DefaultDef | altstep declared in SUPL_Preambles
ts_gps_action | function declared in SUPL_CommonSteps Sends a given request to the GPS simulator as upper tester command (MMIMessage)
ts_gps_action_withtimer | function declared in SUPL_CommonSteps Sends a given request to the GPS simulator with a given timer as upper tester commands (MMIMessage)
ts_msrPositionReq_V10 | template declared in RRLP_Templates
ts_msrPositionReq_V5 | template declared in RRLP_Templates
ts_Postamble | function declared in SUPL_Postambles
TYPE_IDENTIFIER | type declared in ASNAUX
TYPENULL | type declared in ASNAUX
TypeOfUpdate | type declared in MAP_MS_DataTypes_V10

© Copyright Testing Technologies IST GmbH 2012