OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group suplIcsItemsGroup

Declared in module SUPL_V2_Parameters
Subgroups: TransportSMS

Modulepars Summary
ics_AGANSSSETassisted_Galileo_Network_initiated | (boolean) UE supports A-GANSS SET assited Galileo Positioning Method (Network initiated)
ics_AGANSSSETbased_Galileo_Network_initiated | (boolean) UE supports A-GANSS SET based Galileo Positioning Method (Network initiated)
ics_AGANSSSETassisted_GLONASS_Network_initiated | (boolean) UE supports A-GANSS SET assited GLONASS Positioning Method (Network initiated)
ics_AGANSSSETbased_GLONASS_Network_initiated | (boolean) UE supports A-GANSS SET based GLONASS Positioning Method (Network initiated)
ics_autonomousGANSS_Network_initiated | (boolean) UE supports autonomous GNSS Positioning Method in Network initiated session
ics_AGANSSSETassisted_GLONASS_SET_initiated | (boolean) UE supports A-GANSS SET assited GLONASS Positioning Method in SET initiated session
ics_AGANSSSETbased_GLONASS_SET_initiated | (boolean) UE supports A-GANSS SET based GLONASS Positioning Method in SET initiated session
ics_autonomousGANSS_SET_initiated | (boolean) UE supports autonomous GNSS Positioning Method in SET initiated session
ics_AGANSSSETassisted_Galileo_SET_initiated | (boolean) UE supports SET assisted A-GANSS Positioning Method in SET initiated session
ics_AGANSSSETbased_Galileo_SET_initiated | (boolean) UE supports SET based A-GANSS Positioning Method in SET initiated session
ics_AGNSSSETassisted_preferred | (boolean) UE supports SET declares A-GNSS SET-assisted preferred in Pref Method in SUPL START
ics_AGNSSSETbased_preferred | (boolean) UE supports SET declares A-GNSS SET-based preferred in Pref Method in SUPL START
ics_OTDOA_SET_initiated | (boolean) UE supports SET based OTDOA Positioning Method in SET initiated session
ics_OTDOA_Network_initiated | (boolean) UE supports SET based OTDOA Positioning Method in Network initiated session
ics_AreaEvent_Network_initiated | (boolean) Area Event Triggered Service in Network initiated call flows supported
ics_periodic_Network_initiated | (boolean) Periodic trigger in Network initiated call flows supported
ics_quasi_real_time | (boolean) Quasi real time reporting supported
ics_stop_triggered_session | (boolean) Ability to stop Triggered Location Session supported
ics_event_Network_initiated | (boolean) Area Event Triggered Service in Network initiated call flows supported
ics_periodic_SET_initiated | (boolean) Periodic trigger in SET initiated call flows supported
ics_event_SET_initiated | (boolean) Area Event Triggered Service in SET initiated call flows supported
ics_real_time | (boolean) Real time reporting supported
ics_GeoTargetArea | (boolean) Geographic Target Area supported
ics_AreaId | (boolean) Area Id supported
ics_AreaEvent_SET_initiated | (boolean) Area Event initiated at SET
icsStopTimeSupport | (boolean) True, if SUT supports Stop Time
icsStartTimeSupport | (boolean) True, if SUT supports Start Time
ics_support_SUPLV1 | (boolean) True, if SUT supports SUPL V1_0
ics_batch | (boolean) Basic Batch reporting supported
ics_SipPush |
ics_UDP |

## Details

ics_AGANSSSETassisted_Galileo_Network_initiated

    boolean ics_AGANSSSETassisted_Galileo_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited Galileo Positioning Method (Network initiated)

ics_AGANSSSETbased_Galileo_Network_initiated

    boolean ics_AGANSSSETbased_Galileo_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based Galileo Positioning Method (Network initiated)

ics_AGANSSSETassisted_GLONASS_Network_initiated

    boolean ics_AGANSSSETassisted_GLONASS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited GLONASS Positioning Method (Network initiated)

ics_AGANSSSETbased_GLONASS_Network_initiated

    boolean ics_AGANSSSETbased_GLONASS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based GLONASS Positioning Method (Network initiated)

ics_autonomousGANSS_Network_initiated

    boolean ics_autonomousGANSS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports autonomous GNSS Positioning Method in Network initiated session

ics_AGANSSSETassisted_GLONASS_SET_initiated

    boolean ics_AGANSSSETassisted_GLONASS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited GLONASS Positioning Method in SET initiated session

ics_AGANSSSETbased_GLONASS_SET_initiated

    boolean ics_AGANSSSETbased_GLONASS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based GLONASS Positioning Method in SET initiated session

ics_autonomousGANSS_SET_initiated

    boolean ics_autonomousGANSS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports autonomous GNSS Positioning Method in SET initiated session

ics_AGANSSSETassisted_Galileo_SET_initiated

    boolean ics_AGANSSSETassisted_Galileo_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET assisted A-GANSS Positioning Method in SET initiated session

ics_AGANSSSETbased_Galileo_SET_initiated

    boolean ics_AGANSSSETbased_Galileo_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based A-GANSS Positioning Method in SET initiated session

ics_AGNSSSETassisted_preferred

    boolean ics_AGNSSSETassisted_preferred := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET declares A-GNSS SET-assisted preferred in Pref Method in SUPL START

ics_AGNSSSETbased_preferred

    boolean ics_AGNSSSETbased_preferred := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET declares A-GNSS SET-based preferred in Pref Method in SUPL START

ics_OTDOA_SET_initiated

    boolean ics_OTDOA_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based OTDOA Positioning Method in SET initiated session

ics_OTDOA_Network_initiated

    boolean ics_OTDOA_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based OTDOA Positioning Method in Network initiated session

ics_AreaEvent_Network_initiated

    boolean ics_AreaEvent_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in Network initiated call flows supported

ics_periodic_Network_initiated

    boolean ics_periodic_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Periodic trigger in Network initiated call flows supported

ics_quasi_real_time

    boolean ics_quasi_real_time := true

Declared in group suplIcsItemsGroup
(boolean) Quasi real time reporting supported

ics_stop_triggered_session

    boolean ics_stop_triggered_session := true

Declared in group suplIcsItemsGroup
(boolean) Ability to stop Triggered Location Session supported

ics_event_Network_initiated

    boolean ics_event_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in Network initiated call flows supported

ics_periodic_SET_initiated

    boolean ics_periodic_SET_initiated := false

Declared in group suplIcsItemsGroup
(boolean) Periodic trigger in SET initiated call flows supported

ics_event_SET_initiated

    boolean ics_event_SET_initiated := false

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in SET initiated call flows supported

ics_real_time

    boolean ics_real_time := true

Declared in group suplIcsItemsGroup
(boolean) Real time reporting supported

ics_GeoTargetArea

    boolean ics_GeoTargetArea := true

Declared in group suplIcsItemsGroup
(boolean) Geographic Target Area supported

ics_AreaId

    boolean ics_AreaId := true

Declared in group suplIcsItemsGroup
(boolean) Area Id supported

ics_AreaEvent_SET_initiated

    boolean ics_AreaEvent_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event initiated at SET

icsStopTimeSupport

    boolean icsStopTimeSupport := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports Stop Time

icsStartTimeSupport

    boolean icsStartTimeSupport := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports Start Time

ics_support_SUPLV1

    boolean ics_support_SUPLV1 := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports SUPL V1_0

ics_batch

    boolean ics_batch := true

Declared in group suplIcsItemsGroup
(boolean) Basic Batch reporting supported

ics_SipPush

    boolean ics_SipPush := true

Declared in group suplIcsItemsGroup.TransportSMS

ics_UDP

    boolean ics_UDP := true

Declared in group suplIcsItemsGroup.TransportSMS

© Copyright Testing Technologies IST GmbH 2012