OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module SUPL_V2_SET_INITIATED_Tests

Import Declarations:

- Tokyo_Steps
  all
- SUPL_V2_TypeDefinitions
  all
- SUPL_ExternalSteps
  all
- SUPL_TypeDefinitions
  all
- Tokyo_Templates_RRLP
  all
- RRLPV10Types
  all
- RRLP_CommonTypes
  all
- SUPLTypes
  all
- SUPL_V2_Templates
  all
- LPP_Templates
  all
- SUPL_Postambles
  all
- SUPL_CommonSteps
  all
- SUPL_Preambles
  all
- SUPL_Parameters
  all
- RRLPV5Types
  all
- SUPL_V2_CommonSteps
  all
- SUPL_Templates
  all
- LibCommon_DataStrings
  all
- SUPL_Configuration
  all
- RRLP_Templates
  all
- SUPL_V2_Parameters
  all

Groups:

- TC_10x

- TC_100
- TC_103

- TC_11x

- TC_110

- TC_13x

- TC_130

- TC_130_1
- TC_130_2

- TC_131

- TC_131_1
- TC_131_2

- TC_14x

- TC_140
- TC_141
- TC_142

Test cases Summary
TC_100_1 |
TC_100_2 |
TC_100_3 |
TC_101 |
TC_102 |
TC_103_1 | To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
TC_103_2 | To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
TC_110_1 |
TC_110_2 |
TC_110_3 |
TC_110_4 |
TC_110_5 |
TC_110_7 | To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
TC_110_9 | To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
TC_110_10 | To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
TC_110_11_1 | To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_11_2 | To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only.
TC_110_12_1 | To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_12_2 | To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
TC_110_13 | To test SET correctly actions single session Positioning method - Test 13: OTDOA
TC_130_1_1 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_130_1_2 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_130_1_3 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_130_1_4 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_130_2_1 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
TC_130_2_2 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
TC_130_2_3 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
TC_130_2_4 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Leaving event type
TC_131_1_1 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_131_1_2 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_131_1_3 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_131_1_4 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_131_2_1 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
TC_131_2_2 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
TC_131_2_3 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
TC_131_2_4 | To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type
TC_140_1 |
TC_140_2 | To test SET correctly actions timer UT1 - Test 2: Triggered Session
TC_141_1 |
TC_141_2 | To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
TC_141_3 | To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
TC_141_4 | To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
TC_142_1 |
TC_142_2 | To test SET correctly actions timer UT3 - Test 2: Triggered Session
TC_143 | To test SET correctly actions timer UT7

## Details

TC_100_1

    testcase TC_100_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_100
Runs On: SUPLComponent
System: SystemInterfaces

TC_100_2

    testcase TC_100_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_100
Runs On: SUPLComponent
System: SystemInterfaces

TC_100_3

    testcase TC_100_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_100
Runs On: SUPLComponent
System: SystemInterfaces

TC_101

    testcase TC_101() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x
Runs On: SUPLComponent
System: SystemInterfaces

TC_102

    testcase TC_102() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x
Runs On: SUPLComponent
System: SystemInterfaces

TC_103_1

    testcase TC_103_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_103
To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
Purpose: SUPL-2.0-con-103-1 TP version: Test Case Id : SUPL-2.0-con-103 Test Object : Client Test Case Description : To test SET correctly accepts compatible Version numbers in SUPL messages Specification Reference : ULP TS 7,9,10 SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : State: Continuation of / Can be tested at the same time as: Prerequisite for this test: o Applicability: Test Procedure : Test 1: Support for higher versions of SUPL 2.X.X 1. Start a SI Location Session 2. In the Common Part of all messages set: Version to: o Maj set to 2 o Min set to a higher value than that supported by the SET o Serv ind set to a higher value than that supported by the SET 3. The SET sends SUPL START 4. Send SUPL RESPONSE with Version set as in step 2. 5. The SET sends SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET 6. The Location Session completes successfully. Pass-Criteria : Test 1 and 2: 1. 1. At step 5 the SET shall respond with SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET
Runs On: SUPLComponent
System: SystemInterfaces

TC_103_2

    testcase TC_103_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_103
To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
Purpose: SUPL-2.0-con-103-2 TP version: Test Case Id : SUPL-2.0-con-103 Test Object : Client Test Case Description : To test SET correctly accepts compatible Version numbers in SUPL messages Specification Reference : ULP TS 7,9,10 SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : State: Continuation of / Can be tested at the same time as: Prerequisite for this test: o Applicability: Test Procedure : Test 2: Support for lower versions of SUPL 2.X.X. Only applicable if there exists SUPL V2.X where X>0 1. Start a SI Location Session 2. In the Common Part of all messages set: Version to: o Maj set to 2 o Min set to a lower values than the maximum value supported by the SET o Serv ind set to a lower values than the maximum value supported by the SET 3. The SET sends SUPL START 4. Send SUPL RESPONSE with Version set as in step 2. 5. The SET sends SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET 6. The Location Session completes successfully. Pass-Criteria : Test 1 and 2: 1. 1. At step 5 the SET shall respond with SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_1

    testcase TC_110_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_2

    testcase TC_110_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_3

    testcase TC_110_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_4

    testcase TC_110_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_5

    testcase TC_110_5() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_7

    testcase TC_110_7() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 7: A-GANSS SET assisted - GLONASS
Purpose: SUPL-2.0-con-110-7 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGANSSSETassisted_GLONASS_SET_initiated Test Procedure : Test 7: A-GANSS SET assisted –GLONASS [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: A-GNSS SET assisted only GNSS Positioning Technology set to: GLONASS 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 5. Do nothing (only Test 4 and Test 5) 6. A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. 7. Do nothing (only Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2) 8. send SUPL END with: Position set to a realistic position for the SET. 9. The SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_9

    testcase TC_110_9() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 9: A-GANSS SET based - GLONASS
Purpose: SUPL-2.0-con-110-9 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGANSSSETbased_GLONASS_SET_initiated Test Procedure : Test 9: A-GANSS SET based –GLONASS [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. 7. Test 9: send SUPL END 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_10

    testcase TC_110_10() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 10: Autonomous GANSS
Purpose: SUPL-2.0-con-110-10 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_autonomousGANSS_SET_initiated AND ixit_gANSS Test Procedure : Test 10: Autonomous GANSS [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_11_1

    testcase TC_110_11_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only. Otherwise A-GANSS SET based only
Purpose: SUPL-2.0-con-110-11_1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGNSSSETassisted_preferred AND ixit_gANSS Test Procedure : Test 11: SET declares A-GNSS SET-assisted Preferred method [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. Test 11: If A-GPS is supported by the SET then A-GPS SET based shall be used. Otherwise A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_11_2

    testcase TC_110_11_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 11: If A-GPS is supported by the SET then A-GPS SET based only. Otherwise A-GANSS SET based only
Purpose: SUPL-2.0-con-110-11_1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AGNSSSETassisted_preferred AND ixit_gANSS Test Procedure : Test 11: SET declares A-GNSS SET-assisted Preferred method [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to: Autonomous GANSS GNSS Positioning Technology set to: Not set 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 3 and Test 10: No Assistance Data is sent. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics Test 4 only: Location ID, Cell info, the following parameters: NMR and/or TA if testing using GSM, Measured Results List if testing using WCDMA. All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 10: one of Galileo or GLONASS can be used depending on the technology supported by the SET and declared in ixit_gANSS. Test 11: If A-GPS is supported by the SET then A-GPS SET based shall be used. Otherwise A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_12_1

    testcase TC_110_12_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
Purpose: SUPL-2.0-con-110-12-1 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ( (ics_AGANSSSETassisted_Galileo_SET_initiated AND ics_AGANSSSETbased_Galileo_SET_initiated) OR (ics_AGANSSSETassisted_GLONASS_SET_initiated AND ics_AGANSSSETbased_GLONASS_SET_initiated)) AND (ixit_gANSS.galileo or ixit_gANSS.gloneass) Test Procedure : Test 12: A-GANSS Preferred methods [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 1: A-GANSS SET assisted is used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 8. Test 1, Test 6, Test 7, Test 11 Case 1 and Test 12 Case 1: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 1: A-GANSS SET assisted shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_12_2

    testcase TC_110_12_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 12: A-GANSS SET Preferred methods
Purpose: SUPL-2.0-con-110-12-2 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ( (ics_AGANSSSETassisted_Galileo_SET_initiated AND ics_AGANSSSETbased_Galileo_SET_initiated) OR (ics_AGANSSSETassisted_GLONASS_SET_initiated AND ics_AGANSSSETbased_GLONASS_SET_initiated)) AND ixit_gANSS Test Procedure : Test 12: A-GANSS Preferred methods [Includes optional features] Note that these test cases only test a single GNSS at one time. Testing of support for multiple simultaneous GNSSs is for further study. 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based is used, where in both cases the GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 7. Test 2, Test 3, Test 8, Test 9, Test 10, Test 11 Case 2 and Test 12 Case 2: send SUPL END 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_110_13

    testcase TC_110_13() runs on SUPLComponent system SystemInterfaces

Declared in group TC_11x.TC_110
To test SET correctly actions single session Positioning method - Test 13: OTDOA
Purpose: SUPL-2.0-con-110-13 TP version: Test Case Id : SUPL-2.0-con-110 Test Object : Client Test Case Description : To test SET correctly actions single session Positioning method Specification Reference : ULP TS 5.2.1, 8, 9 SCR Reference : ULP-PRO-C-009-O, ULP-PRO-C-011-M, ULP-PRO-C-012-O, ULP-PRO-C-013-O, ULP-PRO-C-014-O, ULP-PRO-C-015-O, ULP-PRO-C-016-O, ULP-PRO-C-018-O, ULP-PRO-C-020 Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_OTDOA_SET_initiated Test Procedure : Test 13: OTDOA [Includes optional features] 1. All tests: start a SI Location Session 2. The SET sends SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 3. Send SUPL RESPONSE with: Positioning Method set to the value specified in the table below GNSS Positioning Technology set to the value specified in the table below 4. The SET sends SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 6. All tests except Test 4 and Test 5: A SUPL POS session takes place and completes successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based is used, where in both cases the GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. 8. Test 1, Test 6, Test 7, Test 12 and Test 13: send SUPL END with: Position set to a realistic position for the SET. 9. All tests: the SET releases the secure IP connection. Note: Repeat for all Positioning technologies supported by the SET as declared in the ics Pass-Criteria : All tests: 1. At step 2 the SET shall send SUPL START with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics 2. At step 2 the SET shall send SUPL POS INIT with: SET capabilities parameter consistent with the Positioning technologies supported by the SET as declared in the ics All tests except Test 4 and Test 5: 3. At step 6 a SUPL POS session shall take place and shall complete successfully using the Positioning Method defined by the test case. Test 12, Case 2: A-GANSS SET based shall be used. The GANSS used can be one of Galileo or GLONASS depending on the technology supported by the SET and declared in ixit_gANSS. Test 13: OTDOA shall be used.
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_1

    testcase TC_130_1_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
Purpose: SUPL-2.0-con-130-1-1 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 1: Entering event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 1: Entering event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s Test 1: A-GPS SET assisted: 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 1: Entering event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 1: The SET does not immediately display the position estimate as Entering event has not been met. Note however that the SET will eventually respond as described in step 7. 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 1: After one of these sequences the SET displays the position estimate as Entering event has been met. At other times the SET does not display the position estimate as Entering event has not been met. 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_2

    testcase TC_130_1_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
Purpose: SUPL-2.0-con-130-1-2 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 2: Inside event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 2: Inside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 2: Inside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 2: The SET displays the calculated position estimate as Inside event has been met 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7.Case 2: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Inside event has been met 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 4: At step 7: Case 2 and Case 3: After each of these sequences the SET shall display the position estimate at intervals of at least 60 seconds after the display of the previous position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_3

    testcase TC_130_1_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
Purpose: SUPL-2.0-con-130-1-3 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 3: Outside event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 3: Outside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 3: Outside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 3: The SET displays the calculated position estimate as Outside event has been met 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Outside event has been met 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. Case 2 and Case 3: After each of these sequences the SET shall display the position estimate at intervals of at least 60 seconds after the display of the previous position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_4

    testcase TC_130_1_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
Purpose: SUPL-2.0-con-130-1-4 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 4: Leaving event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 4: Leaving event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 4: Leaving event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 4: The SET does not immediately display the position estimate as Leaving event has not been met. Note however that the SET will eventually respond as described in step 7. 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 4: After one of these sequences the SET displays the position estimate as Leaving event has been met. At other times the SET does not display the position estimate as Leaving event has not been met. 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_2_1

    testcase TC_130_2_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_2
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Entering event type
Purpose: SUPL-2.0-con-130-2-1 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 1: Entering event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 1: Entering event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 1: Entering event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET based. - Trigger Params not set Note that the SET may release the secure connection at this point. 10. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 11. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: Case 1: The SET does not immediately display the position estimate as Entering event has not been met. Note however that the SET will eventually respond as described in step 12. 12. Until step 13 is reached: Case 1: At one time the SET displays the position estimate as Entering event has been met. The remainder of the time the SET does not display the position estimate as Entering event has not been met. 13. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 2: 6. At step 11: Case 1and Case 4: The SET shall not display the position estimate 7: At step 12: Case 1and Case 4: At one time the SET shall display the position estimate. The remainder of the time the SET shall not display the position estimate. 8. At step 13: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2. If Stop Time is not supported: Case 1 and Case 4: No requirement
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_2_2

    testcase TC_130_2_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_2
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 2: Inside event type
Purpose: SUPL-2.0-con-130-2-2 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 2: Inside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 2: Inside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET based. - Trigger Params not set 10. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 11. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: Case 2: The SET displays the calculated position estimate as Inside event has been met 12. Until step 13 is reached: Case 2: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Inside event has been met 13. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 2: 6. At step 11: Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 7: At step 12: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET shall display the position estimate. 8. At step 13: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_2_3

    testcase TC_130_2_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_2
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 3: Outside event type
Purpose: SUPL-2.0-con-130-2-3 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 3: Outside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] Figure 3: Case 3: SET is outside area 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 3: Outside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET based. - Trigger Params not set Note that the SET may release the secure connection at this point. 10. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 11. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: Case 3: The SET displays the calculated position estimate as Outside event has been met 12. Until step 13 is reached: Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Outside event has been met 13. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 2: 6. At step 11: Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 7: At step 12: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET shall display the position estimate. 8. At step 13: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_2_4

    testcase TC_130_2_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_2
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 2: A-GPS SET based, Case 1: Leaving event type
Purpose: SUPL-2.0-con-130-2-4 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 4: Leaving event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 4: Leaving event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 4: Leaving event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET based. - Trigger Params not set 10. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 11. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: Case 4: The SET does not immediately display the position estimate as Leaving event has not been met. Note however that the SET will eventually respond as described in step 12. 12. Until step 13 is reached: Case 4: At one time the SET displays the position estimate as Leaving event has been met. The remainder of the time the SET does not display the position estimate as Leaving event has not been met. 13. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 2: 6. At step 11: Case 1and Case 4: The SET shall not display the position estimate Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 7: At step 12: Case 1and Case 4: At one time the SET shall display the position estimate. The remainder of the time the SET shall not display the position estimate. Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET shall display the position estimate. 8. At step 13: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2. If Stop Time is not supported: Case 1 and Case 4: No requirement Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_1

    testcase TC_131_1_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 1: Entering event type
Purpose: SUPL-2.0-con-131-1-1 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 1: Entering event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 1: Entering event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 1: Entering event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: - Case 1: The SET does not respond as Entering event has not been met. 5. Do nothing (Step only applies to cases 2 and 3) 6. At some time: Case 1 and Case 4: - Case 1: The SET does not respond as Entering event has not been met. 7. Do nothing (Step only applies to cases 2 and 3) 8. Do nothing (Step only applies to cases 2 and 3) 9. Case 1 and Case 4: 120 seconds after step 2: Case 1: force a cellular handover to the GSM or WCDMA Cell ID that is normally used for testing. 10. Case 1 and Case 4: At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 11. Case 1 and Case 4: Case 1: The SET displays the calculated position estimate as Entering event has been met. 12. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 1 and Case 4 the SET shall not respond 4. At step 6: Case 1 and Case 4 the SET shall not respond 7. At step 10: Case 1 and Case 4 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully 8. At step 11: Case 1 and Case 4 the SET shall display the calculated position estimate 9. At step 12: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2.
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_2

    testcase TC_131_1_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 2: Inside event type
Purpose: SUPL-2.0-con-131-1-2 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 2: Inside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 2: Inside event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in the Area ID list. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 2: Inside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 2: Inside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: - Case 2: The SET displays the calculated position estimate as Inside event has been met 6. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. After at least 60 seconds (set by Minimum Interval Time) after step 5: - Case 2: The SET displays the calculated position estimate as Inside event has been met 8. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more sequence as detailed below may take place before this occurs. If Stop Time is not supported the following sequence takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. Case 2: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Inside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 3. At step 5: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 4 if Start Time is not supported 4. At step 6: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 6. At step 8: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END - The SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. - After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_3

    testcase TC_131_1_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 3: Outside event type
Purpose: SUPL-2.0-con-131-1-3 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 3: Outside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 3: Outside event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The cell that is normally used for testing is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 3: Outside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 3: Outside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: - Case 3: The SET displays the calculated position estimate as Outside event has been met 6. At some time: Case 2 and Case 3: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. After at least 60 seconds (set by Minimum Interval Time) after step 5: - Case 3: The SET displays the calculated position estimate as Outside event has been met 8. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more sequence as detailed below may take place before this occurs. If Stop Time is not supported the following sequence takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. Case 3: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Outside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 3. At step 5: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 4 if Start Time is not supported 4. At step 6: Case 2 and Case 3 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 6. At step 8: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END - The SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully. - After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_1_4

    testcase TC_131_1_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_1
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 1: A-GPS SET assisted, Case 4: Leaving event type
Purpose: SUPL-2.0-con-131-1-4 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Assisted Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 4: Leaving event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 4: Leaving event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in Area ID list. The SET then handsover to a cell that is not normally used for testing and that is not present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 4: Leaving event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET assisted. Trigger Params set to Area Event Params with: o Area Event Type: Case 4: Leaving event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 4. At some time: Case 1 and Case 4: - Case 4: The SET does not respond as Leaving event has not been met 5. Do nothing (Applies only to Case 2 and Case 3) 6. At some time: - Case 4: The SET does not respond as Leaving event has not been met 7. Do nothing (Applies only to Case 2 and Case 3) 8. Do nothing (Applies only to Case 2 and Case 3) 9. Case 1 and Case 4: 120 seconds after step 2: Case 4: force a cellular handover to a GSM or WCDMA Cell ID that is not normally used for testing. 10. Case 1 and Case 4: At some time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 11. Case 1 and Case 4: Case 4: The SET displays the calculated position estimate as Leaving event has been met. 12. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. Test 1: 2. At step 4: Case 1 and Case 4 the SET shall not respond 4. At step 6: Case 1 and Case 4 the SET shall not respond 5. At step 7: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 5 7. At step 10: Case 1 and Case 4 the SET shall respond with SUPL POS INIT and a SUPL POS session shall take place and complete successfully 8. At step 11: Case 1 and Case 4 the SET shall display the calculated position estimate 9. At step 12: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2.
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_1

    testcase TC_131_2_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 1: Entering event type
Purpose: SUPL-2.0-con-131-2-1 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 1: Entering event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 1: Entering event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 1: Entering event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 1: The SET does not respond as Entering event has not been met. 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 1: The SET does not respond as Entering event has not been met. 17. Do nothing (Applies only to Case 2 and Case 3) 18. Case 1 and Case 4: 120 seconds after step 3: Case 1: force a cellular handover to the GSM or WCDMA Cell ID that is normally used for testing. 19. Case 1 and Case 4: Case 1: The SET displays the calculated position estimate as Entering event has been met. 20. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 1and Case 4: The SET shall not display the position estimate. 11. At step 16: Case 1 and Case 4 the SET shall not respond 13: At step 19: Case 1 and Case 4 the SET shall display the calculated position estimate. 14. At step 20: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_2

    testcase TC_131_2_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 2: Inside event type
Purpose: SUPL-2.0-con-131-2-2 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 2: Inside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 1: Entering event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The SET then handsover to the cell that is normally used for testing and that is present in the Area ID List. Case 2: Inside event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in the Area ID list. Figure 2: Case 2: SET is inside area 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 2: Inside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 2: Inside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 2: The SET displays the calculated position estimate as Inside event has been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 2: The SET displays the calculated position estimate as Inside event has been met 17. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more display of the calculated position estimate as detailed below may take place before this occurs. If Stop Time is not supported the following takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Case 2: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Inside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 2 and Case 3 The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 11. At step 16: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 15 12. At step 17: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_3

    testcase TC_131_2_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 3: Outside event type
Purpose: SUPL-2.0-con-131-2-3 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 3: Outside event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 3: Outside event type The SET camps on a GSM or WCDMA Cell ID that is not normally used for testing and that is not present in Area ID list. The cell that is normally used for testing is present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 3: Outside event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 2 and Case 3: 120 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 3: Outside event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 3: The SET displays the calculated position estimate as Outside event has been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 3: The SET displays the calculated position estimate as Outside event has been met 17. Case 2 and Case 3: If Stop Time is supported, the SET sends SUPL END approximately 120 seconds (set by Stop Time) after step 2. Note that one more display of the calculated position estimate as detailed below may take place before this occurs. If Stop Time is not supported the following takes place repeatedly until the SET has displayed the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Case 3: After at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the calculated position estimate as Outside event has been met Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 2 and Case 3 The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 11. At step 16: Case 2 and Case 3 the SET shall display the calculated position estimate after at least 60 seconds after step 15 12. At step 17: Case 2 and Case 3: If Stop Time is supported the SET shall send SUPL END approximately 120 seconds after step 2. If Stop Time is not supported the following shall take place repeatedly until the SET has displayed the remaining number of position estimates, and then the SET shall send SUPL END After at least 60 seconds after the display of the previous position estimate, the SET shall display the calculated position estimate
Runs On: SUPLComponent
System: SystemInterfaces

TC_131_2_4

    testcase TC_131_2_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_131.TC_131_2
To test SET correctly performs Area Event reporting using Area ID generated by the SLP - Test 2: A-GPS SET based, Case 4: Leaving event type
Purpose: SUPL-2.0-con-131-2-4 TP version: Test Case Id : SUPL-2.0-con-131 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Area ID generated by the SLP: MS Based Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AreaId AND ics_AGPSSETbased_SET_initiated Test Procedure : Test 2: A-GPS SET based Case 4: Leaving event type Details of cellular scenarios to be used and figures showing locations to aid understanding of test cases: In all cases the SET specifies the “Tokyo” Geographical target area and the SLP converts this into the Cell ID that is normally Case 4: Leaving event type The SET camps on the GSM or WCDMA Cell ID that is normally used for testing and that is present in Area ID list. The SET then handsover to a cell that is not normally used for testing and that is not present in the Area ID List. 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: Area Event Type: o Case 4: Leaving event type Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 4 Start Time: If supported: 30 seconds Stop Time: If supported: o Case 1 and Case 4: 240 seconds Geographic Target Area List with: o Geographic Target Area set to: Circular with: Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East Radius set to: 1000 meters Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: Trigger Type set to Area Event The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to A-GPS SET based. Trigger Params set to Area Event Params with: o Area Event Type: Case 4: Leaving event type o Location estimate: True o Repeated reporting not set o Geographic Target Area List not set o Area Id List with: Area Id Set set to one of the following, depending on the technology being used for testing: GSM Area Id with: Cell Global Identity set to value normally used during testing with GSM and Mobile Country Code, Mobile Network Code and Location Area Code not set WCDMA Area Id with: Cell Identity set to value normally used during testing with WCDMA and Mobile Country Code, Mobile Network Code and Location Area Code not set Area Id Set Type and Geographic Area Mapping List not set Note that the SET may release the secure connection at this point. 14. At any time during the following part of the test when the SET is required to make a position estimate, if the SET requires Assistance Data, then: - The SET responds with SUPL POS INIT - A SUPL POS session takes place and completes successfully - Send SUPL REPORT with no parameters. Note that the SET may release the secure connection at this point. 15. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 3 if Start Time is not supported: - Case 4: The SET does not respond as Leaving event has not been met 16. After at least 60 seconds (set by Minimum Interval Time) after step 15: - Case 4: The SET does not respond as Leaving event has not been met 17. Do nothing (Only applies to Case 2 and Case 3) 18. Case 1 and Case 4: 120 seconds after step 3: Case 4: force a cellular handover to a GSM or WCDMA Cell ID that is not normally used for testing. 19. Case 1 and Case 4: Case 4: The SET displays the calculated position estimate as Leaving event has been met. 20. Case 1 and Case 4: If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported, 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 10. At step 15: Case 1and Case 4: The SET shall not display the position estimate. 11. At step 16: Case 1 and Case 4 the SET shall not respond 13: At step 19: Case 1 and Case 4 the SET shall display the calculated position estimate. 14. At step 20: Case 1 and Case 4 if Stop Time is supported, the SET shall send SUPL END approximately 240 seconds after step 2
Runs On: SUPLComponent
System: SystemInterfaces

TC_140_1

    testcase TC_140_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
Runs On: SUPLComponent
System: SystemInterfaces

TC_140_2

    testcase TC_140_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_140
To test SET correctly actions timer UT1 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-140-2 TP version: Test Case Id : SUPL-2.0-con-140 Test Object : Client Test Case Description : To test SET correctly actions timer UT1 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 2: Triggered session [Includes Optional Features] 6. Start a SI Periodic Triggered Location Session, or a SI Area Event Triggered Location session if Periodic Location sessions are not supported in the SET. 7. The SET sends SUPL TRIGGERED START 8. Do not respond 9. After timer UT1 expires (depending on ixit_timer_UT1) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 10. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : 1. At step 4 and step 9 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 5 and step 10 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_1

    testcase TC_141_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_2

    testcase TC_141_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-2 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 8. Start a SI Periodic Triggered Location Session 9. The SET sends SUPL TRIGGERED START 10. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 11. When the first periodic trigger occurs the SET sends SUPL POS INIT 12. Do not respond 13. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the SUPL POS session) Note that the SET may release the secure connection at this time. 14. When the second periodic trigger occurs the SET sends SUPL POS INIT 15. A SUPL POS session takes place 16. Send SUPL REPORT 17. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_3

    testcase TC_141_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 3: No SUPL POS session
Purpose: SUPL-2.0-con-141-3 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Test Procedure : Test 3: No SUPL POS session (Immediate session) 18. Start a SI Location Session 19. The SET sends SUPL START 20. Send SUPL RESPONSE with: Positioning Method set to Enhanced Cell/sector 21. The SET sends SUPL POS INIT 22. Do not respond 23. After timer UT2 expires (depending on ixit_timer_UT2) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 24. The Location Session ends and the SET releases the secure IP connection. Pass-Criteria : Test 1 and Test 3: 1. At step 6 and step 23 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 7 and step 24 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

TC_141_4

    testcase TC_141_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_141
To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session)
Purpose: SUPL-2.0-con-141-4 TP version: Test Case Id : SUPL-2.0-con-141 Test Object : Client Test Case Description : To test SET correctly actions timer UT2 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_periodic_SET_initiated OR ics_event_SET_initiated Test Procedure : Test 4: No SUPL POS session (Triggered session) [Includes optional features] Note: This test case is applicable to SETs that support any triggered service. This test case has been written for a Periodic Triggered Location Session. The case where Periodic Location sessions is not supported in the SET is FFS 25. Start a SI Periodic Triggered Location Session 26. The SET sends SUPL TRIGGERED START 27. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to Enhanced Cell/sector 28. When the first periodic trigger occurs the SET sends SUPL POS INIT 29. Do not respond 30. (After timer UT2 expires (depending on ixit_timer_UT2) the SET will abandon the individual location session) 31. When the second periodic trigger occurs the SET sends SUPL POS INIT 32. Send SUPL REPORT 33. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2 and Test 4: 3. At step 14 and step 31 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_142_1

    testcase TC_142_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
Runs On: SUPLComponent
System: SystemInterfaces

TC_142_2

    testcase TC_142_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
To test SET correctly actions timer UT3 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-142-2 TP version: Test Case Id : SUPL-2.0-con-142 Test Object : Client Test Case Description : To test SET correctly actions timer UT3 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: Triggered session Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 9. Start a SI Periodic Triggered Location Session 10. The SET sends SUPL TRIGGERED START 11. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 12. When the first periodic trigger occurs the SET sends SUPL POS INIT 13. A SUPL POS session takes place 14. After the SET sends the final SUPL POS do not respond 15. (After timer UT3 expires (depending on ixit_timer_UT3) the SET will continue to the next trigger in the session) Note that the SET may release the secure connection at this time. 16. When the second periodic trigger occurs the SET sends SUPL POS INIT 17. A SUPL POS session takes place 18. Send SUPL REPORT 19. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2: 3. At step 16 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

TC_143

    testcase TC_143() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x
To test SET correctly actions timer UT7
Purpose: SUPL-2.0-con-143 TP version: Test Case Id : SUPL-2.0-con-143 Test Object : Client Test Case Description : To test SET correctly actions timer UT7 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ((ics_periodic_SET_initiated OR ics_event_SET_initiated) AND NOT (ics_periodic_Network_initiated OR ics_event_Network_initiated)) AND ixit_timer_UT7 Test Procedure : 1. Start a SI Periodic Triggered Location Session, or a SI Area Event Triggered Location session if Periodic Location sessions are not supported in the SET. 2. Allow the first trigger to occur (either periodic or area event) and the first location session to complete 3. From the SET stop the Triggered Location Session 4. The SET sends SUPL TRIGGERED STOP 5 Do not respond 6. After timer UT7 expires (depending on ixit_timer_UT7) the SET sends SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 7. The Triggered Location Session ends and the SET releases the secure IP connection. Pass-Criteria : 1. At step 6 the SET shall respond with SUPL END with: Status Code not sent or set to any of: unspecified, systemFailure or posMethodFailure. 2. At step 7 the SET shall release the secure IP connection.
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012