OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module SUPL_V2_CommonSteps

Import Declarations:

- LPP_PDU_Definitions
  all
- LibSip_SIPTypesAndValues
  all
- GeoInformation_TypeDefinitions
  all
- RRLP_Components_V10
  all
- SUPL_HTTP_Steps
  all
- SMS_TypeDefinitions
  all
- Tokyo_TypesDefinitions
  all
- SUPL_TypeDefinitions
  all
- SUPL_ExternalSteps
  all
- Tokyo_Templates_RRLP
  all
- SUPL_V2_ExternalSteps
  all
- RRLPV10Types
  all
- SUPLTypes
  all
- SUPL_Postambles
  all
- SUPL_CommonSteps
  all
- SUPL_Preambles
  all
- SUPL_DHCP_DNS_Steps
  all
- SUPL_Parameters
  all
- Tokyo_Templates_LPP
  all
- LibCommon_DataStrings
  all
- RRLP_Templates
  all
- Tokyo_Steps
  all
- SUPL_V2_TypeDefinitions
  all
- RRLP_CommonTypes
  all
- SUPL_V2_Templates
  all
- LPP_Templates
  all
- SUPL_SMS_TypeDefinitions
  all
- RRLPV5Types
  all
- SUPL_Templates
  all
- LibSip_Templates
  all
- SUPL_Configuration
  all
- SUPL_V2_Parameters
  all

Groups:

- externalFunctionGroup
- awaitingMessagesGroup
- sendingMessagesGroup
- PosSessionGroup
- ConfigurationGroup
- Preambles
- Postambles
- Altsteps_group
- checkFunctionsGroup
- helperFunctionsGroup
- dns
- messageGeneration
- con024Flow

Functions Summary
fx_gpsPositionCalculation | calculates a Position value based on the last received SUPL POS
fx_positionIsIn | calculation if a Position estimate value is located within the geographic area
fx_GadLatitude | convertion of latitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
fx_GadLongitude | convertion of logitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
f_awaitSuplPosInit |
f_generateSuplInitwithMAC |
f_sendMTSmsMAC |
f_sendSuplEnd |
f_sendSuplNotify |
f_sendSms |
f_sendSmsInternal |
f_sendSipPushSms |
f_sendSipPushSms_Header |
f_sendUDPSms |
f_sendUDPSms_invalidPort |
f_sendC2KSms |
f_startPosSessionADOnly | Starts and complete a SUPL POS Session with AD only
f_startAndCompletePosSession | Starts and complete a SUPL POS Session with the SET
f_HandleLPPMessages | This function will complete the MO LPP message exchange with LTE device.
f_HandleLPPMessagesUT3Timer | This function will complete the MO LPP message exchange with LTE device to test its UT3 timer.
f_HandleLPPMessagesWithAutonomousGPS | This function will complete the MO LPP message exchange with LTE device using Autonomous GPS(No assistance data sending to UE)
f_ConstructLPPMessageForIncorretSessionID |
f_ProvideAGpsAssistData |
f_RequestLocationInfo |
f_sendPositionReq | Send SUPL POS message with GPS position request, await measurement response
runGPSPosition |
endSession |
f_nwc_action_withtimer | funtion requests handover from NWcontroller
f_resetUePositionStoredInformation |
f_init_SSC |
f_start_SCC |
f_stop_SCC |
f_stop_Communication |
f_restart_Communication |
f_init |
f_initPRS |
f_initPRSNumDLFrames |
f_initPRSConfigurationIndex |
f_initPRSMutingInfoBitLength |
f_initSetNumberOfAntennas |
f_initfinalizePRSConfiguration |
f_initSetTargetAreaCell |
f_initgetCellTimingDelay |
f_initsetCellTimingDelay |
f_initWithTlsVersion |
f_initIntern |
f_initWithDefinedFQDN |
f_initWithDefinedCiphersuite |
f_Postamble |
f_checkPosCapabilitiesParam_againstSET | Checks that the details of the positioning capability parameter contained in incoming ULP-PDU message are consistent with the known positioning capabilities supported by the SET.
f_checkReportingAndServiceCaps_againstSET | Checks that the details of the reporting capability parameter contained in incoming TRIGGERED START message are consistent with the known reporting capabilities supported by the SET.
f_checkServiceCaps_againstSET | Checks that the details of the service capability parameter contained in incoming TRIGGERED START message are consistent with the known service capabilities supported by the SET.
f_checkSET_positionEstimate_displayed | Checks that a position estimate is displayed at the SET
f_checkSET_positionEstimate_displayed_atEnd | Checks that position estimate(s) is displayed at the SET at the end of the test
f_triggerParams2String | Converts a TriggerParams value into a character string
f_areaEventType2String | Converts an AreaEventType value into a character string
f_bool2String | Converts a boolean value into a character string
f_areaList2String | Converts a GeographicTargetAreaList value into a character string
f_areaIdLists2String | Converts an AreaIdLists value into a character string
f_geographicTargetArea2String | Convert a GeographicTargetArea value into a character string representation
f_coordinate2String | Converts a Coordinate value into its character string representation
f_coordinateList2String | Converts a list of coordinates into a correspunding character string representation
f_latitudeSign2String | Converts a latitude sign value into its character string representation
f_areaIdList2String | Converts an AreaIdList value in its character string representation
f_areaIdSet2String | Converts an AreaIdSet value into a character string
f_areaId2String | Converts ans AreaId value in its character string representation
f_geoAreaMappingList2String | Converts a GeoAreaMappingList into its character string representation
f_SLPAddressIP |
dnsService |
f_generateCompletedSessionId | generates a SUPL session ID depending on the receiving SUPL session ID (used to get the SET session ID) and a SLP session will be added
flowFor024 |
encodingType2Name |
getFormatIndicator |
getRequestorIdValueForFormatIndicator |
getClientNameValueForFormatIndicator |
isFormatIndicatorSupported |

Altsteps Summary
a_receiveSuplReportIsIn | await SUPL_REPORT due to the expected area event (SET is in area)
a_receiveSuplReportIsOut | await SUPL_REPORT due to the expected area event (SET is out of area)
a_receiveSuplReportIsInArea | await SUPL_REPORT due to the expected area event (SET is in of cell)
a_receiveSuplReportIsOutArea | await SUPL_REPORT due to the expected area event (SET is out of cell)
a_acceptConnectionRelease |
a_receiveSuplPosInitSETbased |
a_receiveSuplPosInitSETbasedAndRepeat |
a_receiveSuplPosInitSETassisted |
a_receiveSuplPosInitSETassistedAndRepeat |
a_acceptSuplEnd |
a_acceptSessionStoppedSuplEnd |
a_unexpectedAfterSuplInit | unexpected messages from SET that that could occure after SUPL INIT
a_noSUPLmessagebySET | SUPL messages from SET not accepted for location session

## Details

fx_gpsPositionCalculation

    external function fx_gpsPositionCalculation(in ULP_PDU p_supl_pos, in integer p_gpsTOW, in GNSSScenario p_GNSSScenario, in integer p_rrlpVersion, out SUPLTypes.PositionEstimate p_PositionEstimate) return boolean;

Declared in group externalFunctionGroup
calculates a Position value based on the last received SUPL POS
Returns: boolean - Position of SET
Parameters:

- p_supl_pos -
- p_gpsTOW -
- p_GNSSScenario -
- p_rrlpVersion -
- p_PositionEstimate -

fx_positionIsIn

    external function fx_positionIsIn(in SUPLTypes.PositionEstimate p_positionEstimate,
    in GeographicTargetArea p_geographicTargetArea) return boolean;

Declared in group externalFunctionGroup
calculation if a Position estimate value is located within the geographic area
Returns: boolean - true if estimate is in the area
Parameters:

- p_positionEstimate -
- p_geographicTargetArea -

fx_GadLatitude

    external function fx_GadLatitude(float coordinate) return integer;

Declared in group externalFunctionGroup
convertion of latitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
Returns: integer - integer
Parameters:

- coordinate -

fx_GadLongitude

    external function fx_GadLongitude(float coordinate) return integer;

Declared in group externalFunctionGroup
convertion of logitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
Returns: integer - integer
Parameters:

- coordinate -

f_awaitSuplPosInit

    function f_awaitSuplPosInit (in template UlpMessage p_suplInit)
                                    runs on SUPLComponent return ULP_PDU

Declared in group awaitingMessagesGroup
Runs On: SUPLComponent
Returns: ULP_PDU -
Parameters:

- p_suplInit -

f_generateSuplInitwithMAC

    function f_generateSuplInitwithMAC(_0BasicProtectionParams p_keyIdentifier, _0BasicProtectionParams0 p_basicReplyCounter, HMACHash p_hash) runs on SUPLComponent return ULP_PDU

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: ULP_PDU -
Parameters:

- p_keyIdentifier -
- p_basicReplyCounter -
- p_hash -

f_sendMTSmsMAC

    function f_sendMTSmsMAC(_0BasicProtectionParams p_keyIdentifier, _0BasicProtectionParams0 p_basicReplyCounter, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_keyIdentifier -
- p_basicReplyCounter -
- p_hash -

f_sendSuplEnd

    function f_sendSuplEnd(UlpMessage p_suplEnd, SessionID p_sessionId) runs on SUPLComponent

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_suplEnd -
- p_sessionId -

f_sendSuplNotify

    function f_sendSuplNotify(SessionID p_sessionId, NotificationType p_notificationType) runs on SUPLComponent

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_sessionId -
- p_notificationType -

f_sendSms

    function f_sendSms(template ULP_PDU p_suplInit) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -

f_sendSmsInternal

    function f_sendSmsInternal(template ULP_PDU p_suplInit, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -

f_sendSipPushSms

    function f_sendSipPushSms(template ULP_PDU p_suplInit, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -

f_sendSipPushSms_Header

    function f_sendSipPushSms_Header(template ULP_PDU p_suplInit, HMACHash p_hash, SipUrl p_SipUrl, MessageHeader p_messageHeader) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -
- p_SipUrl -
- p_messageHeader -

f_sendUDPSms

    function f_sendUDPSms(template ULP_PDU p_suplInit, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -

f_sendUDPSms_invalidPort

    function f_sendUDPSms_invalidPort(template ULP_PDU p_suplInit, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -

f_sendC2KSms

    function f_sendC2KSms(template ULP_PDU p_suplInit, HMACHash p_hash) runs on SUPLComponent return octetstring

Declared in group sendingMessagesGroup
Runs On: SUPLComponent
Returns: octetstring -
Parameters:

- p_suplInit -
- p_hash -

f_startPosSessionADOnly

    function f_startPosSessionADOnly(ULP_PDU p_ulpPdu,SessionID p_sessionId, RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent
      return UlpMessage

Declared in group PosSessionGroup
Starts and complete a SUPL POS Session with AD only
Runs On: SUPLComponent
Returns: UlpMessage - a Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_ulpPdu -
- p_sessionId -
- p_methodType -
- p_commonIEsRequestLocationInformation -

f_startAndCompletePosSession

    function f_startAndCompletePosSession(ULP_PDU p_ulpPdu,SessionID p_sessionId, template (omit)RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent return UlpMessage

Declared in group PosSessionGroup
Starts and complete a SUPL POS Session with the SET
Runs On: SUPLComponent
Returns: UlpMessage - a Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_ulpPdu -
- p_sessionId -
- p_methodType -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessages

    function f_HandleLPPMessages (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device.
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessagesUT3Timer

    function f_HandleLPPMessagesUT3Timer (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device to test its UT3 timer.
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessagesWithAutonomousGPS

    function f_HandleLPPMessagesWithAutonomousGPS (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device using Autonomous GPS(No assistance data sending to UE)
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_ConstructLPPMessageForIncorretSessionID

    function f_ConstructLPPMessageForIncorretSessionID () runs on SUPLComponent return LPP_Messages

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: LPP_Messages -

f_ProvideAGpsAssistData

    function f_ProvideAGpsAssistData (A_GNSS_RequestAssistanceData p_RequestAssistData ) runs on SUPLComponent   return A_GNSS_ProvideAssistanceData

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: A_GNSS_ProvideAssistanceData -
Parameters:

- p_RequestAssistData -

f_RequestLocationInfo

    function f_RequestLocationInfo( template(value) CommonIEsRequestLocationInformation commonIEsRequestLocationInformation_data) runs on SUPLComponent   return RequestLocationInformation

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: RequestLocationInformation -
Parameters:

- commonIEsRequestLocationInformation_data -

f_sendPositionReq

    function f_sendPositionReq(SessionID p_sessionId, RRLP_CommonTypes.MethodType p_methodType) runs on SUPLComponent return UlpMessage

Declared in group PosSessionGroup
Send SUPL POS message with GPS position request, await measurement response
Runs On: SUPLComponent
Returns: UlpMessage - SUPL REPORT message to complete the Position session
Parameters:

- p_sessionId -
- p_methodType -

runGPSPosition

    function runGPSPosition(PosMethod p_prefMethod, boolean p_hasAGPSassisted, boolean p_hasAGPSbased, RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_prefMethod -
- p_hasAGPSassisted -
- p_hasAGPSbased -
- p_methodType -
- p_commonIEsRequestLocationInformation -

endSession

    function endSession() runs on SUPLComponent

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: void -

f_nwc_action_withtimer

    function f_nwc_action_withtimer(in TargetAreaCell p_targetAreaCell, in MMIMessage p_mmiMessage, in float p_timer) runs on SUPLComponent

Declared in group ConfigurationGroup
funtion requests handover from NWcontroller
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_targetAreaCell -
- p_mmiMessage - message text if no automation at the port
- p_timer - delay time after handover command

f_resetUePositionStoredInformation

    function f_resetUePositionStoredInformation(ResetType p_resetType) runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_resetType -

f_init_SSC

    function f_init_SSC(GNSSScenario p_GNSSScenario) runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -

f_start_SCC

    function f_start_SCC() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_stop_SCC

    function f_stop_SCC() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_stop_Communication

    function f_stop_Communication() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_restart_Communication

    function f_restart_Communication() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_init

    function f_init(GNSSScenario p_GNSSScenario) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -

f_initPRS

    function f_initPRS(PRSBandwidth p_PRSBandwidth) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_PRSBandwidth -

f_initPRSNumDLFrames

    function f_initPRSNumDLFrames(NoDLFrames p_NumDLFrames) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_NumDLFrames -

f_initPRSConfigurationIndex

    function f_initPRSConfigurationIndex(integer p_ConfigurationIndex) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_ConfigurationIndex -

f_initPRSMutingInfoBitLength

    function f_initPRSMutingInfoBitLength(PRSMutingInfoBitLength p_MutingInfoBitLength) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_MutingInfoBitLength -

f_initSetNumberOfAntennas

    function f_initSetNumberOfAntennas(NumAntennas p_NumberOfAntennas) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_NumberOfAntennas -

f_initfinalizePRSConfiguration

    function f_initfinalizePRSConfiguration() runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -

f_initSetTargetAreaCell

    function f_initSetTargetAreaCell(TargetAreaCell p_TargetAreaCell) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_TargetAreaCell -

f_initgetCellTimingDelay

    function f_initgetCellTimingDelay() runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -

f_initsetCellTimingDelay

    function f_initsetCellTimingDelay(integer p_CellTimingDelay) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_CellTimingDelay -

f_initWithTlsVersion

    function f_initWithTlsVersion(GNSSScenario p_GNSSScenario, TlsVersionConfig p_tlsVersion, ResetType p_resetType := agps) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -
- p_tlsVersion -
- p_resetType -

f_initIntern

    function f_initIntern(in boolean withDNSSimulation, in boolean withBSFSimulation, in charstring p_slpFqdn, CipherSuites usedCipherSuite, TlsVersionConfig p_tlsVersion) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- withDNSSimulation -
- withBSFSimulation -
- p_slpFqdn -
- usedCipherSuite -
- p_tlsVersion -

f_initWithDefinedFQDN

    function f_initWithDefinedFQDN(GNSSScenario p_GNSSScenario, in boolean p_withDNSSimulation, in charstring p_slpFqdn) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -
- p_withDNSSimulation -
- p_slpFqdn -

f_initWithDefinedCiphersuite

    function f_initWithDefinedCiphersuite(GNSSScenario p_GNSSScenario, in CipherSuites p_usedCipherSuite) runs on SUPLComponent

Declared in group Preambles
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -
- p_usedCipherSuite -

f_Postamble

    function f_Postamble() runs on SUPLComponent

Declared in group Postambles
Runs On: SUPLComponent
Returns: void -

f_checkPosCapabilitiesParam_againstSET

    function f_checkPosCapabilitiesParam_againstSET(ULP_PDU p_inPDU)
    runs on SUPLComponent return boolean

Declared in group checkFunctionsGroup
Checks that the details of the positioning capability parameter contained in incoming ULP-PDU message are consistent with the known positioning capabilities supported by the SET.
Runs On: SUPLComponent
Returns: boolean - true if the details are consistent, false otherwise
Parameters:

- p_inPDU -

f_checkReportingAndServiceCaps_againstSET

    function f_checkReportingAndServiceCaps_againstSET(ULP_PDU p_inPDU)
    return boolean

Declared in group checkFunctionsGroup
Checks that the details of the reporting capability parameter contained in incoming TRIGGERED START message are consistent with the known reporting capabilities supported by the SET. Also checks that if present, the reporting capabilities parameters are consistent with the known reporting capabilities supported by the SET
Returns: boolean -
Parameters:

- p_inPDU -

f_checkServiceCaps_againstSET

    function f_checkServiceCaps_againstSET(ULP_PDU p_inPDU)
    return boolean

Declared in group checkFunctionsGroup
Checks that the details of the service capability parameter contained in incoming TRIGGERED START message are consistent with the known service capabilities supported by the SET. Do not check the reporting capabilities
Returns: boolean -
Parameters:

- p_inPDU -

f_checkSET_positionEstimate_displayed

    function f_checkSET_positionEstimate_displayed(AreaEventType p_eventKind, charstring p_context)
    runs on SUPLComponent return boolean

Declared in group checkFunctionsGroup
Checks that a position estimate is displayed at the SET
Runs On: SUPLComponent
Returns: boolean - boolean
Parameters:

- p_eventKind -
- p_context -

f_checkSET_positionEstimate_displayed_atEnd

    function f_checkSET_positionEstimate_displayed_atEnd(AreaEventType p_eventKind, charstring p_context)
    runs on SUPLComponent return boolean

Declared in group checkFunctionsGroup
Checks that position estimate(s) is displayed at the SET at the end of the test
Runs On: SUPLComponent
Returns: boolean - boolean
Parameters:

- p_eventKind -
- p_context -

f_triggerParams2String

    function f_triggerParams2String(TriggerParams p_params) runs on SUPLComponent return charstring

Declared in group helperFunctionsGroup
Converts a TriggerParams value into a character string
Runs On: SUPLComponent
Returns: charstring - A character string representation of the provided value
Parameters:

- p_params - The value to convert

f_areaEventType2String

    function f_areaEventType2String(AreaEventType p_areaEventType) return charstring

Declared in group helperFunctionsGroup
Converts an AreaEventType value into a character string
Returns: charstring - A character string representation of the provided value
Parameters:

- p_areaEventType -

f_bool2String

    function f_bool2String(boolean boolVal) return charstring

Declared in group helperFunctionsGroup
Converts a boolean value into a character string
Returns: charstring - A character string representation of the provided value
Parameters:

- boolVal - The boolean value to convert

f_areaList2String

    function f_areaList2String(GeographicTargetAreaList aList) return charstring

Declared in group helperFunctionsGroup
Converts a GeographicTargetAreaList value into a character string
Returns: charstring - A character string representation of the provided value
Parameters:

- aList -

f_areaIdLists2String

    function f_areaIdLists2String(_0AreaEventParams1 areaIdLists) return charstring

Declared in group helperFunctionsGroup
Converts an AreaIdLists value into a character string
Returns: charstring - A character string representation of the provided value
Parameters:

- areaIdLists -

f_geographicTargetArea2String

    function f_geographicTargetArea2String(GeographicTargetArea area) return charstring

Declared in group helperFunctionsGroup
Convert a GeographicTargetArea value into a character string representation
Returns: charstring -
Parameters:

- area -

f_coordinate2String

    function f_coordinate2String(Coordinate coordinate)  return charstring

Declared in group helperFunctionsGroup
Converts a Coordinate value into its character string representation
Returns: charstring -
Parameters:

- coordinate -

f_coordinateList2String

    function f_coordinateList2String(PolygonDescription coordList)  return charstring

Declared in group helperFunctionsGroup
Converts a list of coordinates into a correspunding character string representation
Returns: charstring -
Parameters:

- coordList -

f_latitudeSign2String

    function f_latitudeSign2String(_0Coordinate latSign) return charstring

Declared in group helperFunctionsGroup
Converts a latitude sign value into its character string representation
Returns: charstring -
Parameters:

- latSign -

f_areaIdList2String

    function f_areaIdList2String(AreaIdList idList)  return charstring

Declared in group helperFunctionsGroup
Converts an AreaIdList value in its character string representation
Returns: charstring -
Parameters:

- idList -

f_areaIdSet2String

    function f_areaIdSet2String(AreaIdSet areaIds) return charstring

Declared in group helperFunctionsGroup
Converts an AreaIdSet value into a character string
Returns: charstring - A character string representation of the provided value
Parameters:

- areaIds -

f_areaId2String

    function f_areaId2String(AreaId areaId) return charstring

Declared in group helperFunctionsGroup
Converts ans AreaId value in its character string representation
Returns: charstring -
Parameters:

- areaId -

f_geoAreaMappingList2String

    function f_geoAreaMappingList2String(GeoAreaMappingList areaMappings) return charstring

Declared in group helperFunctionsGroup
Converts a GeoAreaMappingList into its character string representation
Returns: charstring -
Parameters:

- areaMappings -

f_SLPAddressIP

    function f_SLPAddressIP () return IPAddress

Declared in group helperFunctionsGroup
Returns: IPAddress -

dnsService

    function dnsService(template charstring p_slpFQDN) runs on SUPLComponent

Declared in group dns
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_slpFQDN -

f_generateCompletedSessionId

    function f_generateCompletedSessionId(template SessionID p_sessionId, in slpSessionIdFormat p_slpSessionIdFormat, in octetstring slpSessionId) return SessionID

Declared in group messageGeneration
generates a SUPL session ID depending on the receiving SUPL session ID (used to get the SET session ID) and a SLP session will be added
Returns: SessionID -
Parameters:

- p_sessionId - The 'SessionId' from any receiving SUPL message.
- p_slpSessionIdFormat -
- slpSessionId - A given Session Id to ensure e.g. different Session Id's'

flowFor024

    function flowFor024(EncodingType p_encodingType, FormatIndicator p_formatIndicator) runs on SUPLComponent

Declared in group con024Flow
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_encodingType -
- p_formatIndicator -

encodingType2Name

    function encodingType2Name(EncodingType p_encodingType) return charstring

Declared in group con024Flow
Returns: charstring -
Parameters:

- p_encodingType -

getFormatIndicator

    function getFormatIndicator(integer p_count) runs on SUPLComponent return FormatIndicator

Declared in group con024Flow
Runs On: SUPLComponent
Returns: FormatIndicator -
Parameters:

- p_count -

getRequestorIdValueForFormatIndicator

    function getRequestorIdValueForFormatIndicator(in FormatIndicator p_formatIndicator) runs on SUPLComponent return charstring

Declared in group con024Flow
Runs On: SUPLComponent
Returns: charstring -
Parameters:

- p_formatIndicator -

getClientNameValueForFormatIndicator

    function getClientNameValueForFormatIndicator(in FormatIndicator p_formatIndicator) runs on SUPLComponent return charstring

Declared in group con024Flow
Runs On: SUPLComponent
Returns: charstring -
Parameters:

- p_formatIndicator -

isFormatIndicatorSupported

    function isFormatIndicatorSupported(FormatIndicator p_formatIndicator) runs on SUPLComponent return boolean

Declared in group con024Flow
Runs On: SUPLComponent
Returns: boolean -
Parameters:

- p_formatIndicator -

a_receiveSuplReportIsIn

    altstep a_receiveSuplReportIsIn () runs on SUPLComponent

Declared in group Altsteps_group
await SUPL_REPORT due to the expected area event (SET is in area)
Runs On: SUPLComponent
Returns: void -

a_receiveSuplReportIsOut

    altstep a_receiveSuplReportIsOut () runs on SUPLComponent

Declared in group Altsteps_group
await SUPL_REPORT due to the expected area event (SET is out of area)
Runs On: SUPLComponent
Returns: void -

a_receiveSuplReportIsInArea

    altstep a_receiveSuplReportIsInArea (template AreaId v_areaId) runs on SUPLComponent

Declared in group Altsteps_group
await SUPL_REPORT due to the expected area event (SET is in of cell)
Runs On: SUPLComponent
Returns: void -
Parameters:

- v_areaId -

a_receiveSuplReportIsOutArea

    altstep a_receiveSuplReportIsOutArea (template AreaId v_areaId) runs on SUPLComponent

Declared in group Altsteps_group
await SUPL_REPORT due to the expected area event (SET is out of cell)
Runs On: SUPLComponent
Returns: void -
Parameters:

- v_areaId -

a_acceptConnectionRelease

    altstep a_acceptConnectionRelease() runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_receiveSuplPosInitSETbased

    altstep a_receiveSuplPosInitSETbased () runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_receiveSuplPosInitSETbasedAndRepeat

    altstep a_receiveSuplPosInitSETbasedAndRepeat () runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_receiveSuplPosInitSETassisted

    altstep a_receiveSuplPosInitSETassisted () runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_receiveSuplPosInitSETassistedAndRepeat

    altstep a_receiveSuplPosInitSETassistedAndRepeat () runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_acceptSuplEnd

    altstep
     a_acceptSuplEnd() runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_acceptSessionStoppedSuplEnd

    altstep a_acceptSessionStoppedSuplEnd() runs on SUPLComponent

Declared in group Altsteps_group
Runs On: SUPLComponent
Returns: void -

a_unexpectedAfterSuplInit

    altstep a_unexpectedAfterSuplInit() runs on SUPLComponent

Declared in group Altsteps_group
unexpected messages from SET that that could occure after SUPL INIT
Runs On: SUPLComponent
Returns: void -

a_noSUPLmessagebySET

    altstep a_noSUPLmessagebySET(SessionID p_sessionID) runs on SUPLComponent

Declared in group Altsteps_group
SUPL messages from SET not accepted for location session
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_sessionID -

© Copyright Testing Technologies IST GmbH 2012