OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_07x

Declared in module SUPL_V2_SLP_INITIATED_Tests
Subgroups: TC_070, TC_071, TC_072_, TC_073_, TC_074_

Test cases Summary
TC_070_1 |
TC_070_2 | To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session).
TC_070_3 |
TC_070_4 | To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session).
TC_071_1 |
TC_071_2 | To test SET coorectly actions timer UT3 - Test 2: Triggered session.
TC_072 |
TC_073 | To test SET correctly actions timer UT7
TC_074 | To test SET correctly actions timer UT8

## Details

TC_070_1

    testcase TC_070_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_070
Runs On: SUPLComponent
System: SystemInterfaces

TC_070_2

    testcase TC_070_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_070
To test SET correctly actions timer UT2 - Test 2: SUPL POS session (Triggered session). Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS
Runs On: SUPLComponent
System: SystemInterfaces

TC_070_3

    testcase TC_070_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_070
Runs On: SUPLComponent
System: SystemInterfaces

TC_070_4

    testcase TC_070_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_070
To test SET correctly actions timer UT2 - Test 4: No SUPL POS session (Triggered session). Note: This test case is applicable to SETs that support any triggered service. This test case has been written for a Periodic Triggered Location Session. The case where Periodic Location sessions is not supported in the SET is FFS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_071_1

    testcase TC_071_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_071
Runs On: SUPLComponent
System: SystemInterfaces

TC_071_2

    testcase TC_071_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_071
To test SET coorectly actions timer UT3 - Test 2: Triggered session. Note: This test case is applicable to SETs that support any location method that requires a SUPL PO session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS.
Runs On: SUPLComponent
System: SystemInterfaces

TC_072

    testcase TC_072() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_072_
Runs On: SUPLComponent
System: SystemInterfaces

TC_073

    testcase TC_073() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_073_
To test SET correctly actions timer UT7
Runs On: SUPLComponent
System: SystemInterfaces

TC_074

    testcase TC_074() runs on SUPLComponent system SystemInterfaces

Declared in group TC_07x.TC_074_
To test SET correctly actions timer UT8
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012