OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group suplIxitItemsGroup.triggerParamsGroup

Declared in module SUPL_V2_Parameters

Modulepars Summary
ixit_numberOfReportFixes | (integer) Number of Fixes of position estimate in SUPL REPORT
ixit_numberOfFixes | (integer) Number of Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_intervalBetweenFixes | (integer) interval between Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_startTime | (integer) start time of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_CELL_TYPE | (enumeration) handover refers to which cells (cp tests 051 and 131)
ixit_TEST_GSM_CELL_ID | (integer 0-999) GSM Cell ID used for testing
ixit_TEST_WCDMA_CELL_ID | (integer 0-999) WCDMA ID used for testing
ixit_TEST_LTE_CELL_ID | (BIT STRING(SIZE (29))) LTE ID used for testing
ixit_TEST_CDMA_CELL_ID | refBASEID INTEGER(0.
ixit_TEST_HRPD_CELL_ID | refSECTORID BIT STRING(SIZE (128)), -- HRPD Sector Id
ixit_WCDMA_AREA_ID | WCDMA Area ID

## Details

ixit_numberOfReportFixes

    integer ixit_numberOfReportFixes := 50

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) Number of Fixes of position estimate in SUPL REPORT

ixit_numberOfFixes

    integer ixit_numberOfFixes := 50

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) Number of Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_intervalBetweenFixes

    integer ixit_intervalBetweenFixes := 60

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) interval between Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_startTime

    integer ixit_startTime := 30

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) start time of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_CELL_TYPE

    CellType ixit_CELL_TYPE := WCDMA

Declared in group suplIxitItemsGroup.triggerParamsGroup
(enumeration) handover refers to which cells (cp tests 051 and 131)

ixit_TEST_GSM_CELL_ID

    _0GSMAreaId0 ixit_TEST_GSM_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer 0-999) GSM Cell ID used for testing

ixit_TEST_WCDMA_CELL_ID

    _0WCDMAAreaId0 ixit_TEST_WCDMA_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer 0-999) WCDMA ID used for testing

ixit_TEST_LTE_CELL_ID

    _0LTEAreaId1 ixit_TEST_LTE_CELL_ID := '00000000000000000000000000001'B

Declared in group suplIxitItemsGroup.triggerParamsGroup
(BIT STRING(SIZE (29))) LTE ID used for testing

ixit_TEST_CDMA_CELL_ID

    _0CDMAAreaId1 ixit_TEST_CDMA_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
refBASEID INTEGER(0..65535) OPTIONAL, -- Base Station Id

ixit_TEST_HRPD_CELL_ID

    _0HRPDAreaId ixit_TEST_HRPD_CELL_ID := '00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000'B

Declared in group suplIxitItemsGroup.triggerParamsGroup
refSECTORID BIT STRING(SIZE (128)), -- HRPD Sector Id

ixit_WCDMA_AREA_ID

    WCDMAAreaId ixit_WCDMA_AREA_ID := {
    refMCC := 1,
    refMNC := 1,
    refLAC := 1,
    refUC     := 1
    }

Declared in group suplIxitItemsGroup.triggerParamsGroup
WCDMA Area ID

© Copyright Testing Technologies IST GmbH 2012