OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_10x.TC_103

Declared in module SUPL_V2_SET_INITIATED_Tests

Test cases Summary
TC_103_1 | To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
TC_103_2 | To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X

## Details

TC_103_1

    testcase TC_103_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_103
To test SET correctly accepts compatible Version numbers in SUPL messages - Test 1: Support for higher versions of SUPL 2_X_X
Purpose: SUPL-2.0-con-103-1 TP version: Test Case Id : SUPL-2.0-con-103 Test Object : Client Test Case Description : To test SET correctly accepts compatible Version numbers in SUPL messages Specification Reference : ULP TS 7,9,10 SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : State: Continuation of / Can be tested at the same time as: Prerequisite for this test: o Applicability: Test Procedure : Test 1: Support for higher versions of SUPL 2.X.X 1. Start a SI Location Session 2. In the Common Part of all messages set: Version to: o Maj set to 2 o Min set to a higher value than that supported by the SET o Serv ind set to a higher value than that supported by the SET 3. The SET sends SUPL START 4. Send SUPL RESPONSE with Version set as in step 2. 5. The SET sends SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET 6. The Location Session completes successfully. Pass-Criteria : Test 1 and 2: 1. 1. At step 5 the SET shall respond with SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET
Runs On: SUPLComponent
System: SystemInterfaces

TC_103_2

    testcase TC_103_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_10x.TC_103
To test SET correctly accepts compatible Version numbers in SUPL messages - Test 2: Support for lower versions of SUPL 2_X_X
Purpose: SUPL-2.0-con-103-2 TP version: Test Case Id : SUPL-2.0-con-103 Test Object : Client Test Case Description : To test SET correctly accepts compatible Version numbers in SUPL messages Specification Reference : ULP TS 7,9,10 SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : State: Continuation of / Can be tested at the same time as: Prerequisite for this test: o Applicability: Test Procedure : Test 2: Support for lower versions of SUPL 2.X.X. Only applicable if there exists SUPL V2.X where X>0 1. Start a SI Location Session 2. In the Common Part of all messages set: Version to: o Maj set to 2 o Min set to a lower values than the maximum value supported by the SET o Serv ind set to a lower values than the maximum value supported by the SET 3. The SET sends SUPL START 4. Send SUPL RESPONSE with Version set as in step 2. 5. The SET sends SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET 6. The Location Session completes successfully. Pass-Criteria : Test 1 and 2: 1. 1. At step 5 the SET shall respond with SUPL POS INIT with: In the Common Part, Version set to: o Maj set to 2 o Min set to 0 or correct version supported by the SET o Serv ind set to 0 or correct version supported by the SET
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012