OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_13x.TC_130.TC_130_1

Declared in module SUPL_V2_SET_INITIATED_Tests

Test cases Summary
TC_130_1_1 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_130_1_2 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_130_1_3 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_130_1_4 | To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type

## Details

TC_130_1_1

    testcase TC_130_1_1()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 1: Entering event type
Purpose: SUPL-2.0-con-130-1-1 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 1: Entering event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 1: Entering event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s Test 1: A-GPS SET assisted: 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 1: Entering event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 1: The SET does not immediately display the position estimate as Entering event has not been met. Note however that the SET will eventually respond as described in step 7. 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 1: After one of these sequences the SET displays the position estimate as Entering event has been met. At other times the SET does not display the position estimate as Entering event has not been met. 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_2

    testcase TC_130_1_2()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 2: Inside event type
Purpose: SUPL-2.0-con-130-1-2 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 2: Inside event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 2: Inside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 2: Inside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #1, Case #2: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.75 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred on the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 2: The SET displays the calculated position estimate as Inside event has been met 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7.Case 2: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Inside event has been met 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 4: At step 7: Case 2 and Case 3: After each of these sequences the SET shall display the position estimate at intervals of at least 60 seconds after the display of the previous position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_3

    testcase TC_130_1_3()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 3: Outside event type
Purpose: SUPL-2.0-con-130-1-3 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 3: Outside event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 3: Outside event type Use the static GPS “Tokyo” scenario specified in [3GPP TS 34.108] 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 3: Outside event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 3: The SET displays the calculated position estimate as Outside event has been met 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the position estimate as Outside event has been met 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 2 and Case 3: At intervals of at least 60 seconds (set by Minimum Interval Time) after the display of the previous position estimate, the SET displays the remaining number of position estimates (the total number set by Maximum Number of Reports), and then the SET sends SUPL END Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate Case 2 and Case 3: The SET shall display the calculated position estimate after at least 30 seconds after step 2 or immediately after step 3 if Start Time is not supported 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. Case 2 and Case 3: After each of these sequences the SET shall display the position estimate at intervals of at least 60 seconds after the display of the previous position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement Case 2 and Case 3: At intervals of at least 60 seconds after the display of the previous position estimate, the SET shall display the remaining number of position estimates and then the SET shall send SUPL END
Runs On: SUPLComponent
System: SystemInterfaces

TC_130_1_4

    testcase TC_130_1_4()
    runs on SUPLComponent system SystemInterfaces

Declared in group TC_13x.TC_130.TC_130_1
To test SET correctly performs Area Event reporting using Geographic Target Area - Test 1: A-GPS SET assisted, Case 4: Leaving event type
Purpose: SUPL-2.0-con-130-1-4 TP version: Test Case Id : SUPL-2.0-con-130 Test Object : Client Test Case Description : To test SET correctly performs Area Event reporting using Geographic Target Area Specification Reference : ULP TS 5.2.9 SCR Reference : ULP-PRO-C-033-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : ics_AreaEvent_SET_initiated AND ics_GeoTargetArea AND ics_AGPSSETassisted_SET_initiated Test Procedure : Test 1: A-GPS SET assisted Case 4: Leaving event type Details of GPS scenarios to be used and figures showing locations to aid understanding of test cases: Case 4: Leaving event type Simulate a moving GPS scenario starting at latitude 35.666667 degrees North, longitude 139.77 degrees East and ending at latitude 35.666667 degrees North, longitude 139.75 degrees East, moving with a speed of 8 m/s 1. Start a SI Area Event Triggered Session with the following values set in the application running on the SET or otherwise: - Area Event Type: o Case 4: Leaving event type - Repeated reporting o Minimum Interval Time: 60 seconds o Maximum Number of Reports: 6 - Start Time: If supported: 30 seconds - Stop Time: If supported: 240 seconds - Geographic Target Area List with: o Geographic Target Area set to: - Circular with: Case #3, Case #4: - Coordinate set to: o latitude set to: 35.666667 degrees North o longitude set to: 139.77 degrees East - Radius set to: 1000 meters - Radius-min radius and Radius-max radius not set or set to 1 meter Note that this is an area centred approximately 2km from the coordinates of the GPS “Tokyo” scenario specified in [3GPP TS 34.108] - Area Id Lists not set 2. The SET sends SUPL TRIGGERED START with: - Trigger Type set to Area Event - The details of the Reporting Capability parameter consistent with the known reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters are consistent with the known reporting capabilities supported by the SET. 3. Send SUPL TRIGGERED RESPONSE with: - Positioning Method set to A-GPS SET assisted. - Trigger Params not set Note that the SET may release the secure connection at this point. 4. At any time: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position Note that the SET may release the secure connection at this point. 5. After at least 30 seconds (set by Start Time) after step 2, or immediately after step 4 if Start Time is not supported: Case 4: The SET does not immediately display the position estimate as Leaving event has not been met. Note however that the SET will eventually respond as described in step 7. 6. Until step 8 is reached, the following sequence takes place repeatedly: - The SET responds with SUPL POS INIT and a SUPL POS session takes place - The SUPL POS Session completes successfully - Send SUPL REPORT with the correctly calculated position. Note that the SET may release the secure connection at this point. 7. Case 4: After one of these sequences the SET displays the position estimate as Leaving event has been met. At other times the SET does not display the position estimate as Leaving event has not been met. 8. If Stop Time is supported, the SET sends SUPL END approximately 240 seconds (set by Stop Time) after step 2. If Stop Time is not supported: Case 1 and Case 4: 240 seconds after step 2 send SUPL TRIGGERED STOP (to terminate the test) Pass-Criteria : 1. At step 2: - The Trigger Type shall be set to Area Event - The details of the Reporting Capability parameter shall be consistent with the known Reporting capabilities supported by the SET. - If the SET sends the Service Capabilities parameter in the SET Capabilities then the details of the Services Supported and the Reporting Capabilities parameters shall be consistent with the known reporting capabilities supported by the SET. 2. At step 4 and step 6 the SUPL POS Sessions shall complete successfully 3. At step 5: Case 1and Case 4: The SET shall not display the position estimate 4: At step 7: Case 1and Case 4: After one of these sequences the SET shall display the position estimate. After the others of these sequences the SET shall not display the position estimate. 5. At step 8: If Stop Time is supported the SET shall send SUPL END approximately 240 seconds after step 2.If Stop Time is not supported: Case 1 and Case 4: No requirement
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012