OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module SUPL_V2_Parameters

Import Declarations:

- RRLP_Components_V10
  all
- SUPL_Parameters
  all
- RRLPV5Types
  all
- SUPL_TypeDefinitions
  all
- BSF_XML_TypeDefinitions
  all
- LibCommon_DataStrings
  all
- RRLPV10Types
  all
- SUPLTypes
  all

Groups:

- ParamterTypesGroup
- suplIxitItemsGroup

- triggerParamsGroup
- BatchReport
- SET

- suplIcsItemsGroup

- TransportSMS

Modulepars Summary
ixit_gANSS | (boolean galileo, boolean gloneass) GANSS technology supported
ixit_NwcDataAutomation | (NwcAutomationType) Tester sends NWC commands to MMI or Automation Interface
ixit_SscDataAutomation | (NwcAutomationType) Tester sends SSC commands to MMI or Automation Interface
ixit_emergency_call_required | (ixit_emergency_call_required) SET requires emergency call to accept Emergency Services Location Request
ixit_DEFAULT_NWC_ACTION_MAX_DELAY | (float) Default max delay for NWC actions (over nwcPort interface)
ixit_DEFAULT_MS_BASED_ACCURACY_V5 | (Integer 1-127) Default accuracy value for MS Based method type
ixit_DEFAULT_MS_BASED_ACCURACY_V10 |
ixit_ESLP_FQDN |
ixit_Default_ESLP_FQDN |
ixit_ESLP_IPversion |
ixit_ESLP_IPv4Address |
ixit_ESLP_IPv6Address |
ixit_Default_ESLP_IPversion |
ixit_Default_ESLP_IPv4Address |
ixit_Default_ESLP_IPv6Address |
ixit_Default_SUPL_INIT_ROOT_KEY |
ixit_numberOfReportFixes | (integer) Number of Fixes of position estimate in SUPL REPORT
ixit_numberOfFixes | (integer) Number of Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_intervalBetweenFixes | (integer) interval between Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_startTime | (integer) start time of Periodic Params (TriggerParams) in TRIGGERED RESPONSE
ixit_CELL_TYPE | (enumeration) handover refers to which cells (cp tests 051 and 131)
ixit_TEST_GSM_CELL_ID | (integer 0-999) GSM Cell ID used for testing
ixit_TEST_WCDMA_CELL_ID | (integer 0-999) WCDMA ID used for testing
ixit_TEST_LTE_CELL_ID | (BIT STRING(SIZE (29))) LTE ID used for testing
ixit_TEST_CDMA_CELL_ID | refBASEID INTEGER(0.
ixit_TEST_HRPD_CELL_ID | refSECTORID BIT STRING(SIZE (128)), -- HRPD Sector Id
ixit_WCDMA_AREA_ID | WCDMA Area ID
ixit_BatchReportingAfterNumOfFixes | (integer) Batch report after after a number of fixes per measurements (Batch report Params) in TRIGGERED RESPONSE
ixit_BatchReportingAfterNumOfMinutes | (integer) Batch report after a number of minutes per measurements (Batch report Params) in TRIGGERED RESPONSE
ixit_timer_UT7 | (integer) value of Timer UT7, default = 10s
ixit_timer_UT8 | (integer) value of Timer UT8, default = 10s
ixit_SUPL_MAJ_VERSION | (integer 0-255) Current SUPL major version supported by this test suite
ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX | (integer 0-255) SUPL servind version number higher than maximally supported by SET
ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX | (integer 0-255) SUPL min version number higher than maximally supported by SET
ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX | (integer 0-255) SUPL servind version lower than the maximum value supported by the SET
ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX | (integer 0-255) SUPL min version lower than the maximum value supported by the SET
ixit_SET_MAJ_VERSION | (integer 0-255) The maj version number supported by the SET
ixit_SET_SERVIND_VERSION | (integer 0-255) A server ind version number higher than the one supported by the SUT
ixit_SET_SERVIND_VERSION_V1 | (integer 0-255) A server ind version number higher than the one supported by the SUT (if SUPL V1 selected)
ixit_SET_MIN_VERSION | (integer 0-255) SUPL min version number supported by the SET
ixit_SET_MIN_VERSION_V1 | (integer 0-255) SUPL min version number supported by the SET (if SUPL V1 selected)
ixit_SET_REPORTING_CAP | (ReportingCap) Reporting Capabilities supported by the SET
ixit_SET_SERVICE_SUPPORTED | (serviceSupported) service supported by the SET
ixit_SET_EVENTTRIGGER_CAP | (EventTriggerCap)Event Trigger Capabilities supported by the SET
ixit_SIP_push_user | (charstring) SIP push method request, user
ixit_SIP_push_host | (charstring) SIP push method request, host
ics_AGANSSSETassisted_Galileo_Network_initiated | (boolean) UE supports A-GANSS SET assited Galileo Positioning Method (Network initiated)
ics_AGANSSSETbased_Galileo_Network_initiated | (boolean) UE supports A-GANSS SET based Galileo Positioning Method (Network initiated)
ics_AGANSSSETassisted_GLONASS_Network_initiated | (boolean) UE supports A-GANSS SET assited GLONASS Positioning Method (Network initiated)
ics_AGANSSSETbased_GLONASS_Network_initiated | (boolean) UE supports A-GANSS SET based GLONASS Positioning Method (Network initiated)
ics_autonomousGANSS_Network_initiated | (boolean) UE supports autonomous GNSS Positioning Method in Network initiated session
ics_AGANSSSETassisted_GLONASS_SET_initiated | (boolean) UE supports A-GANSS SET assited GLONASS Positioning Method in SET initiated session
ics_AGANSSSETbased_GLONASS_SET_initiated | (boolean) UE supports A-GANSS SET based GLONASS Positioning Method in SET initiated session
ics_autonomousGANSS_SET_initiated | (boolean) UE supports autonomous GNSS Positioning Method in SET initiated session
ics_AGANSSSETassisted_Galileo_SET_initiated | (boolean) UE supports SET assisted A-GANSS Positioning Method in SET initiated session
ics_AGANSSSETbased_Galileo_SET_initiated | (boolean) UE supports SET based A-GANSS Positioning Method in SET initiated session
ics_AGNSSSETassisted_preferred | (boolean) UE supports SET declares A-GNSS SET-assisted preferred in Pref Method in SUPL START
ics_AGNSSSETbased_preferred | (boolean) UE supports SET declares A-GNSS SET-based preferred in Pref Method in SUPL START
ics_OTDOA_SET_initiated | (boolean) UE supports SET based OTDOA Positioning Method in SET initiated session
ics_OTDOA_Network_initiated | (boolean) UE supports SET based OTDOA Positioning Method in Network initiated session
ics_AreaEvent_Network_initiated | (boolean) Area Event Triggered Service in Network initiated call flows supported
ics_periodic_Network_initiated | (boolean) Periodic trigger in Network initiated call flows supported
ics_quasi_real_time | (boolean) Quasi real time reporting supported
ics_stop_triggered_session | (boolean) Ability to stop Triggered Location Session supported
ics_event_Network_initiated | (boolean) Area Event Triggered Service in Network initiated call flows supported
ics_periodic_SET_initiated | (boolean) Periodic trigger in SET initiated call flows supported
ics_event_SET_initiated | (boolean) Area Event Triggered Service in SET initiated call flows supported
ics_real_time | (boolean) Real time reporting supported
ics_GeoTargetArea | (boolean) Geographic Target Area supported
ics_AreaId | (boolean) Area Id supported
ics_AreaEvent_SET_initiated | (boolean) Area Event initiated at SET
icsStopTimeSupport | (boolean) True, if SUT supports Stop Time
icsStartTimeSupport | (boolean) True, if SUT supports Start Time
ics_support_SUPLV1 | (boolean) True, if SUT supports SUPL V1_0
ics_batch | (boolean) Basic Batch reporting supported
ics_SipPush |
ics_UDP |

Data Types Summary
NwcAutomationType |
SscAutomationType |
CellType |
gANSStechnology |

## Details

ixit_gANSS

    gANSStechnology ixit_gANSS := {false,false}

Declared in group suplIxitItemsGroup
(boolean galileo, boolean gloneass) GANSS technology supported

ixit_NwcDataAutomation

    NwcAutomationType ixit_NwcDataAutomation := OFF

Declared in group suplIxitItemsGroup
(NwcAutomationType) Tester sends NWC commands to MMI or Automation Interface

ixit_SscDataAutomation

    SscAutomationType ixit_SscDataAutomation := OFF

Declared in group suplIxitItemsGroup
(NwcAutomationType) Tester sends SSC commands to MMI or Automation Interface

ixit_emergency_call_required

    boolean ixit_emergency_call_required := false

Declared in group suplIxitItemsGroup
(ixit_emergency_call_required) SET requires emergency call to accept Emergency Services Location Request

ixit_DEFAULT_NWC_ACTION_MAX_DELAY

    float ixit_DEFAULT_NWC_ACTION_MAX_DELAY  := 2.0

Declared in group suplIxitItemsGroup
(float) Default max delay for NWC actions (over nwcPort interface)

ixit_DEFAULT_MS_BASED_ACCURACY_V5

    RRLPV5Types.Accuracy ixit_DEFAULT_MS_BASED_ACCURACY_V5 := 10

Declared in group suplIxitItemsGroup
(Integer 1-127) Default accuracy value for MS Based method type

ixit_DEFAULT_MS_BASED_ACCURACY_V10

    RRLP_Components_V10.Accuracy ixit_DEFAULT_MS_BASED_ACCURACY_V10 := 10

Declared in group suplIxitItemsGroup

ixit_ESLP_FQDN

    FQDN ixit_ESLP_FQDN := "e-slp.spirent-lcs.com"

Declared in group suplIxitItemsGroup

ixit_Default_ESLP_FQDN

    FQDN ixit_Default_ESLP_FQDN := "e-slp.mnc001.mcc001.pub.3gppnetwork.org"

Declared in group suplIxitItemsGroup

ixit_ESLP_IPversion

    integer ixit_ESLP_IPversion := 4

Declared in group suplIxitItemsGroup

ixit_ESLP_IPv4Address

    IPAddress ixit_ESLP_IPv4Address := {ipv4Address:= '01020304'O}

Declared in group suplIxitItemsGroup

ixit_ESLP_IPv6Address

    IPAddress ixit_ESLP_IPv6Address := {ipv6Address:= '000102030405060708090a0b0c0d0e0f'O}

Declared in group suplIxitItemsGroup

ixit_Default_ESLP_IPversion

    integer ixit_Default_ESLP_IPversion := 4

Declared in group suplIxitItemsGroup

ixit_Default_ESLP_IPv4Address

    IPAddress ixit_Default_ESLP_IPv4Address := {ipv4Address:= '01020304'O}

Declared in group suplIxitItemsGroup

ixit_Default_ESLP_IPv6Address

    IPAddress ixit_Default_ESLP_IPv6Address := {ipv6Address:= '000102030405060708090a0b0c0d0e0f'O}

Declared in group suplIxitItemsGroup

ixit_Default_SUPL_INIT_ROOT_KEY

    charstring ixit_Default_SUPL_INIT_ROOT_KEY := "default SUPL INIT ROOT KEY"

Declared in group suplIxitItemsGroup

ixit_numberOfReportFixes

    integer ixit_numberOfReportFixes := 50

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) Number of Fixes of position estimate in SUPL REPORT

ixit_numberOfFixes

    integer ixit_numberOfFixes := 50

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) Number of Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_intervalBetweenFixes

    integer ixit_intervalBetweenFixes := 60

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) interval between Fixes of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_startTime

    integer ixit_startTime := 30

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer) start time of Periodic Params (TriggerParams) in TRIGGERED RESPONSE

ixit_CELL_TYPE

    CellType ixit_CELL_TYPE := WCDMA

Declared in group suplIxitItemsGroup.triggerParamsGroup
(enumeration) handover refers to which cells (cp tests 051 and 131)

ixit_TEST_GSM_CELL_ID

    _0GSMAreaId0 ixit_TEST_GSM_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer 0-999) GSM Cell ID used for testing

ixit_TEST_WCDMA_CELL_ID

    _0WCDMAAreaId0 ixit_TEST_WCDMA_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
(integer 0-999) WCDMA ID used for testing

ixit_TEST_LTE_CELL_ID

    _0LTEAreaId1 ixit_TEST_LTE_CELL_ID := '00000000000000000000000000001'B

Declared in group suplIxitItemsGroup.triggerParamsGroup
(BIT STRING(SIZE (29))) LTE ID used for testing

ixit_TEST_CDMA_CELL_ID

    _0CDMAAreaId1 ixit_TEST_CDMA_CELL_ID := 0

Declared in group suplIxitItemsGroup.triggerParamsGroup
refBASEID INTEGER(0..65535) OPTIONAL, -- Base Station Id

ixit_TEST_HRPD_CELL_ID

    _0HRPDAreaId ixit_TEST_HRPD_CELL_ID := '00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000'B

Declared in group suplIxitItemsGroup.triggerParamsGroup
refSECTORID BIT STRING(SIZE (128)), -- HRPD Sector Id

ixit_WCDMA_AREA_ID

    WCDMAAreaId ixit_WCDMA_AREA_ID := {
    refMCC := 1,
    refMNC := 1,
    refLAC := 1,
    refUC     := 1
    }

Declared in group suplIxitItemsGroup.triggerParamsGroup
WCDMA Area ID

ixit_BatchReportingAfterNumOfFixes

    integer ixit_BatchReportingAfterNumOfFixes := 8

Declared in group suplIxitItemsGroup.BatchReport
(integer) Batch report after after a number of fixes per measurements (Batch report Params) in TRIGGERED RESPONSE

ixit_BatchReportingAfterNumOfMinutes

    integer ixit_BatchReportingAfterNumOfMinutes := 5

Declared in group suplIxitItemsGroup.BatchReport
(integer) Batch report after a number of minutes per measurements (Batch report Params) in TRIGGERED RESPONSE

ixit_timer_UT7

    integer ixit_timer_UT7 := 10

Declared in group suplIxitItemsGroup.SET
(integer) value of Timer UT7, default = 10s

ixit_timer_UT8

    integer ixit_timer_UT8 := 10

Declared in group suplIxitItemsGroup.SET
(integer) value of Timer UT8, default = 10s

ixit_SUPL_MAJ_VERSION

    _0Version ixit_SUPL_MAJ_VERSION := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) Current SUPL major version supported by this test suite

ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX

    _0Version1 ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL servind version number higher than maximally supported by SET

ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX

    _0Version0 ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number higher than maximally supported by SET

ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX

    _0Version1 ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX := 1

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL servind version lower than the maximum value supported by the SET

ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX

    _0Version0 ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX := 1

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version lower than the maximum value supported by the SET

ixit_SET_MAJ_VERSION

    _0Version ixit_SET_MAJ_VERSION := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) The maj version number supported by the SET

ixit_SET_SERVIND_VERSION

    _0Version1 ixit_SET_SERVIND_VERSION := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) A server ind version number higher than the one supported by the SUT

ixit_SET_SERVIND_VERSION_V1

    _0Version1 ixit_SET_SERVIND_VERSION_V1 := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) A server ind version number higher than the one supported by the SUT (if SUPL V1 selected)

ixit_SET_MIN_VERSION

    _0Version1 ixit_SET_MIN_VERSION := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number supported by the SET

ixit_SET_MIN_VERSION_V1

    _0Version1 ixit_SET_MIN_VERSION_V1 := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number supported by the SET (if SUPL V1 selected)

ixit_SET_REPORTING_CAP

    ReportingCap ixit_SET_REPORTING_CAP := {
    minInt := 1,
    maxInt := 1,
    repMode := {
    realtime := true,
    quasirealtime := true,
    batch := true
    },
    batchRepCap := {
    report_position := true,
    report_measurements := true,
    max_num_positions := 1,
    max_num_measurements := 1
    }
    }

Declared in group suplIxitItemsGroup.SET
(ReportingCap) Reporting Capabilities supported by the SET

ixit_SET_SERVICE_SUPPORTED

    ServicesSupported ixit_SET_SERVICE_SUPPORTED := {
    periodicTrigger := true,
    areaEventTrigger := true
    }

Declared in group suplIxitItemsGroup.SET
(serviceSupported) service supported by the SET

ixit_SET_EVENTTRIGGER_CAP

    EventTriggerCapabilities ixit_SET_EVENTTRIGGER_CAP := {
       geoAreaShapesSupported := {
       ellipticalArea := false,
       polygonArea := false
       },
       maxNumGeoAreaSupported := 3,
       maxAreaIdListSupported := 6,
       maxAreaIdSupportedPerList := 256
       }

Declared in group suplIxitItemsGroup.SET
(EventTriggerCap)Event Trigger Capabilities supported by the SET

ixit_SIP_push_user

    charstring ixit_SIP_push_user := ""

Declared in group suplIxitItemsGroup
(charstring) SIP push method request, user

ixit_SIP_push_host

    charstring ixit_SIP_push_host := ""

Declared in group suplIxitItemsGroup
(charstring) SIP push method request, host

ics_AGANSSSETassisted_Galileo_Network_initiated

    boolean ics_AGANSSSETassisted_Galileo_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited Galileo Positioning Method (Network initiated)

ics_AGANSSSETbased_Galileo_Network_initiated

    boolean ics_AGANSSSETbased_Galileo_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based Galileo Positioning Method (Network initiated)

ics_AGANSSSETassisted_GLONASS_Network_initiated

    boolean ics_AGANSSSETassisted_GLONASS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited GLONASS Positioning Method (Network initiated)

ics_AGANSSSETbased_GLONASS_Network_initiated

    boolean ics_AGANSSSETbased_GLONASS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based GLONASS Positioning Method (Network initiated)

ics_autonomousGANSS_Network_initiated

    boolean ics_autonomousGANSS_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports autonomous GNSS Positioning Method in Network initiated session

ics_AGANSSSETassisted_GLONASS_SET_initiated

    boolean ics_AGANSSSETassisted_GLONASS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET assited GLONASS Positioning Method in SET initiated session

ics_AGANSSSETbased_GLONASS_SET_initiated

    boolean ics_AGANSSSETbased_GLONASS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports A-GANSS SET based GLONASS Positioning Method in SET initiated session

ics_autonomousGANSS_SET_initiated

    boolean ics_autonomousGANSS_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports autonomous GNSS Positioning Method in SET initiated session

ics_AGANSSSETassisted_Galileo_SET_initiated

    boolean ics_AGANSSSETassisted_Galileo_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET assisted A-GANSS Positioning Method in SET initiated session

ics_AGANSSSETbased_Galileo_SET_initiated

    boolean ics_AGANSSSETbased_Galileo_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based A-GANSS Positioning Method in SET initiated session

ics_AGNSSSETassisted_preferred

    boolean ics_AGNSSSETassisted_preferred := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET declares A-GNSS SET-assisted preferred in Pref Method in SUPL START

ics_AGNSSSETbased_preferred

    boolean ics_AGNSSSETbased_preferred := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET declares A-GNSS SET-based preferred in Pref Method in SUPL START

ics_OTDOA_SET_initiated

    boolean ics_OTDOA_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based OTDOA Positioning Method in SET initiated session

ics_OTDOA_Network_initiated

    boolean ics_OTDOA_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) UE supports SET based OTDOA Positioning Method in Network initiated session

ics_AreaEvent_Network_initiated

    boolean ics_AreaEvent_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in Network initiated call flows supported

ics_periodic_Network_initiated

    boolean ics_periodic_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Periodic trigger in Network initiated call flows supported

ics_quasi_real_time

    boolean ics_quasi_real_time := true

Declared in group suplIcsItemsGroup
(boolean) Quasi real time reporting supported

ics_stop_triggered_session

    boolean ics_stop_triggered_session := true

Declared in group suplIcsItemsGroup
(boolean) Ability to stop Triggered Location Session supported

ics_event_Network_initiated

    boolean ics_event_Network_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in Network initiated call flows supported

ics_periodic_SET_initiated

    boolean ics_periodic_SET_initiated := false

Declared in group suplIcsItemsGroup
(boolean) Periodic trigger in SET initiated call flows supported

ics_event_SET_initiated

    boolean ics_event_SET_initiated := false

Declared in group suplIcsItemsGroup
(boolean) Area Event Triggered Service in SET initiated call flows supported

ics_real_time

    boolean ics_real_time := true

Declared in group suplIcsItemsGroup
(boolean) Real time reporting supported

ics_GeoTargetArea

    boolean ics_GeoTargetArea := true

Declared in group suplIcsItemsGroup
(boolean) Geographic Target Area supported

ics_AreaId

    boolean ics_AreaId := true

Declared in group suplIcsItemsGroup
(boolean) Area Id supported

ics_AreaEvent_SET_initiated

    boolean ics_AreaEvent_SET_initiated := true

Declared in group suplIcsItemsGroup
(boolean) Area Event initiated at SET

icsStopTimeSupport

    boolean icsStopTimeSupport := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports Stop Time

icsStartTimeSupport

    boolean icsStartTimeSupport := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports Start Time

ics_support_SUPLV1

    boolean ics_support_SUPLV1 := true

Declared in group suplIcsItemsGroup
(boolean) True, if SUT supports SUPL V1_0

ics_batch

    boolean ics_batch := true

Declared in group suplIcsItemsGroup
(boolean) Basic Batch reporting supported

ics_SipPush

    boolean ics_SipPush := true

Declared in group suplIcsItemsGroup.TransportSMS

ics_UDP

    boolean ics_UDP := true

Declared in group suplIcsItemsGroup.TransportSMS

NwcAutomationType

    type enumerated NwcAutomationType {
    OFF,
    AutomationManager
    }

Declared in group ParamterTypesGroup

SscAutomationType

    type enumerated SscAutomationType {
    OFF,
    AutomationManager
    }

Declared in group ParamterTypesGroup

CellType

    type enumerated CellType {
        GSM,
        WCDMA,
        CDMA,
        HRPD,
        LTE
    }

gANSStechnology

    type  record gANSStechnology {boolean galileo, boolean gloneass}

Declared in group ParamterTypesGroup

© Copyright Testing Technologies IST GmbH 2012