OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module MAP_CommonDataTypes_V10

Import Declarations:

- ASNAUX
  all
- MAP_BS_Code_V10
  all
- MAP_SS_Code_V10
  all
- MAP_TS_Code_V10
  all
- MAP_ExtensionDataTypes_V10
  all

Data Types Summary
TBCD_STRING |
DiameterIdentity |
AddressString |
ISDN_AddressString |
FTN_AddressString |
ISDN_SubaddressString |
SignalInfo |
LongSignalInfo |
AlertingPattern |
GSN_Address |
Time |
IMSI |
ASCI_CallReference |
TMSI |
IMEI |
HLR_Id |
HLR_List |
LMSI |
GlobalCellId |
NAEA_CIC |
LCSServiceTypeID |
PLMN_Id |
CellGlobalIdOrServiceAreaIdFixedLength |
LAIFixedLength |
EMLPP_Priority |
MaxMC_Bearers |
MC_Bearers |
Ext_SS_Status |
AgeOfLocationInformation |
ProtocolId |
Ext_ProtocolId |
AccessNetworkProtocolId |
NetworkResource |
AdditionalNetworkResource |
LCSClientInternalID |
ExternalSignalInfo |
Ext_ExternalSignalInfo |
AccessNetworkSignalInfo |
IMSI_WithLMSI |
NAEA_PreferredCI |
LCSClientExternalID |
EMLPP_Info |
MC_SS_Info |
Identity |
SubscriberId |
SubscriberIdentity |
CellGlobalIdOrServiceAreaIdOrLAI |
BasicServiceCode |
Ext_BasicServiceCode |

Constants Summary
maxAddressLength |
maxISDN_AddressLength |
maxFTN_AddressLength |
maxISDN_SubaddressLength |
maxSignalInfoLength |
maxLongSignalInfoLength |
alertingLevel_0 |
alertingLevel_1 |
alertingLevel_2 |
alertingCategory_1 |
alertingCategory_2 |
alertingCategory_3 |
alertingCategory_4 |
alertingCategory_5 |
maxNumOfHLR_Id |
emergencyServices |
emergencyAlertServices |
personTracking |
fleetManagement |
assetManagement |
trafficCongestionReporting |
roadsideAssistance |
routingToNearestCommercialEnterprise |
navigation |
citySightseeing |
localizedAdvertising |
mobileYellowPages |
trafficAndPublicTransportationInfo |
weather |
assetAndServiceFinding |
gaming |
findYourFriend |
dating |
chatting |
routeFinding |
whereAmI |
serv64 |
serv65 |
serv66 |
serv67 |
serv68 |
serv69 |
serv70 |
serv71 |
serv72 |
serv73 |
serv74 |
serv75 |
serv76 |
serv77 |
serv78 |
serv79 |
serv80 |
serv81 |
serv82 |
serv83 |
serv84 |
serv85 |
serv86 |
serv87 |
serv88 |
serv89 |
serv90 |
serv91 |
serv92 |
serv93 |
serv94 |
serv95 |
serv96 |
serv97 |
serv98 |
serv99 |
serv100 |
serv101 |
serv102 |
serv103 |
serv104 |
serv105 |
serv106 |
serv107 |
serv108 |
serv109 |
serv110 |
serv111 |
serv112 |
serv113 |
serv114 |
serv115 |
serv116 |
serv117 |
serv118 |
serv119 |
serv120 |
serv121 |
serv122 |
serv123 |
serv124 |
serv125 |
serv126 |
serv127 |
priorityLevelA |
priorityLevelB |
priorityLevel0 |
priorityLevel1 |
priorityLevel2 |
priorityLevel3 |
priorityLevel4 |
maxNumOfMC_Bearers |

## Details

TBCD_STRING

    TBCD-STRING ::= OCTET STRING
         -- This type (Telephony Binary Coded Decimal String) is used to
         -- represent several digits from 0 through 9, *, #, a, b, c, two
         -- digits per octet, each digit encoded 0000 to 1001 (0 to 9),
         -- 1010 (*), 1011 (#), 1100 (a), 1101 (b) or 1110 (c); 1111 used
         -- as filler when there is an odd number of digits.
         -- bits 8765 of octet n encoding digit 2n
         -- bits 4321 of octet n encoding digit 2(n-1) +1
    DiameterIdentity

DiameterIdentity

    DiameterIdentity ::= OCTET STRING (SIZE(9..55))
    -- content of DiameterIdentity is defined in IETF RFC 3588 [139]
    AddressString

AddressString

    AddressString ::= OCTET STRING (SIZE (1..maxAddressLength))
         -- This type is used to represent a number for addressing
         -- purposes. It is composed of
         --   a)   one octet for nature of address, and numbering plan
         --        indicator.
         --   b)   digits of an address encoded as TBCD-String.
         -- a)     The first octet includes a one bit extension indicator, a
         --        3 bits nature of address indicator and a 4 bits numbering
         --        plan indicator, encoded as follows:
         -- bit 8: 1   (no extension)
         -- bits 765: nature of address indicator
         --   000 unknown
         --   001 international number
         --   010 national significant number
         --   011 network specific number
         --   100 subscriber number
         --   101 reserved
         --   110 abbreviated number
         --   111 reserved for extension
         -- bits 4321: numbering plan indicator
         --   0000 unknown
         --   0001 ISDN/Telephony Numbering Plan (Rec ITU-T E.164)
         --   0010 spare
         --   0011 data numbering plan (ITU-T Rec X.121)
         --   0100 telex numbering plan (ITU-T Rec F.69)
         --   0101 spare
         --   0110 land mobile numbering plan (ITU-T Rec E.212)
         --   0111 spare
         --   1000 national numbering plan
         --   1001 private numbering plan
         --   1111 reserved for extension
         --   all other values are reserved.
         -- b)     The following octets representing digits of an address
         --        encoded as a TBCD-STRING.
    maxAddressLength

ISDN_AddressString

    ISDN-AddressString ::=
                   AddressString (SIZE (1..maxISDN-AddressLength))
         -- This type is used to represent ISDN numbers.
    maxISDN-AddressLength

FTN_AddressString

    FTN-AddressString ::=
                   AddressString (SIZE (1..maxFTN-AddressLength))
         -- This type is used to represent forwarded-to numbers.
         -- If NAI = international the first digits represent the country code (CC)
         -- and the network destination code (NDC) as for E.164.
    maxFTN-AddressLength

ISDN_SubaddressString

    ISDN-SubaddressString ::=
                   OCTET STRING (SIZE (1..maxISDN-SubaddressLength))
         -- This type is used to represent ISDN subaddresses.
         -- It is composed of
         --   a)   one octet for type of subaddress and odd/even indicator.
         --   b)   20 octets for subaddress information.
         --   a)   The first octet includes a one bit extension indicator, a
         --        3 bits type of subaddress and a one bit odd/even indicator,
         --        encoded as follows:
         --   bit 8: 1  (no extension)
         --   bits 765: type of subaddress
         --        000 NSAP  (X.213/ISO 8348 AD2)
         --        010 User  Specified
         --        All other values are reserved
         --   bit 4: odd/even indicator
         --        0 even number of address signals
         --        1 odd number of address signals
         --        The odd/even indicator is used when the type of subaddress
         --        is "user specified" and the coding is BCD.
         --   bits 321: 000 (unused)
         --   b) Subaddress information.
         --   The NSAP X.213/ISO8348AD2 address shall be formatted as specified
         --   by octet 4 which contains the Authority and Format Identifier
         --   (AFI). The encoding is made according to the "preferred binary
         --   encoding" as defined in X.213/ISO834AD2. For the definition
         --   of this type of subaddress, see ITU-T Rec I.334.
         --   For User-specific subaddress, this field is encoded according
         --   to the user specification, subject to a maximum length of 20
         --   octets. When interworking with X.25 networks BCD coding should
         --   be applied.
    maxISDN-SubaddressLength

SignalInfo

    SignalInfo ::= OCTET STRING (SIZE (1..maxSignalInfoLength))
    maxSignalInfoLength

LongSignalInfo

    LongSignalInfo ::= OCTET STRING (SIZE (1..maxLongSignalInfoLength))
    maxLongSignalInfoLength

AlertingPattern

    AlertingPattern ::= OCTET STRING (SIZE (1) )
         -- This type is used to represent Alerting Pattern
         --   bits 8765 : 0000 (unused)
         --   bits 43 : type of Pattern
         --        00 level
         --        01 category
         --        10 category
         --        all other values are reserved.
         --   bits 21 : type of alerting
    alertingLevel-0

GSN_Address

    GSN-Address ::= OCTET STRING (SIZE (5..17))
         -- Octets are coded according to TS 3GPP TS 23.003 [17]
    Time

Time

    Time ::= OCTET STRING (SIZE (4))
         -- Octets are coded according to IETF RFC 3588 [139]
    -- data types for numbering and identification
    IMSI

IMSI

    IMSI ::= TBCD-STRING (SIZE (3..8))
         -- digits of MCC, MNC, MSIN are concatenated in this order.
    Identity

ASCI_CallReference

    ASCI-CallReference ::= TBCD-STRING (SIZE (1..8))
         -- digits of VGCS/VBS-area,Group-ID are concatenated in this order if there is a
         -- VGCS/VBS-area.
    TMSI

TMSI

    TMSI ::= OCTET STRING (SIZE (1..4))
    SubscriberId

IMEI

    IMEI ::=  TBCD-STRING (SIZE (8))
         --   Refers to International Mobile Station Equipment Identity
         --   and Software Version Number (SVN) defined in TS 3GPP TS 23.003 [17].
         --   If the SVN is not present the last octet shall contain the
         --   digit 0 and a filler.
         --   If present the SVN shall be included in the last octet.
    HLR-Id

HLR_Id

    IMSI
     -- leading digits of IMSI, i.e. (MCC, MNC, leading digits of
     -- MSIN) forming HLR Id defined in TS 3GPP TS 23.003 [17].
    HLR-List

HLR_List

    HLR-List ::= SEQUENCE SIZE (1..maxNumOfHLR-Id) OF
                                              HLR-Id
    maxNumOfHLR-Id

LMSI

    LMSI ::= OCTET STRING (SIZE (4))
    GlobalCellId

GlobalCellId

    GlobalCellId ::= OCTET STRING (SIZE (5..7))
         -- Refers to Cell Global Identification defined in TS 3GPP TS 23.003 [17].
         -- The internal structure is defined as follows:
         -- octet 1 bits 4321                 Mobile Country Code 1st digit
         --          bits 8765                Mobile Country Code 2nd digit
         -- octet 2 bits 4321                 Mobile Country Code 3rd digit
         --          bits 8765                Mobile Network Code 3rd digit
         --                                   or filler (1111) for 2 digit MNCs
         -- octet 3 bits 4321                 Mobile Network Code 1st digit
         --          bits 8765                Mobile Network Code 2nd digit
         -- octets 4 and 5                    Location Area Code according to TS 3GPP TS 24.008[35]
         -- octets 6 and 7                    Cell Identity (CI) according to TS 3GPP TS 24.008[35]
    NetworkResource

NAEA_CIC

    NAEA-CIC ::= OCTET STRING (SIZE (3))
         -- The internal structure is defined by the Carrier Identification
         -- parameter in ANSI T1.113.3. Carrier codes between “000” and “999” may
         -- be encoded as 3 digits using “000” to “999” or as 4 digits using
         -- “0000” to “0999”. Carrier codes between “1000” and “9999” are encoded
         -- using 4 digits.
    SubscriberIdentity

LCSServiceTypeID

    LCSServiceTypeID ::= INTEGER (0..127)
         -- the integer values 0-63 are reserved for Standard LCS service types
         -- the integer values 64-127 are reserved for Non Standard LCS service types
    -- Standard LCS Service Types
    emergencyServices

PLMN_Id

    PLMN-Id ::= OCTET STRING (SIZE (3))
         -- The internal structure is defined as follows:
         -- octet 1 bits 4321                 Mobile Country Code 1st digit
         --         bits 8765                 Mobile Country Code 2nd digit
         -- octet 2 bits 4321                 Mobile Country Code 3rd digit
         --         bits 8765                 Mobile Network Code 3rd digit
         --                                   or filler (1111) for 2 digit MNCs
         -- octet 3 bits 4321                 Mobile Network Code 1st digit
         --         bits 8765                 Mobile Network Code 2nd digit
    -- data types for CAMEL
    CellGlobalIdOrServiceAreaIdOrLAI

CellGlobalIdOrServiceAreaIdFixedLength

    CellGlobalIdOrServiceAreaIdFixedLength ::= OCTET STRING (SIZE (7))
         -- Refers to Cell Global Identification or Service Are Identification
         -- defined in 3GPP TS 23.003.
         -- The internal structure is defined as follows:
         -- octet 1 bits 4321                 Mobile Country Code 1st digit
         --         bits 8765                 Mobile Country Code 2nd digit
         -- octet 2 bits 4321                 Mobile Country Code 3rd digit
         --         bits 8765                 Mobile Network Code 3rd digit
         --                                   or filler (1111) for 2 digit MNCs
         -- octet 3 bits 4321                 Mobile Network Code 1st digit
         --         bits 8765                 Mobile Network Code 2nd digit
         -- octets 4 and 5                    Location Area Code according to 3GPP TS 24.008
         -- octets 6 and 7                    Cell Identity (CI) value or
         --                                   Service Area Code (SAC) value
         --                                   according to 3GPP TS 23.003
    LAIFixedLength

LAIFixedLength

    LAIFixedLength ::= OCTET STRING (SIZE (5))
         -- Refers to Location Area Identification defined in 3GPP TS 23.003 [17].
         -- The internal structure is defined as follows:
         -- octet 1 bits 4321                 Mobile Country Code 1st digit
         --         bits 8765                 Mobile Country Code 2nd digit
         -- octet 2 bits 4321                 Mobile Country Code 3rd digit
         --         bits 8765                 Mobile Network Code 3rd digit
         --                                   or filler (1111) for 2 digit MNCs
         -- octet 3 bits 4321                 Mobile Network Code 1st digit
         --         bits 8765                 Mobile Network Code 2nd digit
         -- octets 4 and 5                    Location Area Code according to 3GPP TS 24.008 [35]
    -- data types for subscriber management
    BasicServiceCode

EMLPP_Priority

    EMLPP-Priority ::= INTEGER (0..15)
         -- The mapping from the values A,B,0,1,2,3,4 to the integer-value is
         -- specified as follows where A is the highest and 4 is the lowest
         -- priority level
         -- the integer values 7-15 are spare and shall be mapped to value 4
    priorityLevelA

MaxMC_Bearers

    MaxMC-Bearers ::= INTEGER (2..maxNumOfMC-Bearers)
    MC-Bearers

MC_Bearers

    MC-Bearers ::= INTEGER (1..maxNumOfMC-Bearers)
    maxNumOfMC-Bearers

Ext_SS_Status

    Ext-SS-Status ::= OCTET STRING (SIZE (1..5))
         -- OCTET 1:
         --
         -- bits 8765: 0000 (unused)
         -- bits 4321: Used to convey the "P bit","R bit","A bit" and "Q bit",
         --           representing supplementary service state information
         --           as defined in TS 3GPP TS 23.011 [22]
         -- bit 4: "Q bit"
         -- bit 3: "P bit"
         -- bit 2: "R bit"
         -- bit 1: "A bit"
         -- OCTETS 2-5: reserved for future use. They shall be discarded if
         -- received and not understood.
       -- data types for geographic location
    AgeOfLocationInformation

AgeOfLocationInformation

    AgeOfLocationInformation ::= INTEGER (0..32767)
    -- the value represents the elapsed time in minutes since the last
    -- network contact of the mobile station (i.e. the actuality of the
    -- location information).
    -- value “0” indicates that the MS is currently in contact with the
    --           network
    -- value “32767” indicates that the location information is at least
    --               32767 minutes old
    END

ProtocolId

    ENUMERATED {
     gsm-0408 (1),
     gsm-0806 (2),
     gsm-BSSMAP (3),
     -- Value 3 is reserved and must not be used
     ets-300102-1 (4)}
    Ext-ExternalSignalInfo

Ext_ProtocolId

    ENUMERATED {
     ets-300356 (1),
     ...
      }
    -- exception handling:
    -- For Ext-ExternalSignalInfo sequences containing this parameter with any
    -- other value than the ones listed the receiver shall ignore the whole
    -- Ext-ExternalSignalInfo sequence.
    AccessNetworkSignalInfo

AccessNetworkProtocolId

    ENUMERATED {
     ts3G-48006    (1),
     ts3G-25413 (2),
     ...}
     -- exception handling:
     -- For AccessNetworkSignalInfo sequences containing this parameter with any
     -- other value than the ones listed the receiver shall ignore the whole
     -- AccessNetworkSignalInfo sequence.
    AlertingPattern

NetworkResource

    ENUMERATED {
     plmn (0),
     hlr (1),
     vlr (2),
     pvlr (3),
     controllingMSC (4),
     vmsc (5),
     eir (6),
     rss (7)}
    AdditionalNetworkResource

AdditionalNetworkResource

    ENUMERATED {
     sgsn (0),
     ggsn (1),
     gmlc (2),
     gsmSCF (3),
     nplr (4),
     auc (5),
     ... ,
     ue (6),
     mme (7)}
     -- if unknown value is received in AdditionalNetworkResource
     -- it shall be ignored.
    NAEA-PreferredCI

LCSClientInternalID

    ENUMERATED {
     broadcastService                     (0),
     o-andM-HPLMN                         (1),
     o-andM-VPLMN                         (2),
     anonymousLocation                    (3),
     targetMSsubscribedService            (4),
     ... }
    -- for a CAMEL phase 3 PLMN operator client, the value targetMSsubscribedService shall be used
    LCSServiceTypeID

ExternalSignalInfo

    ExternalSignalInfo ::= SEQUENCE {
         protocolId                           ProtocolId,
         signalInfo                           SignalInfo,
         -- Information about the internal structure is given in
         -- clause 7.6.9.
         extensionContainer                   ExtensionContainer                OPTIONAL,
         -- extensionContainer must not be used in version 2
         ...}
    SignalInfo

Ext_ExternalSignalInfo

    Ext-ExternalSignalInfo ::= SEQUENCE {
         ext-ProtocolId                       Ext-ProtocolId,
         signalInfo                           SignalInfo,
         -- Information about the internal structure is given in
         -- clause 7.6.9.10
         extensionContainer                   ExtensionContainer                OPTIONAL,
         ...}
    Ext-ProtocolId

AccessNetworkSignalInfo

    AccessNetworkSignalInfo ::= SEQUENCE {
         accessNetworkProtocolId              AccessNetworkProtocolId,
         signalInfo                           LongSignalInfo,
         -- Information about the internal structure is given in clause 7.6.9.1
         extensionContainer                   ExtensionContainer                OPTIONAL,
         ...}
    LongSignalInfo

IMSI_WithLMSI

    IMSI-WithLMSI ::= SEQUENCE {
         imsi                                 IMSI,
         lmsi                                 LMSI,
         -- a special value 00000000 indicates that the LMSI is not in use
         ...}
    ASCI-CallReference

NAEA_PreferredCI

    NAEA-PreferredCI ::= SEQUENCE {
         naea-PreferredCIC                    [0] NAEA-CIC,
         extensionContainer                   [1] ExtensionContainer            OPTIONAL,
         ...}
    NAEA-CIC

LCSClientExternalID

    LCSClientExternalID ::= SEQUENCE {
         externalAddress                      [0] ISDN-AddressString            OPTIONAL,
         extensionContainer                   [1] ExtensionContainer            OPTIONAL,
         ... }
    LCSClientInternalID

EMLPP_Info

    EMLPP-Info ::= SEQUENCE {
         maximumentitledPriority              EMLPP-Priority,
         defaultPriority                      EMLPP-Priority,
         extensionContainer                   ExtensionContainer                  OPTIONAL,
         ...}
    EMLPP-Priority

MC_SS_Info

    MC-SS-Info ::= SEQUENCE {
         ss-Code                              [0]  SS-Code,
         ss-Status                            [1]  Ext-SS-Status,
         nbrSB                                [2]  MaxMC-Bearers,
         nbrUser                              [3]  MC-Bearers,
         extensionContainer                   [4]  ExtensionContainer             OPTIONAL,
         ...}
    MaxMC-Bearers

Identity

    Identity ::= CHOICE {
         imsi                                 IMSI,
         imsi-WithLMSI                        IMSI-WithLMSI}
    IMSI-WithLMSI

SubscriberId

    SubscriberId ::= CHOICE {
         imsi                                 [0] IMSI,
         tmsi                                 [1] TMSI}
    IMEI

SubscriberIdentity

    SubscriberIdentity ::= CHOICE {
         imsi                                 [0] IMSI,
         msisdn                               [1] ISDN-AddressString
         }
    LCSClientExternalID

CellGlobalIdOrServiceAreaIdOrLAI

    CellGlobalIdOrServiceAreaIdOrLAI ::= CHOICE {
         cellGlobalIdOrServiceAreaIdFixedLength     [0] CellGlobalIdOrServiceAreaIdFixedLength,
         laiFixedLength                       [1] LAIFixedLength}
    CellGlobalIdOrServiceAreaIdFixedLength

BasicServiceCode

    BasicServiceCode ::= CHOICE {
         bearerService                        [2] BearerServiceCode,
         teleservice                          [3] TeleserviceCode}
    Ext-BasicServiceCode

Ext_BasicServiceCode

    Ext-BasicServiceCode ::= CHOICE {
         ext-BearerService                    [2] Ext-BearerServiceCode,
         ext-Teleservice                      [3] Ext-TeleserviceCode}
    EMLPP-Info

maxAddressLength

    const integer maxAddressLength   INTEGER ::= 20
    ISDN-AddressString

maxISDN_AddressLength

    const integer maxISDN-AddressLength   INTEGER ::= 9
    FTN-AddressString

maxFTN_AddressLength

    const integer maxFTN-AddressLength   INTEGER ::= 15
    ISDN-SubaddressString

maxISDN_SubaddressLength

    const integer maxISDN-SubaddressLength   INTEGER ::= 21
    ExternalSignalInfo

maxSignalInfoLength

    const integer maxSignalInfoLength INTEGER ::= 200
         -- This NamedValue represents the theoretical maximum number of octets which is
         -- available to carry a single instance of the SignalInfo data type,
         -- without requiring segmentation to cope with the network layer service.
         -- However, the actual maximum size available for an instance of the data
         -- type may be lower, especially when other information elements
         -- have to be included in the same component.
    ProtocolId

maxLongSignalInfoLength

    const integer maxLongSignalInfoLength INTEGER ::= 2560
         -- This Named Value represents the maximum number of octets which is available
         -- to carry a single instance of the LongSignalInfo data type using
         -- White Book SCCP with the maximum number of segments.
         -- It takes account of the octets used by the lower layers of the protocol, and
         -- other information elements which may be included in the same component.
    AccessNetworkProtocolId

alertingLevel_0

    const AlertingPattern alertingLevel-0    AlertingPattern ::= '00000000'B
    alertingLevel-1

alertingLevel_1

    const AlertingPattern alertingLevel-1    AlertingPattern ::= '00000001'B
    alertingLevel-2

alertingLevel_2

    const AlertingPattern alertingLevel-2    AlertingPattern ::= '00000010'B
         -- all other values of Alerting level are reserved
         -- Alerting Levels are defined in GSM 02.07
    alertingCategory-1

alertingCategory_1

    const AlertingPattern alertingCategory-1    AlertingPattern ::= '00000100'B
    alertingCategory-2

alertingCategory_2

    const AlertingPattern alertingCategory-2    AlertingPattern ::= '00000101'B
    alertingCategory-3

alertingCategory_3

    const AlertingPattern alertingCategory-3    AlertingPattern ::= '00000110'B
    alertingCategory-4

alertingCategory_4

    const AlertingPattern alertingCategory-4    AlertingPattern ::= '00000111'B
    alertingCategory-5

alertingCategory_5

    const AlertingPattern alertingCategory-5    AlertingPattern ::= '00001000'B
         -- all other values of Alerting Category are reserved
         -- Alerting categories are defined in GSM 02.07
    GSN-Address

maxNumOfHLR_Id

    const integer maxNumOfHLR-Id   INTEGER ::= 50
    LMSI

emergencyServices

    const LCSServiceTypeID emergencyServices                              LCSServiceTypeID ::= 0
    emergencyAlertServices

emergencyAlertServices

    const LCSServiceTypeID emergencyAlertServices                         LCSServiceTypeID ::= 1
    personTracking

personTracking

    const LCSServiceTypeID personTracking                                 LCSServiceTypeID ::= 2
    fleetManagement

fleetManagement

    const LCSServiceTypeID fleetManagement                                LCSServiceTypeID ::= 3
    assetManagement

assetManagement

    const LCSServiceTypeID assetManagement                                LCSServiceTypeID ::= 4
    trafficCongestionReporting

trafficCongestionReporting

    const LCSServiceTypeID trafficCongestionReporting                     LCSServiceTypeID ::= 5
    roadsideAssistance

roadsideAssistance

    const LCSServiceTypeID roadsideAssistance                             LCSServiceTypeID ::= 6
    routingToNearestCommercialEnterprise

routingToNearestCommercialEnterprise

    const LCSServiceTypeID routingToNearestCommercialEnterprise           LCSServiceTypeID ::= 7
    navigation

navigation

    const LCSServiceTypeID navigation                                     LCSServiceTypeID ::= 8
         --this service type is reserved for use in previous releases
    citySightseeing

citySightseeing

    const LCSServiceTypeID citySightseeing                                LCSServiceTypeID ::= 9
    localizedAdvertising

localizedAdvertising

    const LCSServiceTypeID localizedAdvertising                           LCSServiceTypeID ::= 10
    mobileYellowPages

mobileYellowPages

    const LCSServiceTypeID mobileYellowPages                              LCSServiceTypeID ::= 11
    trafficAndPublicTransportationInfo

trafficAndPublicTransportationInfo

    const LCSServiceTypeID trafficAndPublicTransportationInfo             LCSServiceTypeID ::= 12
    weather

weather

    const LCSServiceTypeID weather                                        LCSServiceTypeID ::= 13
    assetAndServiceFinding

assetAndServiceFinding

    const LCSServiceTypeID assetAndServiceFinding                         LCSServiceTypeID ::= 14
    gaming

gaming

    const LCSServiceTypeID gaming                                         LCSServiceTypeID ::= 15
    findYourFriend

findYourFriend

    const LCSServiceTypeID findYourFriend                                 LCSServiceTypeID ::= 16
    dating

dating

    const LCSServiceTypeID dating                                         LCSServiceTypeID ::= 17
    chatting

chatting

    const LCSServiceTypeID chatting                                       LCSServiceTypeID ::= 18
    routeFinding

routeFinding

    const LCSServiceTypeID routeFinding                                   LCSServiceTypeID ::= 19
    whereAmI

whereAmI

    const LCSServiceTypeID whereAmI                                       LCSServiceTypeID ::= 20
    -- The values of LCSServiceTypeID are defined according to 3GPP TS 22.071.
    -- Non Standard LCS Service Types
    serv64

serv64

    const LCSServiceTypeID serv64                                         LCSServiceTypeID ::= 64
    serv65

serv65

    const LCSServiceTypeID serv65                                         LCSServiceTypeID ::= 65
    serv66

serv66

    const LCSServiceTypeID serv66                                         LCSServiceTypeID ::= 66
    serv67

serv67

    const LCSServiceTypeID serv67                                         LCSServiceTypeID ::= 67
    serv68

serv68

    const LCSServiceTypeID serv68                                         LCSServiceTypeID ::= 68
    serv69

serv69

    const LCSServiceTypeID serv69                                         LCSServiceTypeID ::= 69
    serv70

serv70

    const LCSServiceTypeID serv70                                         LCSServiceTypeID ::= 70
    serv71

serv71

    const LCSServiceTypeID serv71                                         LCSServiceTypeID ::= 71
    serv72

serv72

    const LCSServiceTypeID serv72                                         LCSServiceTypeID ::= 72
    serv73

serv73

    const LCSServiceTypeID serv73                                         LCSServiceTypeID ::= 73
    serv74

serv74

    const LCSServiceTypeID serv74                                         LCSServiceTypeID ::= 74
    serv75

serv75

    const LCSServiceTypeID serv75                                         LCSServiceTypeID ::= 75
    serv76

serv76

    const LCSServiceTypeID serv76                                         LCSServiceTypeID ::= 76
    serv77

serv77

    const LCSServiceTypeID serv77                                         LCSServiceTypeID ::= 77
    serv78

serv78

    const LCSServiceTypeID serv78                                         LCSServiceTypeID ::= 78
    serv79

serv79

    const LCSServiceTypeID serv79                                         LCSServiceTypeID ::= 79
    serv80

serv80

    const LCSServiceTypeID serv80                                         LCSServiceTypeID ::= 80
    serv81

serv81

    const LCSServiceTypeID serv81                                         LCSServiceTypeID ::= 81
    serv82

serv82

    const LCSServiceTypeID serv82                                         LCSServiceTypeID ::= 82
    serv83

serv83

    const LCSServiceTypeID serv83                                         LCSServiceTypeID ::= 83
    serv84

serv84

    const LCSServiceTypeID serv84                                         LCSServiceTypeID ::= 84
    serv85

serv85

    const LCSServiceTypeID serv85                                         LCSServiceTypeID ::= 85
    serv86

serv86

    const LCSServiceTypeID serv86                                         LCSServiceTypeID ::= 86
    serv87

serv87

    const LCSServiceTypeID serv87                                         LCSServiceTypeID ::= 87
    serv88

serv88

    const LCSServiceTypeID serv88                                         LCSServiceTypeID ::= 88
    serv89

serv89

    const LCSServiceTypeID serv89                                         LCSServiceTypeID ::= 89
    serv90

serv90

    const LCSServiceTypeID serv90                                         LCSServiceTypeID ::= 90
    serv91

serv91

    const LCSServiceTypeID serv91                                         LCSServiceTypeID ::= 91
    serv92

serv92

    const LCSServiceTypeID serv92                                         LCSServiceTypeID ::= 92
    serv93

serv93

    const LCSServiceTypeID serv93                                         LCSServiceTypeID ::= 93
    serv94

serv94

    const LCSServiceTypeID serv94                                         LCSServiceTypeID ::= 94
    serv95

serv95

    const LCSServiceTypeID serv95                                         LCSServiceTypeID ::= 95
    serv96

serv96

    const LCSServiceTypeID serv96                                         LCSServiceTypeID ::= 96
    serv97

serv97

    const LCSServiceTypeID serv97                                         LCSServiceTypeID ::= 97
    serv98

serv98

    const LCSServiceTypeID serv98                                         LCSServiceTypeID ::= 98
    serv99

serv99

    const LCSServiceTypeID serv99                                         LCSServiceTypeID ::= 99
    serv100

serv100

    const LCSServiceTypeID serv100                                        LCSServiceTypeID ::= 100
    serv101

serv101

    const LCSServiceTypeID serv101                                        LCSServiceTypeID ::= 101
    serv102

serv102

    const LCSServiceTypeID serv102                                        LCSServiceTypeID ::= 102
    serv103

serv103

    const LCSServiceTypeID serv103                                        LCSServiceTypeID ::= 103
    serv104

serv104

    const LCSServiceTypeID serv104                                        LCSServiceTypeID ::= 104
    serv105

serv105

    const LCSServiceTypeID serv105                                        LCSServiceTypeID ::= 105
    serv106

serv106

    const LCSServiceTypeID serv106                                        LCSServiceTypeID ::= 106
    serv107

serv107

    const LCSServiceTypeID serv107                                        LCSServiceTypeID ::= 107
    serv108

serv108

    const LCSServiceTypeID serv108                                        LCSServiceTypeID ::= 108
    serv109

serv109

    const LCSServiceTypeID serv109                                        LCSServiceTypeID ::= 109
    serv110

serv110

    const LCSServiceTypeID serv110                                        LCSServiceTypeID ::= 110
    serv111

serv111

    const LCSServiceTypeID serv111                                        LCSServiceTypeID ::= 111
    serv112

serv112

    const LCSServiceTypeID serv112                                        LCSServiceTypeID ::= 112
    serv113

serv113

    const LCSServiceTypeID serv113                                        LCSServiceTypeID ::= 113
    serv114

serv114

    const LCSServiceTypeID serv114                                        LCSServiceTypeID ::= 114
    serv115

serv115

    const LCSServiceTypeID serv115                                        LCSServiceTypeID ::= 115
    serv116

serv116

    const LCSServiceTypeID serv116                                        LCSServiceTypeID ::= 116
    serv117

serv117

    const LCSServiceTypeID serv117                                        LCSServiceTypeID ::= 117
    serv118

serv118

    const LCSServiceTypeID serv118                                        LCSServiceTypeID ::= 118
    serv119

serv119

    const LCSServiceTypeID serv119                                        LCSServiceTypeID ::= 119
    serv120

serv120

    const LCSServiceTypeID serv120                                        LCSServiceTypeID ::= 120
    serv121

serv121

    const LCSServiceTypeID serv121                                        LCSServiceTypeID ::= 121
    serv122

serv122

    const LCSServiceTypeID serv122                                        LCSServiceTypeID ::= 122
    serv123

serv123

    const LCSServiceTypeID serv123                                        LCSServiceTypeID ::= 123
    serv124

serv124

    const LCSServiceTypeID serv124                                        LCSServiceTypeID ::= 124
    serv125

serv125

    const LCSServiceTypeID serv125                                        LCSServiceTypeID ::= 125
    serv126

serv126

    const LCSServiceTypeID serv126                                        LCSServiceTypeID ::= 126
    serv127

serv127

    const LCSServiceTypeID serv127                                        LCSServiceTypeID ::= 127
    PLMN-Id

priorityLevelA

    const EMLPP_Priority priorityLevelA                            EMLPP-Priority  ::= 6
    priorityLevelB

priorityLevelB

    const EMLPP_Priority priorityLevelB                            EMLPP-Priority  ::= 5
    priorityLevel0

priorityLevel0

    const EMLPP_Priority priorityLevel0                            EMLPP-Priority  ::= 0
    priorityLevel1

priorityLevel1

    const EMLPP_Priority priorityLevel1                            EMLPP-Priority  ::= 1
    priorityLevel2

priorityLevel2

    const EMLPP_Priority priorityLevel2                            EMLPP-Priority  ::= 2
    priorityLevel3

priorityLevel3

    const EMLPP_Priority priorityLevel3                            EMLPP-Priority  ::= 3
    priorityLevel4

priorityLevel4

    const EMLPP_Priority priorityLevel4                            EMLPP-Priority  ::= 4
    MC-SS-Info

maxNumOfMC_Bearers

    const integer maxNumOfMC-Bearers   INTEGER ::= 7
    Ext-SS-Status

© Copyright Testing Technologies IST GmbH 2012