OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group PosSessionGroup

Declared in module SUPL_V2_CommonSteps

Functions Summary
f_startPosSessionADOnly | Starts and complete a SUPL POS Session with AD only
f_startAndCompletePosSession | Starts and complete a SUPL POS Session with the SET
f_HandleLPPMessages | This function will complete the MO LPP message exchange with LTE device.
f_HandleLPPMessagesUT3Timer | This function will complete the MO LPP message exchange with LTE device to test its UT3 timer.
f_HandleLPPMessagesWithAutonomousGPS | This function will complete the MO LPP message exchange with LTE device using Autonomous GPS(No assistance data sending to UE)
f_ConstructLPPMessageForIncorretSessionID |
f_ProvideAGpsAssistData |
f_RequestLocationInfo |
f_sendPositionReq | Send SUPL POS message with GPS position request, await measurement response
runGPSPosition |
endSession |

## Details

f_startPosSessionADOnly

    function f_startPosSessionADOnly(ULP_PDU p_ulpPdu,SessionID p_sessionId, RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent
      return UlpMessage

Declared in group PosSessionGroup
Starts and complete a SUPL POS Session with AD only
Runs On: SUPLComponent
Returns: UlpMessage - a Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_ulpPdu -
- p_sessionId -
- p_methodType -
- p_commonIEsRequestLocationInformation -

f_startAndCompletePosSession

    function f_startAndCompletePosSession(ULP_PDU p_ulpPdu,SessionID p_sessionId, template (omit)RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent return UlpMessage

Declared in group PosSessionGroup
Starts and complete a SUPL POS Session with the SET
Runs On: SUPLComponent
Returns: UlpMessage - a Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_ulpPdu -
- p_sessionId -
- p_methodType -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessages

    function f_HandleLPPMessages (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device.
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessagesUT3Timer

    function f_HandleLPPMessagesUT3Timer (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device to test its UT3 timer.
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_HandleLPPMessagesWithAutonomousGPS

    function f_HandleLPPMessagesWithAutonomousGPS (SessionID p_sessionId,template (value) ULP_PDU p_suplPosInit, template (value) CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent    return UlpMessage

Declared in group PosSessionGroup
This function will complete the MO LPP message exchange with LTE device using Autonomous GPS(No assistance data sending to UE)
Runs On: SUPLComponent
Returns: UlpMessage - A Ver2_SUPLREPORT for the completed session or null otherwise
Parameters:

- p_sessionId -
- p_suplPosInit -
- p_commonIEsRequestLocationInformation -

f_ConstructLPPMessageForIncorretSessionID

    function f_ConstructLPPMessageForIncorretSessionID () runs on SUPLComponent return LPP_Messages

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: LPP_Messages -

f_ProvideAGpsAssistData

    function f_ProvideAGpsAssistData (A_GNSS_RequestAssistanceData p_RequestAssistData ) runs on SUPLComponent   return A_GNSS_ProvideAssistanceData

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: A_GNSS_ProvideAssistanceData -
Parameters:

- p_RequestAssistData -

f_RequestLocationInfo

    function f_RequestLocationInfo( template(value) CommonIEsRequestLocationInformation commonIEsRequestLocationInformation_data) runs on SUPLComponent   return RequestLocationInformation

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: RequestLocationInformation -
Parameters:

- commonIEsRequestLocationInformation_data -

f_sendPositionReq

    function f_sendPositionReq(SessionID p_sessionId, RRLP_CommonTypes.MethodType p_methodType) runs on SUPLComponent return UlpMessage

Declared in group PosSessionGroup
Send SUPL POS message with GPS position request, await measurement response
Runs On: SUPLComponent
Returns: UlpMessage - SUPL REPORT message to complete the Position session
Parameters:

- p_sessionId -
- p_methodType -

runGPSPosition

    function runGPSPosition(PosMethod p_prefMethod, boolean p_hasAGPSassisted, boolean p_hasAGPSbased, RRLP_CommonTypes.MethodType p_methodType, template (value)CommonIEsRequestLocationInformation p_commonIEsRequestLocationInformation) runs on SUPLComponent

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_prefMethod -
- p_hasAGPSassisted -
- p_hasAGPSbased -
- p_methodType -
- p_commonIEsRequestLocationInformation -

endSession

    function endSession() runs on SUPLComponent

Declared in group PosSessionGroup
Runs On: SUPLComponent
Returns: void -

© Copyright Testing Technologies IST GmbH 2012