OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group ConfigurationGroup

Declared in module SUPL_V2_CommonSteps

Functions Summary
f_nwc_action_withtimer | funtion requests handover from NWcontroller
f_resetUePositionStoredInformation |
f_init_SSC |
f_start_SCC |
f_stop_SCC |
f_stop_Communication |
f_restart_Communication |

## Details

f_nwc_action_withtimer

    function f_nwc_action_withtimer(in TargetAreaCell p_targetAreaCell, in MMIMessage p_mmiMessage, in float p_timer) runs on SUPLComponent

Declared in group ConfigurationGroup
funtion requests handover from NWcontroller
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_targetAreaCell -
- p_mmiMessage - message text if no automation at the port
- p_timer - delay time after handover command

f_resetUePositionStoredInformation

    function f_resetUePositionStoredInformation(ResetType p_resetType) runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_resetType -

f_init_SSC

    function f_init_SSC(GNSSScenario p_GNSSScenario) runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -
Parameters:

- p_GNSSScenario -

f_start_SCC

    function f_start_SCC() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_stop_SCC

    function f_stop_SCC() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_stop_Communication

    function f_stop_Communication() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

f_restart_Communication

    function f_restart_Communication() runs on SUPLComponent

Declared in group ConfigurationGroup
Runs On: SUPLComponent
Returns: void -

© Copyright Testing Technologies IST GmbH 2012