OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_14x.TC_142

Declared in module SUPL_V2_SET_INITIATED_Tests

Test cases Summary
TC_142_1 |
TC_142_2 | To test SET correctly actions timer UT3 - Test 2: Triggered Session

## Details

TC_142_1

    testcase TC_142_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
Runs On: SUPLComponent
System: SystemInterfaces

TC_142_2

    testcase TC_142_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_14x.TC_142
To test SET correctly actions timer UT3 - Test 2: Triggered Session
Purpose: SUPL-2.0-con-142-2 TP version: Test Case Id : SUPL-2.0-con-142 Test Object : Client Test Case Description : To test SET correctly actions timer UT3 Specification Reference : ULP TS Appendix D SCR Reference : ULP-PRO-C-009-O Tool : SUPL Client Conformance Test Tool Test code : Validated test code for this test case Preconditions : (ics_AGPSSETassisted_SET_initiated OR ics_AGPSSETbased_SET_initiated OR [others FFS]) AND (ics_periodic_SET_initiated OR ics_event_SET_initiated) Test Procedure : Test 2: Triggered session Note: This test case is applicable to SETs that support any location method that requires a SUPL POS session and that supports any triggered service. This test case has been written for a Periodic Triggered, SET assisted mode Location Session. The case where Periodic Location sessions or a SET assisted mode is not supported in the SET is FFS 9. Start a SI Periodic Triggered Location Session 10. The SET sends SUPL TRIGGERED START 11. Send SUPL TRIGGERED RESPONSE with: Positioning Method set to any SET assisted method that requires a SUPL POS session that is supported by the SET 12. When the first periodic trigger occurs the SET sends SUPL POS INIT 13. A SUPL POS session takes place 14. After the SET sends the final SUPL POS do not respond 15. (After timer UT3 expires (depending on ixit_timer_UT3) the SET will continue to the next trigger in the session) Note that the SET may release the secure connection at this time. 16. When the second periodic trigger occurs the SET sends SUPL POS INIT 17. A SUPL POS session takes place 18. Send SUPL REPORT 19. The Triggered Location Session can be allowed to continue, or send SUPL TRIGGERED STOP to terminate the session Pass-Criteria : Test 2: 3. At step 16 the SET shall send SUPL POS INIT
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012