OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group TC_05x.TC_051

Declared in module SUPL_V2_SLP_INITIATED_Tests

Test cases Summary
TC_051_1_1 | To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 1: Entering event type
TC_051_1_2 | To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 2: Inside event type
TC_051_1_3 | To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 3: Outside event type
TC_051_1_4 | To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 4: Leaving event type
TC_051_2_1 | To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 1: Entering event type
TC_051_2_2 | To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 2: Inside event type
TC_051_2_3 | To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 3: Outside event type
TC_051_2_4 | To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 4: Leaving event type

## Details

TC_051_1_1

    testcase TC_051_1_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 1: Entering event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_1_2

    testcase TC_051_1_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 2: Inside event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_1_3

    testcase TC_051_1_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 3: Outside event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_1_4

    testcase TC_051_1_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 1: A-GPS SET assisted, Case 4: Leaving event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_2_1

    testcase TC_051_2_1() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 1: Entering event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_2_2

    testcase TC_051_2_2() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 2: Inside event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_2_3

    testcase TC_051_2_3() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 3: Outside event type
Runs On: SUPLComponent
System: SystemInterfaces

TC_051_2_4

    testcase TC_051_2_4() runs on SUPLComponent system SystemInterfaces

Declared in group TC_05x.TC_051
To test SET correctly performs Area Event reporting with Area ID - Test 2: A-GPS SET based, Case 4: Leaving event type
Runs On: SUPLComponent
System: SystemInterfaces

© Copyright Testing Technologies IST GmbH 2012