OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test Cases Modules

INDEX

A B C D E F G H I J K L M N O P Q R S T U V W X Y Z _

m_AcceptContact_invalid | template declared in LibSip_Templates
m_accuracyOpt_omittedV10 | template declared in SUPL_V2_Templates TODO: Add description
m_accuracyOpt_omittedV5 | template declared in SUPL_V2_Templates TODO: Add description
m_AcRcValue_empty | template declared in LibSip_Templates
m_areaId_cdma_cellId | template declared in SUPL_V2_Templates Builds an Area Id message instance from a CDMA cell ID
m_areaId_gsm_cellId | template declared in SUPL_V2_Templates Builds an Area Id message instance from a GSM cell ID
m_areaId_hrpd_cellId | template declared in SUPL_V2_Templates Builds an Area Id message instance from a hRPD cell ID
m_areaId_lte_cellId | template declared in SUPL_V2_Templates Builds an Area Id message instance from a LTE cell ID
m_areaId_wcdma_cellId | template declared in SUPL_V2_Templates Builds an Area Id message instance from a WCDMA cell ID
m_areaIdList | template declared in SUPL_V2_Templates
m_areaIdLists_one_areaId | template declared in SUPL_V2_Templates TODO: Add description
m_basicMAC | template declared in SUPL_V2_Templates
m_basicMAC_zero | template declared in SUPL_V2_Templates
m_BasicProtectionLevel | template declared in SUPL_V2_Templates basic ProtectionLevel from SUPL INIT
m_basicReplayCounter | template declared in SUPL_V2_Templates
m_batchRepConditionsByEndofsession | template declared in SUPL_V2_Templates
m_batchRepConditionsByInterval | template declared in SUPL_V2_Templates
m_batchRepConditionsByMinutes | template declared in SUPL_V2_Templates
m_batchRepType | template declared in SUPL_V2_Templates
m_C2K_SuplInit | template declared in SUPL_V2_Templates
m_cdmaAreaId_cellId | template declared in SUPL_V2_Templates CDMA Area ID from cell ID
m_ContentType_invalid | template declared in LibSip_Templates
M_CSI | type declared in MAP_MS_DataTypes_V10
m_ESLPAddressIP | template declared in SUPL_V2_Templates
m_gsmAreaId_cellId | template declared in SUPL_V2_Templates GSM area ID from cell ID
m_hrpdAreaId_cellId | template declared in SUPL_V2_Templates hRPD Area ID from cell ID
m_keyIdentifier | template declared in SUPL_V2_Templates
m_keyIdentifier_incorrect | template declared in SUPL_V2_Templates
m_lppProvAssistData_Agps | template declared in LPP_Templates
m_lppProvAssistData_AGPS | template declared in LPP_Templates
m_lppReqLocInfo_AGPS | template declared in LPP_Templates
m_lteAreaId_cellId | template declared in SUPL_V2_Templates LTE Area ID from cell ID
m_MESSAGE_Dummy | template declared in LibSip_Templates
m_MessageBodyUlp | template declared in LibSip_Templates
m_MESSAGEreq | template declared in LibSip_Templates
m_methodType_msAssistedV10 | template declared in SUPL_V2_Templates TODO: Add description
m_methodType_msAssistedV5 | template declared in SUPL_V2_Templates TODO: Add description
m_methodType_msAssitedPrefV10 | template declared in SUPL_V2_Templates MS-AssistedPref Method Type
m_methodType_msAssitedPrefV5 | template declared in SUPL_V2_Templates MS-AssistedPref Method Type
m_methodType_msBasedPrefV10 | template declared in SUPL_V2_Templates MS-BasedPref Method Type
m_methodType_msBasedPrefV5 | template declared in SUPL_V2_Templates MS-BasedPref Method Type
m_methodType_msBasedV10 | template declared in SUPL_V2_Templates
m_methodType_msBasedV5 | template declared in SUPL_V2_Templates
m_MMICmd | template declared in SUPL_CommonSteps
m_mmiMessage | template declared in SUPL_V2_Templates
m_msgHeader_dummy | template declared in LibSip_Templates
m_notificationEmergency | template declared in SUPL_V2_Templates
m_ProtectionLevel | template declared in SUPL_V2_Templates
m_ProtectionParamsDefault | template declared in SUPL_V2_Templates
m_reportingModeBatch | template declared in SUPL_V2_Templates
m_reportingModeQuasiReal | template declared in SUPL_V2_Templates
m_requestLine | template declared in LibSip_Templates
m_requestLine_dummy | template declared in LibSip_Templates
m_setEventTriggerCap | template declared in SUPL_V2_Templates
m_setTriggerServiceSupported | template declared in SUPL_V2_Templates
m_sipUri | template declared in LibSip_Templates
m_SLPAddressFQDN | template declared in SUPL_V2_Templates
m_suplInitBase | template declared in SUPL_V2_Templates
m_suplNotify | template declared in SUPL_V2_Templates
m_suplPosLPP | template declared in LPP_Templates
m_suplReport | template declared in SUPL_V2_Templates
m_suplReportPosition | template declared in SUPL_V2_Templates
m_suplResponse_posTechnology | template declared in SUPL_V2_Templates
m_suplTriggeredResponse | template declared in SUPL_V2_Templates
m_suplTriggeredResponse_posMethod_trigParams | template declared in SUPL_V2_Templates SUPL TRIGGERED RESPONSE with positioning method and trigger parameters
m_suplTriggeredResponsePosMethodTriggerParams | template declared in SUPL_V2_Templates
m_suplTriggeredResponsePosMethodTriggerParamsReportingMode | template declared in SUPL_V2_Templates
m_suplTriggeredResponseTriggerParams | template declared in SUPL_V2_Templates
m_suplTriggeredStop | template declared in SUPL_V2_Templates
m_triggerParamsAreaEvent | template declared in SUPL_V2_Templates
m_triggerParamsPeriodic | template declared in SUPL_V2_Templates
m_UDP_SuplInit | template declared in SUPL_V2_Templates
m_UDP_SuplInit_invalidPort | template declared in SUPL_V2_Templates
m_ulpMessage_suplReport | template declared in SUPL_V2_Templates TODO: Add description
m_ulpMessage_suplTriggeredResponse | template declared in SUPL_V2_Templates TODO: Add description
m_ulpMessageSuplResponse_posTechnology | template declared in SUPL_V2_Templates TODO: Add description
m_ulpPdu | template declared in SUPL_V2_Templates
m_ulpPduVersion | template declared in SUPL_V2_Templates Creates a ULP_PDU using a given version
m_ulpSuplInit | template declared in SUPL_V2_Templates
m_ver2_SUPL_RESPONSE_extension_pos_technology | template declared in SUPL_V2_Templates TODO: Add description
m_ver2SuplInitESlpAddress | template declared in SUPL_V2_Templates
m_ver2SuplInitExtensionGnssPosTechnology | template declared in SUPL_V2_Templates
m_ver2SuplInitExtensionTriggerType | template declared in SUPL_V2_Templates
m_ver2SuplInitMinimumMajorVersion | template declared in SUPL_V2_Templates
m_ver2SuplInitProtectionLevel | template declared in SUPL_V2_Templates
m_Version | template declared in SUPL_V2_Templates Default outgoing Version template
m_Version1 | template declared in SUPL_V2_Templates Default Version 1.
m_version_min_serverind_p | template declared in SUPL_V2_Templates Version based on min and server ind
m_Version_p | template declared in SUPL_V2_Templates Version template taking each field as parameter for outgoing messages
m_wcdmaAreaId_cellId | template declared in SUPL_V2_Templates WCDMA Area ID from cell ID
MAC | type declared in SUPLTypes
mah | const declared in MAP_SS_Code_V10
Make_all |
MAP_BS_Code_V10 |
MAP_CommonDataTypes_V10 |
MAP_ER_DataTypes_V10 |
MAP_EXTENSION | type declared in MAP_ExtensionDataTypes_V10
MAP_EXTENSION | type declared in RRLPV5Types
MAP_ExtensionDataTypes_V10 |
MAP_LCS_DataTypes_V10 |
MAP_MS_DataTypes_V10 |
MAP_OM_DataTypes_V10 |
MAP_SM_DataTypes_V10 |
MAP_SS_Code_V10 |
MAP_SS_DataTypes_V10 |
MAP_TS_Code_V10 |
mapChiperSuiteToNumber | function declared in SUPL_CommonSteps
MatchType | type declared in MAP_MS_DataTypes_V10
maxAdd_GeographicalInformation | const declared in MAP_LCS_DataTypes_V10
maxAddressLength | const declared in MAP_CommonDataTypes_V10
maxAreaId | const declared in SUPLTypes
maxAreaIdList | const declared in SUPLTypes
maxBands | const declared in LPP_PDU_Definitions
maxCellMeas | const declared in SUPLTypes
maxCellReport | const declared in SUPLTypes
maxClientLength | const declared in SUPLTypes
maxEPDU | const declared in LPP_PDU_Definitions
maxEventSpecification | const declared in MAP_SS_DataTypes_V10
maxExt_GeographicalInformation | const declared in MAP_LCS_DataTypes_V10
maxExt_GeographicalInformation | const declared in RRLPV5Types
MaxForwards | type declared in LibSip_SIPTypesAndValues
maxFreq | const declared in SUPLTypes
maxFreqLayers | const declared in LPP_PDU_Definitions
maxFTN_AddressLength | const declared in MAP_CommonDataTypes_V10
maxGANSS | const declared in SUPLTypes
maxGANSSAssistanceData | const declared in RRLP_Components_V10
maxGANSSSat | const declared in SUPLTypes
maxGeranGANSSpositioningData | const declared in MAP_LCS_DataTypes_V10
maxGPSAssistanceData | const declared in RRLP_Components_V10
maxGPSAssistanceData | const declared in RRLPV5Types
maxISDN_AddressLength | const declared in MAP_CommonDataTypes_V10
maxISDN_SubaddressLength | const declared in MAP_CommonDataTypes_V10
maxLCSCodewordStringLength | const declared in MAP_LCS_DataTypes_V10
maxLidSize | const declared in SUPLTypes
maxLongSignalInfoLength | const declared in MAP_CommonDataTypes_V10
MaxMC_Bearers | type declared in MAP_CommonDataTypes_V10
maxNameStringLength | const declared in MAP_LCS_DataTypes_V10
maxNrOfRABs | const declared in MAP_MS_DataTypes_V10
maxNumGeoArea | const declared in SUPLTypes
maxNumOfAPN_Configurations | const declared in MAP_MS_DataTypes_V10
maxNumOfAreas | const declared in MAP_LCS_DataTypes_V10
maxNumOfBasicServiceGroups | const declared in MAP_SS_DataTypes_V10
maxNumOfBasicServices | const declared in MAP_MS_DataTypes_V10
maxNumOfBearerServices | const declared in MAP_MS_DataTypes_V10
maxNumOfCAMEL_O_CauseValueCriteria | const declared in MAP_MS_DataTypes_V10
maxNumOfCAMEL_T_CauseValueCriteria | const declared in MAP_MS_DataTypes_V10
maxNumOfCamelBasicServiceCriteria | const declared in MAP_MS_DataTypes_V10
maxNumOfCamelDestinationNumberLengths | const declared in MAP_MS_DataTypes_V10
maxNumOfCamelDestinationNumbers | const declared in MAP_MS_DataTypes_V10
maxNumOfCamelSSEvents | const declared in MAP_MS_DataTypes_V10
maxNumOfCamelTDPData | const declared in MAP_MS_DataTypes_V10
maxNumOfCCBS_Requests | const declared in MAP_SS_DataTypes_V10
maxNumOfCUG | const declared in MAP_MS_DataTypes_V10
maxNumOfDispatchers | const declared in MAP_SM_DataTypes_V10
maxNumOfDP_AnalysedInfoCriteria | const declared in MAP_MS_DataTypes_V10
maxNumOfEncryptionInfo | const declared in MAP_MS_DataTypes_V10
maxNumOfExt_BasicServiceGroups | const declared in MAP_MS_DataTypes_V10
maxNumOfExt_ExternalClient | const declared in MAP_MS_DataTypes_V10
maxNumOfExternalClient | const declared in MAP_MS_DataTypes_V10
maxNumOfGMLC | const declared in MAP_MS_DataTypes_V10
maxNumOfHLR_Id | const declared in MAP_CommonDataTypes_V10
maxNumOfIntegrityInfo | const declared in MAP_MS_DataTypes_V10
maxNumOfISDN_AddressDigits | const declared in MAP_MS_DataTypes_V10
maxNumOfLSAs | const declared in MAP_MS_DataTypes_V10
maxNumOfMC_Bearers | const declared in MAP_CommonDataTypes_V10
maxNumOfMobilityTriggers | const declared in MAP_MS_DataTypes_V10
maxNumOfMOLR_Class | const declared in MAP_MS_DataTypes_V10
maxNumOfMSISDN | const declared in MAP_MS_DataTypes_V10
maxNumOfPDP_Contexts | const declared in MAP_MS_DataTypes_V10
maxNumOfPLMNClient | const declared in MAP_MS_DataTypes_V10
maxNumOfPrivacyClass | const declared in MAP_MS_DataTypes_V10
maxNumOfPrivateExtensions | const declared in MAP_ExtensionDataTypes_V10
maxNumOfPrivateExtensions | const declared in RRLPV5Types
maxNumOfRadioResources | const declared in MAP_MS_DataTypes_V10
maxNumOfRelocationNumber | const declared in MAP_MS_DataTypes_V10
maxNumOfReportingPLMN | const declared in MAP_LCS_DataTypes_V10
maxNumOfServiceHandovers | const declared in MAP_MS_DataTypes_V10
maxNumOfServiceType | const declared in MAP_MS_DataTypes_V10
maxNumOfSpecificAPNInfos | const declared in MAP_MS_DataTypes_V10
maxNumOfSS | const declared in MAP_SS_DataTypes_V10
maxNumOfTeleservices | const declared in MAP_MS_DataTypes_V10
maxNumOfTPDUTypes | const declared in MAP_MS_DataTypes_V10
maxNumOfVBSGroupIds | const declared in MAP_MS_DataTypes_V10
maxNumOfVGCSGroupIds | const declared in MAP_MS_DataTypes_V10
maxNumOfZoneCodes | const declared in MAP_MS_DataTypes_V10
maxnumSessions | const declared in SUPLTypes
maxPermittedEncryptionAlgorithmsLength | const declared in MAP_MS_DataTypes_V10
maxPermittedIntegrityProtectionAlgorithmsLength | const declared in MAP_MS_DataTypes_V10
maxPositioningDataInformation | const declared in MAP_LCS_DataTypes_V10
maxReportingAmount | const declared in MAP_LCS_DataTypes_V10
maxReportingInterval | const declared in MAP_LCS_DataTypes_V10
maxReqLength | const declared in SUPLTypes
maxRequestorIDStringLength | const declared in MAP_LCS_DataTypes_V10
maxSignalInfoLength | const declared in MAP_CommonDataTypes_V10
maxTS | const declared in SUPLTypes
maxUSSD_StringLength | const declared in MAP_SS_DataTypes_V10
maxUtranGANSSpositioningData | const declared in MAP_LCS_DataTypes_V10
maxUtranPositioningDataInfo | const declared in MAP_LCS_DataTypes_V10
maxWimaxBSMeas | const declared in SUPLTypes
maxWLANApDataSize | const declared in SUPLTypes
mc | const declared in MAP_SS_Code_V10
MC_Bearers | type declared in MAP_CommonDataTypes_V10
MC_SS_Info | type declared in MAP_CommonDataTypes_V10
MCC | type declared in SUPLTypes
MCC_MNC_Digit | type declared in SUPLTypes
mci | const declared in MAP_SS_Code_V10
MeasResultEUTRA | type declared in SUPLTypes
MeasResultListEUTRA | type declared in SUPLTypes
MeasuredResults | type declared in SUPLTypes
MeasuredResultsElement | type declared in LPP_PDU_Definitions
MeasuredResultsList | type declared in LPP_PDU_Definitions
MeasuredResultsList | type declared in SUPLTypes
MeasurementReferenceTime | type declared in LPP_PDU_Definitions
MeasureResponseTime | type declared in RRLP_CommonTypes
MeasureResponseTime | type declared in RRLP_Components_V10
MeasureResponseTime | type declared in RRLPV5Types
MESSAGE_Request | type declared in LibSip_SIPTypesAndValues
MessageBody | type declared in LibSip_SIPTypesAndValues
MessageHeader | type declared in LibSip_SIPTypesAndValues
MessageWaitListFullParam | type declared in MAP_ER_DataTypes_V10
Method | type declared in LibSip_SIPTypesAndValues
Method_List | type declared in LibSip_SIPTypesAndValues
MethodType | type declared in RRLP_CommonTypes
MethodType | type declared in RRLP_Components_V10
MethodType | type declared in RRLPV5Types
MG_CSI | type declared in MAP_MS_DataTypes_V10
MGW_EventList | type declared in MAP_OM_DataTypes_V10
MGW_EventList_context_ | const declared in MAP_OM_DataTypes_V10
MGW_InterfaceList | type declared in MAP_OM_DataTypes_V10
MGW_InterfaceList_iu_up_ | const declared in MAP_OM_DataTypes_V10
MGW_InterfaceList_mc_ | const declared in MAP_OM_DataTypes_V10
MGW_InterfaceList_nb_up_ | const declared in MAP_OM_DataTypes_V10
MimeVersion | type declared in LibSip_SIPTypesAndValues
MinExpires | type declared in LibSip_SIPTypesAndValues
MinSE | type declared in LibSip_SIPTypesAndValues
MM_Code | type declared in MAP_MS_DataTypes_V10
MM_EventNotSupported_Param | type declared in MAP_ER_DataTypes_V10
MME_EventList | type declared in MAP_OM_DataTypes_V10
MME_EventList_bearerActivationModificationDeletion_ | const declared in MAP_OM_DataTypes_V10
MME_EventList_handover_ | const declared in MAP_OM_DataTypes_V10
MME_EventList_initialAttachTrackingAreaUpdateDetach_ | const declared in MAP_OM_DataTypes_V10
MME_EventList_serviceRequestts_ | const declared in MAP_OM_DataTypes_V10
MME_EventList_ue_initiatedPDNconectivityRequest_ | const declared in MAP_OM_DataTypes_V10
MME_EventList_ue_initiatedPDNdisconnection_ | const declared in MAP_OM_DataTypes_V10
MME_InterfaceList | type declared in MAP_OM_DataTypes_V10
MME_InterfaceList_s10_ | const declared in MAP_OM_DataTypes_V10
MME_InterfaceList_s11_ | const declared in MAP_OM_DataTypes_V10
MME_InterfaceList_s1_mme_ | const declared in MAP_OM_DataTypes_V10
MME_InterfaceList_s3_ | const declared in MAP_OM_DataTypes_V10
MME_InterfaceList_s6a_ | const declared in MAP_OM_DataTypes_V10
MMIMessage | type declared in SUPL_Configuration
MNC | type declared in SUPLTypes
MNPInfoRes | type declared in MAP_MS_DataTypes_V10
MO_ForwardSM_Arg | type declared in MAP_SM_DataTypes_V10
MO_ForwardSM_Res | type declared in MAP_SM_DataTypes_V10
mobileYellowPages | const declared in MAP_CommonDataTypes_V10
MobilityTriggers | type declared in MAP_MS_DataTypes_V10
ModificationInstruction | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CB_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CF_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CH_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CLIP_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CLIR_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CSG | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CSI | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_CW_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_ECT_Info | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_IP_SM_GW_Data | type declared in MAP_MS_DataTypes_V10
ModificationRequestFor_ODB_data | type declared in MAP_MS_DataTypes_V10
ModuloTimeSlot | type declared in RRLP_Components_V10
ModuloTimeSlot | type declared in RRLPV5Types
MOLR_Class | type declared in MAP_MS_DataTypes_V10
MOLR_List | type declared in MAP_MS_DataTypes_V10
MoreAssDataToBeSent | type declared in RRLP_Components_V10
MoreAssDataToBeSent | type declared in RRLPV5Types
MpathIndic | type declared in RRLP_Components_V10
MpathIndic | type declared in RRLPV5Types
mr_DNS_A_Query | template declared in SUPL_DHCP_DNS_Steps
mr_DNS_AAAA_Query | template declared in SUPL_DHCP_DNS_Steps
mr_DNSMessage_any | template declared in SUPL_DHCP_DNS_Steps
mr_MMI_ok | template declared in SUPL_CommonSteps
MS_Classmark2 | type declared in MAP_MS_DataTypes_V10
MSC_S_EventList | type declared in MAP_OM_DataTypes_V10
MSC_S_EventList_handovers_ | const declared in MAP_OM_DataTypes_V10
MSC_S_EventList_lu_imsiAttach_imsiDetach_ | const declared in MAP_OM_DataTypes_V10
MSC_S_EventList_mo_mt_sms_ | const declared in MAP_OM_DataTypes_V10
MSC_S_EventList_mo_mtCall_ | const declared in MAP_OM_DataTypes_V10
MSC_S_EventList_ss_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList | type declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_a_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_cap_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_iu_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_b_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_c_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_d_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_e_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_f_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_map_g_ | const declared in MAP_OM_DataTypes_V10
MSC_S_InterfaceList_mc_ | const declared in MAP_OM_DataTypes_V10
MSISDN_BS | type declared in MAP_MS_DataTypes_V10
MSISDN_BS_List | type declared in MAP_MS_DataTypes_V10
MSNetworkCapability | type declared in MAP_MS_DataTypes_V10
MSRadioAccessCapability | type declared in MAP_MS_DataTypes_V10
MsrAssistBTS | type declared in RRLP_Components_V10
MsrAssistBTS | type declared in RRLPV5Types
MsrAssistBTS_R98_ExpOTD | type declared in RRLP_Components_V10
MsrAssistBTS_R98_ExpOTD | type declared in RRLPV5Types
MsrAssistData | type declared in RRLP_Components_V10
MsrAssistData | type declared in RRLPV5Types
MsrAssistData_R98_ExpOTD | type declared in RRLP_Components_V10
MsrAssistData_R98_ExpOTD | type declared in RRLPV5Types
MsrPosition_Req | type declared in RRLP_Components_V10
MsrPosition_Req | type declared in RRLPV5Types
MsrPosition_Rsp | type declared in RRLP_Components_V10
MsrPosition_Rsp | type declared in RRLPV5Types
MT_ForwardSM_Arg | type declared in MAP_SM_DataTypes_V10
MT_ForwardSM_Res | type declared in MAP_SM_DataTypes_V10
MT_ForwardSM_VGCS_Arg | type declared in MAP_SM_DataTypes_V10
MT_ForwardSM_VGCS_Res | type declared in MAP_SM_DataTypes_V10
MT_SMS_TPDU_Type | type declared in MAP_MS_DataTypes_V10
MT_smsCAMELTDP_Criteria | type declared in MAP_MS_DataTypes_V10
MT_smsCAMELTDP_CriteriaList | type declared in MAP_MS_DataTypes_V10
MTTransport | type declared in SUPL_TypeDefinitions
MulticallBearerInfo | type declared in MAP_MS_DataTypes_V10
MultiFrameCarrier | type declared in RRLP_Components_V10
MultiFrameCarrier | type declared in RRLPV5Types
MultiFrameOffset | type declared in RRLP_Components_V10
MultiFrameOffset | type declared in RRLPV5Types
MultipleLocationIds | type declared in SUPLTypes
MultipleMeasurementSets | type declared in RRLP_Components_V10
MultipleMeasurementSets_eotd_ | const declared in RRLP_Components_V10
MultipleMeasurementSets_ganss_ | const declared in RRLP_Components_V10
MultipleMeasurementSets_gps_ | const declared in RRLP_Components_V10
MultipleSets | type declared in RRLP_Components_V10
MultipleSets | type declared in RRLPV5Types
multiPTY | const declared in MAP_SS_Code_V10
mw_lppProvCap | template declared in LPP_Templates
mw_lppProvLocInfo_AGPS | template declared in LPP_Templates
mw_lppReqAssistData_AGPS | template declared in LPP_Templates
mw_msgHeader_dummy | template declared in LibSip_Templates
mw_posTech | template declared in SUPL_V2_Templates
mw_posTechICS | template declared in SUPL_V2_Templates
mw_posTechICSV1 | template declared in SUPL_V2_Templates
mw_posTechV1 | template declared in SUPL_V2_Templates
mw_ReportData | template declared in SUPL_V2_Templates
mw_Response_Dummy | template declared in LibSip_Templates
mw_setCapabilities | template declared in SUPL_V2_Templates
mw_setCapabilitiesExt | template declared in SUPL_V2_Templates
MW_Status | type declared in MAP_SM_DataTypes_V10
MW_Status_mcef_Set_ | const declared in MAP_SM_DataTypes_V10
MW_Status_mnrf_Set_ | const declared in MAP_SM_DataTypes_V10
MW_Status_mnrg_Set_ | const declared in MAP_SM_DataTypes_V10
MW_Status_sc_AddressNotIncluded_ | const declared in MAP_SM_DataTypes_V10
mw_suplEndWithCode | template declared in SUPL_V2_Templates
mw_suplPosLPP | template declared in LPP_Templates
mw_suplReportPositionEstimate | template declared in SUPL_V2_Templates
mw_suplReportPositionEstimatePeriodic | template declared in SUPL_V2_Templates
mw_suplTriggeredStart | template declared in SUPL_V2_Templates
mw_suplTriggeredStart_cap | template declared in SUPL_V2_Templates
mw_suplTriggeredStart_triggerType | template declared in SUPL_V2_Templates TODO: Add description
mw_suplTriggeredStop | template declared in SUPL_V2_Templates
mw_ulpMessage_suplPosInit_cap | template declared in SUPL_V2_Templates
mw_ulpMessage_suplPosInit_pos | template declared in SUPL_V2_Templates
mw_ulpMessage_suplStart_cap | template declared in SUPL_V2_Templates
mw_ulpMessage_suplStart_pos | template declared in SUPL_V2_Templates
mw_ulpMessage_triggeredStart | template declared in SUPL_V2_Templates TODO: Add description
mw_Version | template declared in SUPL_V2_Templates Version template taking each field as parameter for incoming messages
mw_Version1 | template declared in SUPL_V2_Templates
mw_Version2 | template declared in SUPL_V2_Templates Default incoming Version 2.
mw_version_minor_ind_0_or_X | template declared in SUPL_V2_Templates

© Copyright Testing Technologies IST GmbH 2012