OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test Cases Modules

INDEX

A B C D E F G H I J K L M N O P Q R S T U V W X Y Z _

f_areaEventType2String | function declared in SUPL_V2_CommonSteps Converts an AreaEventType value into a character string
f_areaId2String | function declared in SUPL_V2_CommonSteps Converts ans AreaId value in its character string representation
f_areaIdList2String | function declared in SUPL_V2_CommonSteps Converts an AreaIdList value in its character string representation
f_areaIdLists2String | function declared in SUPL_V2_CommonSteps Converts an AreaIdLists value into a character string
f_areaIdSet2String | function declared in SUPL_V2_CommonSteps Converts an AreaIdSet value into a character string
f_areaList2String | function declared in SUPL_V2_CommonSteps Converts a GeographicTargetAreaList value into a character string
f_awaitSuplPosInit | function declared in SUPL_V2_CommonSteps
f_bool2String | function declared in SUPL_V2_CommonSteps Converts a boolean value into a character string
f_Build_DNS_A_Response_Default_ESLP | function declared in SUPL_V2_DHCP_DNS_Steps
f_Build_DNS_A_Response_ESLP | function declared in SUPL_V2_DHCP_DNS_Steps
f_checkAGNSSRequestAssistData | function declared in LPP_Templates
f_checkLppMessages | function declared in LPP_Templates
f_checkLppMessagesTypes | function declared in LPP_Templates
f_checkPosCapabilitiesParam_againstSET | function declared in SUPL_V2_CommonSteps Checks that the details of the positioning capability parameter contained in incoming ULP-PDU message are consistent with the known positioning capabilities supported by the SET.
f_checkReportingAndServiceCaps_againstSET | function declared in SUPL_V2_CommonSteps Checks that the details of the reporting capability parameter contained in incoming TRIGGERED START message are consistent with the known reporting capabilities supported by the SET.
f_checkServiceCaps_againstSET | function declared in SUPL_V2_CommonSteps Checks that the details of the service capability parameter contained in incoming TRIGGERED START message are consistent with the known service capabilities supported by the SET.
f_checkSET_positionEstimate_displayed | function declared in SUPL_V2_CommonSteps Checks that a position estimate is displayed at the SET
f_checkSET_positionEstimate_displayed_atEnd | function declared in SUPL_V2_CommonSteps Checks that position estimate(s) is displayed at the SET at the end of the test
f_ConstructLPPMessageForIncorretSessionID | function declared in SUPL_V2_CommonSteps
f_coordinate2String | function declared in SUPL_V2_CommonSteps Converts a Coordinate value into its character string representation
f_coordinateList2String | function declared in SUPL_V2_CommonSteps Converts a list of coordinates into a correspunding character string representation
f_encodeLppPayload | function declared in LPP_Templates
f_endSession | function declared in LPP_Templates
f_generateCompletedSessionId | function declared in SUPL_V2_CommonSteps generates a SUPL session ID depending on the receiving SUPL session ID (used to get the SET session ID) and a SLP session will be added
f_generateSuplInitwithMAC | function declared in SUPL_V2_CommonSteps
f_geoAreaMappingList2String | function declared in SUPL_V2_CommonSteps Converts a GeoAreaMappingList into its character string representation
f_geographicTargetArea2String | function declared in SUPL_V2_CommonSteps Convert a GeographicTargetArea value into a character string representation
f_HandleLPPMessages | function declared in SUPL_V2_CommonSteps This function will complete the MO LPP message exchange with LTE device.
f_HandleLPPMessagesUT3Timer | function declared in SUPL_V2_CommonSteps This function will complete the MO LPP message exchange with LTE device to test its UT3 timer.
f_HandleLPPMessagesWithAutonomousGPS | function declared in SUPL_V2_CommonSteps This function will complete the MO LPP message exchange with LTE device using Autonomous GPS(No assistance data sending to UE)
f_init | function declared in SUPL_V2_CommonSteps
f_init_SSC | function declared in SUPL_V2_CommonSteps
f_initfinalizePRSConfiguration | function declared in SUPL_V2_CommonSteps
f_initgetCellTimingDelay | function declared in SUPL_V2_CommonSteps
f_initIntern | function declared in SUPL_V2_CommonSteps
f_initPRS | function declared in SUPL_V2_CommonSteps
f_initPRSConfigurationIndex | function declared in SUPL_V2_CommonSteps
f_initPRSMutingInfoBitLength | function declared in SUPL_V2_CommonSteps
f_initPRSNumDLFrames | function declared in SUPL_V2_CommonSteps
f_initsetCellTimingDelay | function declared in SUPL_V2_CommonSteps
f_initSetNumberOfAntennas | function declared in SUPL_V2_CommonSteps
f_initSetTargetAreaCell | function declared in SUPL_V2_CommonSteps
f_initWithDefinedCiphersuite | function declared in SUPL_V2_CommonSteps
f_initWithDefinedFQDN | function declared in SUPL_V2_CommonSteps
f_initWithTlsVersion | function declared in SUPL_V2_CommonSteps
f_latitudeSign2String | function declared in SUPL_V2_CommonSteps Converts a latitude sign value into its character string representation
f_nwc_action_withtimer | function declared in SUPL_V2_CommonSteps funtion requests handover from NWcontroller
f_Postamble | function declared in SUPL_V2_CommonSteps
f_ProvideAGpsAssistData | function declared in SUPL_V2_CommonSteps
f_RequestLocationInfo | function declared in SUPL_V2_CommonSteps
f_resetUePositionStoredInformation | function declared in SUPL_V2_CommonSteps
f_restart_Communication | function declared in SUPL_V2_CommonSteps
f_sendC2KSms | function declared in SUPL_V2_CommonSteps
f_sendMTSmsMAC | function declared in SUPL_V2_CommonSteps
f_sendPositionReq | function declared in SUPL_V2_CommonSteps Send SUPL POS message with GPS position request, await measurement response
f_sendSipPushSms | function declared in SUPL_V2_CommonSteps
f_sendSipPushSms_Header | function declared in SUPL_V2_CommonSteps
f_sendSms | function declared in SUPL_V2_CommonSteps
f_sendSmsInternal | function declared in SUPL_V2_CommonSteps
f_sendSuplEnd | function declared in SUPL_V2_CommonSteps
f_sendSuplNotify | function declared in SUPL_V2_CommonSteps
f_sendUDPSms | function declared in SUPL_V2_CommonSteps
f_sendUDPSms_invalidPort | function declared in SUPL_V2_CommonSteps
f_SLPAddressIP | function declared in SUPL_V2_CommonSteps
f_start_SCC | function declared in SUPL_V2_CommonSteps
f_startAndCompletePosSession | function declared in SUPL_V2_CommonSteps Starts and complete a SUPL POS Session with the SET
f_startPosSessionADOnly | function declared in SUPL_V2_CommonSteps Starts and complete a SUPL POS Session with AD only
f_stop_Communication | function declared in SUPL_V2_CommonSteps
f_stop_SCC | function declared in SUPL_V2_CommonSteps
f_TC_009_1 | function declared in SUPL_V2_TCFunctions
f_TC_009_2 | function declared in SUPL_V2_TCFunctions
f_TC_009_3 | function declared in SUPL_V2_TCFunctions
f_TC_009_4 | function declared in SUPL_V2_TCFunctions
f_triggerParams2String | function declared in SUPL_V2_CommonSteps Converts a TriggerParams value into a character string
flowFor024 | function declared in SUPL_V2_CommonSteps
fx_GadLatitude | function declared in SUPL_V2_CommonSteps convertion of latitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
fx_GadLongitude | function declared in SUPL_V2_CommonSteps convertion of logitude coordinates from World Geodetic System 1984 (WGS 84) to GAD [3GPP TS 23 032]
fx_gpsPositionCalculation | function declared in SUPL_V2_CommonSteps calculates a Position value based on the last received SUPL POS
fx_HMAC_SHA256_128 | function declared in SUPL_V2_ExternalSteps
fx_HMAC_SHA256_32 | function declared in SUPL_V2_ExternalSteps
fx_positionIsIn | function declared in SUPL_V2_CommonSteps calculation if a Position estimate value is located within the geographic area

© Copyright Testing Technologies IST GmbH 2012