OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group functions.pskDerivation

Declared in module SUPL_CommonSteps

Functions Summary
mapChiperSuiteToNumber |
generateUaSecurityProtocolId | The Ua security protocol identifier is a string of five octets.

## Details

mapChiperSuiteToNumber

    function mapChiperSuiteToNumber(in CipherSuites p_ciphersuite) return octetstring

Declared in group functions.pskDerivation
Returns: octetstring -
Parameters:

- p_ciphersuite -

generateUaSecurityProtocolId

    function generateUaSecurityProtocolId(in octetstring p_cipherSuiteNumber) return octetstring

Declared in group functions.pskDerivation
The Ua security protocol identifier is a string of five octets. The first octet denotes the organization which specifies the Ua security protocol. The four remaining octets denote a specific security protocol within the responsibility of the organization. The following values for organizations are assigned: "0x01" 3GPP "0x02" 3GPP2 "0x03" Open Mobile Alliance "0x04" GSMA ( 0x01,0x00,0x01,yy,zz ) Ua security protocol for "Shared key-based UE authentication with certificatebased NAF authentication", according to TS 33.222 , or "Shared key-based mutual authentication between UE and NAF", according to TS 33.222. Here, "yy,zz" is the protection mechanism CipherSuite code according to the defined values for TLS CipherSuites in TLS V1.0 and PSK Ciphersuites for TLS.
Returns: octetstring -
Parameters:

- p_cipherSuiteNumber -

© Copyright Testing Technologies IST GmbH 2012