COMMENT

This file is the PoC Application Characteristics file for PoC V2.0.

FILE INFORMATION

OMA Permanent Document
   File: OMA-SUP-AC_ap0006_POC-V2_0-20080507-C.txt
   Type: Text

Public Reachable Information
   Path: http://www.openmobilealliance.org/tech/omna/omna-dm_ac.htm
   Name: ac_ap0006_poc-v2_0.txt


NORMATIVE INFORMATION

Information about this file can be found in PoC Control Plane V2.0 specification 
(OMA-TS-PoC_ControlPlane-V2_0) available at http://www.openmobilealliance.org/

Send comments to technical-comments@mail.openmobilealliance.org

LEGAL DISCLAIMER

Use of this document is subject to all of the terms and conditions
of the Use Agreement located at
	http://www.openmobilealliance.org/UseAgreement.html

You may use this document or any part of the document for internal
or educational purposes only, provided you do not modify, edit or
take out of context the information in this document in any manner.
Information contained in this document may be used, at your sole
risk, for any purposes.

You may not use this document in any other manner without the prior
written permission of the Open Mobile Alliance.  The Open Mobile
Alliance authorizes you to copy this document, provided that you
retain all copyright and other proprietary notices contained in the
original materials on any copies of the materials and that you
comply strictly with these terms.  This copyright permission does
not constitute an endorsement of the products or services.  The
Open Mobile Alliance assumes no responsibility for errors or
omissions in this document.

Each Open Mobile Alliance member has agreed to use reasonable
endeavors to inform the Open Mobile Alliance in a timely manner of
Essential IPR as it becomes aware that the Essential IPR is related
to the prepared or published specification.  However, the members
do not have an obligation to conduct IPR searches.  The declared
Essential IPR is publicly available to members and non-members of
the Open Mobile Alliance and may be found on the "OMA IPR
Declarations" list at http://www.openmobilealliance.org/ipr.html.
The Open Mobile Alliance has not conducted an independent IPR review
of this document and the information contained herein, and makes no
representations or warranties regarding third party IPR, including
without limitation patents, copyrights or trade secret rights.  This
document may contain inventions for which you must obtain licenses
from third parties before making, using or selling the inventions.
Defined terms above are set forth in the schedule to the Open Mobile
Alliance Application Form.

NO REPRESENTATIONS OR WARRANTIES (WHETHER EXPRESS OR IMPLIED) ARE
MADE BY THE OPEN MOBILE ALLIANCE OR ANY OPEN MOBILE ALLIANCE MEMBER
OR ITS AFFILIATES REGARDING ANY OF THE IPR’S REPRESENTED ON THE "OMA
IPR DECLARATIONS" LIST, INCLUDING, BUT NOT LIMITED TO THE ACCURACY,
COMPLETENESS, VALIDITY OR RELEVANCE OF THE INFORMATION OR WHETHER OR
NOT SUCH RIGHTS ARE ESSENTIAL OR NON-ESSENTIAL.

THE OPEN MOBILE ALLIANCE IS NOT LIABLE FOR AND HEREBY DISCLAIMS ANY
DIRECT, INDIRECT, PUNITIVE, SPECIAL, INCIDENTAL, CONSEQUENTIAL, OR
EXEMPLARY DAMAGES ARISING OUT OF OR IN CONNECTION WITH THE USE OF
DOCUMENTS AND THE INFORMATION CONTAINED IN THE DOCUMENTS.

?2007 Open Mobile Alliance Ltd.  All Rights Reserved.
Used with the permission of the Open Mobile Alliance Ltd. under the
terms set forth above.

IDENTIFYING INFORMATION
#######################
APPID: ap0006.
APPID type: OMNA.
Owner: OMA POC Working Group.
Contact: OMA POC Working Group.
Registration version: 2.0.
Registration timestamp: 2007-10-02.
Application description: Push to talk over Cellular (PoC). 
Application reference: 	
	Push to talk over Cellular (PoC) OMA PoC Enabler Release v2.0 specifications, 
	URL: http://www.openmobilealliance.org	


PARAMETERS
#####################
Characteristic/name: APPLICATION/APPID.
Status: Required.
Occurs: 1/1.
Default value: None.
Used values: ap0006.
Interpretation: To uniquely identify the PoC application. 
-------
Characteristic/name: APPLICATION/PROVIDER-ID.
Status: Optional.
Occurs: 0/1.
Default value: None.
Used values: N/A.
Interpretation: An identifier for the PoC application service access point.
-------
Characteristic/name: APPLICATION/APPREF.
Status: Required.
Occurs: 1/1.
Default value: None.
Used values: N/A.
Interpretation: This parameter specifies an unique reference for the PoC application characteristic that another application can refer to with matching TO-APPREF parameter.
-------
Characteristic/name: APPLICATION/TO-APPREF.
Status: Required.
Occurs: 1/*.
Default value: None.
Used values: N/A.
Interpretation: This parameter specifies the linkage between the PoC application characteristic and another application characteristic with a matching APPREF parameter.( e.g SIP-IP core).
-------
Characteristic/name: APPLICATION/NAME.
Status: Required.
Occurs: 1/1.
Default value: None.
Used values: N/A.
Interpretation: User displayable name for PoC application.
-------
Characteristic/name: APPLICATION/TO-NAPID.
Status: Required if direct use of Network Access Point supported.
Occurs: 0/*. 
Default value: None.
Used values: N/A.
Interpretation: N/A.
-------
APPLICATION-SPECIFIC PARAMETERS
###############################
Characteristic/name: APPLICATION/PRE-EST-SESN.
Status: Required.
Occurs: 1/1.
Default value: 0.
Used values: 0/1.
Interpretation: Indicates if the PoC Service Provider supports Pre-established Session or not.
-------
Characteristic/name: APPLICATION/SIMU-SESNS.
Status: Required.
Occurs: 1/1.
Default value: 0.
Used values: Integer.
Interpretation: Indicates the maximum number of Simultaneous PoC Sessions supported for the PoC Client
-------
Characteristic/name: APPLICATION/MAX-ADHOC-GROUP-SIZE.
Status: Required.
Occurs: 1/1.
Default value: N/A.
Used values:  Integer. 
Interpretation: Maximum number of Participants allowed in an Ad-hoc PoC Group Session.
-------
Characteristic/parameter: APPLICATION/CONF-FCTY-URI.
Status: Required.
Occurs: 1/1.
Default value: N/A.
Used values: A SIP URI.
Interpretation: Conference-factory-URI used in Ad-hoc PoC Group Session.
-------
Characteristic/parameter: APPLICATION/CONF-URI-TMPLT.
Status: Required.
Occurs: 1/1.
Default value: N/A.
Used values: A SIP URI.
Interpretation: The Conference-URI Template specifies the syntax of the Conference-URI.
-------
Characteristic/parameter: APPLICATION/EXPLODER-URI.
Status: Optional.
Occurs: 0/1.
Default value: N/A.
Used values: A SIP URI.
Interpretation: The Exploder-URI is used as a SIP URI in Request-URI of a SIP MESSAGE for a PoC Client to send a Group Advertisement.
-------
Characteristic/name: APPLICATION/TALK-BRST-REL-TMR.
Status: Required.
Occurs: 1/1.
Default value: N/A.
Used values: Integer.  
Interpretation: Indicates the value of the Talk Burst Release timer in the PoC Client in milliseconds.
-------
Characteristic/name: APPLICATION/TALK-BRST-REQ-TMR.
Status: Required.
Occurs: 1/1.
Default value: N/A.
Used values: Integer. 
Interpretation: Indicates the value of the Talk Burst Request timer in the PoC Client in milliseconds.
-------
Characteristic/name: APPLICATION/END-RTP-MEDIA-TMR.
Status: Optional.
Occurs: 0/1.
Default value: None.
Used values: Integer. 
Interpretation: Indicates the value of the End of RTP Media timer in the PoC Client in milliseconds.
-------
Characteristic/name: APPLICATION/PRES-SRV-CAP.
Status: Required if Presence is supported.
Occurs: 1/1.
Default value: None.
Used values: Binary. 
Interpretation: Indicates the Presence publishing capability of the PoC Server, the PoC status on behalf of a PoC Client. 
The flag must be given in sequence order according to the list of parameters as b1b2b3b4b5b6b7b8 (bit 8 is the lowest bit).
Where bit 1 is the flag of "Application-specific (PoC) Availability for sessions".
Bit 2 is the flag of  "Application-specific (PoC) Availability for alerts".
Bit3 the flag of "Session Participation". Bit 4-8 are for future extension.
-------
Characteristic/name: APPLICATION/VERSION-NUMBER.
Status: Optional.
Occurs: 0/1
Default value: N/A
Used values: Integer
Interpretation: indicates the release version of the Home PoC Server. If this parameter is not present, the PoC Client assumes the value indicates PoC 1.0. 
-------
Characteristic/name: APPLICATION/NW-POC-BOX-URI
Status: Optional
Occur: 0/1
Default value: N/A
Used values: A SIP URI
Interpretation: indicates a SIP URI of the NW PoC Box of the PoC Subscriber. 
-------
Characteristic/name: QOE-PROFILE/NAME
Status: Required.
Occurs: 1/*
Default value: None
Used values: BASIC, PREMIUM, PROFESSIONAL, OFF-GOV-USE
Interpretation: Indicates the name of the QoE Profile provisioned to the PoC Client.
------
Characteristic/name: QOE-PROFILE/MEDIA-TYPE/NAME
Status: Required.
Occurs: 1/*
Default value: None
Used values: AUDIO, VIDEO, SPEECH, DISCRETE
Interpretation: Indicates the Media Type that may be used by the PoC Client in a PoC Session.
------
Characteristic/name: QOE-PROFILE/MEDIA-TYPE/To-NAPID
Status: Required.
Occurs: 1/*
Default value: None
Used values: N/A
Interpretation: refers to a network access point with a matching NAPID parameter. 
-------
Characteristic/name: INCLUDED-MEDIA-CONTENT-SIZE.
Status: Optional.
Occurs: 0/1.
Default value: None.
Used values: Integer. 
Interpretation: Indicates the maximum total size in bytes of all the media contents included in the request.
-------
Characteristic/name: INCLUDED-TEXT-CONTENT-SIZE.
Status: Optional.
Occurs: 0/1.
Default value: None.
Used values: Integer. 
Interpretation: Indicates the max size of the text content included in the request in bytes.
--------

PARAMETER VALUES
################
Characteristic/name/parameter: QOE-PROFILE/NAME/BASIC
Status: Required.
Interpretation: Basic QoE Profile according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/NAME/PREMIUM
Status: Required.
Interpretation: Premium QoE Profile according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/NAME/PROFESSIONAL
Status: Required.
Interpretation: Professional QoE Profile according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/NAME/OFF-GOV-USE
Status: Optional.
Interpretation: Official Government Use QoE Profile according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/MEDIA-TYPE/NAME/AUDIO
Status: Required
Interpretation: Audio Media Type according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/MEDIA-TYPE/NAME/VIDEO
Status: Required
Interpretation: Video Media Type according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/MEDIA-TYPE/NAME/SPEECH
Status: Required
Interpretation: PoC Speech Media Type according to PoC Control Plane V2.0 specification.
--------
Characteristic/name/parameter: QOE-PROFILE/MEDIA-TYPE/NAME/DISCRETE
Status: Required
Interpretation: Discrete Media Type according to PoC Control Plane V2.0 specification.
--------

EXAMPLE 
#######
<characteristic type="APPLICATION">
  <parm name="APPID" value="ap0006"/>
  <parm name="PROVIDER-ID" value="Best"/>
  <parm name="APPREF" value="PoC"/>
  <parm name="TO-APPREF" value="SIP-IP-CORE"/>
  <parm name="NAME" value="PoC Service"/>
  <parm name="TO-NAPID" value="IMS-NAP"/>
  <parm name="PRE-EST-SESN" value="0"/>
  <parm name="SIMU-SESNS" value="0"/>
  <parm name="MAX_ADHOC_GROUP_SIZE" value="20"/>
  <parm name="CONF-FCTY-URI" value="sip:poc.Con-factory@example.com"/>
  <parm name="CONF-URI-TMPLT" value="sip:id@example.com"/>
  <parm name="EXPLODER-URI" value="sip:list-service@example.com"/>
  <parm name="TALK-BRST-REQ-TMR" value="2000"/>
  <parm name="TALK-BRST-REL-TMR" value="2000"/>
  <parm name="END-RTP-MEDIA-TMR" value="4000"/>
  <parm name="PRES-SRV-CAP" value="11100000"/>
  <parm name="VERSION-NUMBER" value="2"/>
  <parm name="NW-POC-BOX-URI" value="sip:nw-poc-box_id@example.com"/>
  <characteristic type="QOE-PROFILE">
    <parm name="NAME" value="PREMIUM"/>
    <characteristic type="MEDIA-TYPE">
      <parm name="NAME" value="AUDIO"/>
      <parm name="TO-NAPID" value="NAP1"/>
    </characteristic>
    <characteristic type="MEDIA-TYPE">
      <parm name="NAME" value="DISCRETE"/>
      <parm name="TO-NAPID" value="NAP3"/>
    </characteristic>
  </characteristic>
  <characteristic type="QOE-PROFILE">
    <parm name="NAME" value="BASIC"/>
    <characteristic type="MEDIA-TYPE">
      <parm name="NAME" value="AUDIO"/>
      <parm name="TO-NAPID" value="NAP2"/>
    </characteristic>
    <characteristic type="MEDIA-TYPE">
      <parm name="NAME" value="DISCRETE"/>
      <parm name="TO-NAPID" value="NAP3"/>
    </characteristic>
  </characteristic>
  <parm name="INCLUDED-MEDIA-CONTENT-SIZE" value="20000"/>
  <parm name="INCLUDED-TEXT-CONTENT-SIZE" value="40"/>
</characteristic>

###END###
