OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module MAP_SS_Code_V10

Import Declarations:

- ASNAUX
  all

Data Types Summary
SS_Code |

Constants Summary
allSS |
allLineIdentificationSS |
clip |
clir |
colp |
colr |
mci |
allNameIdentificationSS |
cnap |
allForwardingSS |
cfu |
allCondForwardingSS |
cfb |
cfnry |
cfnrc |
cd |
allCallOfferingSS |
ect |
mah |
allCallCompletionSS |
cw |
hold |
ccbs_A |
ccbs_B |
mc |
allMultiPartySS |
multiPTY |
allCommunityOfInterest_SS |
cug |
allChargingSS |
aoci |
aocc |
allAdditionalInfoTransferSS |
uus1 |
uus2 |
uus3 |
allBarringSS |
barringOfOutgoingCalls |
baoc |
boic |
boicExHC |
barringOfIncomingCalls |
baic |
bicRoam |
allPLMN_specificSS |
plmn_specificSS_1 |
plmn_specificSS_2 |
plmn_specificSS_3 |
plmn_specificSS_4 |
plmn_specificSS_5 |
plmn_specificSS_6 |
plmn_specificSS_7 |
plmn_specificSS_8 |
plmn_specificSS_9 |
plmn_specificSS_A |
plmn_specificSS_B |
plmn_specificSS_C |
plmn_specificSS_D |
plmn_specificSS_E |
plmn_specificSS_F |
allCallPrioritySS |
emlpp |
allLCSPrivacyException |
universal_ |
callSessionRelated |
callSessionUnrelated |
plmnoperator |
serviceType |
allMOLR_SS |
basicSelfLocation |
autonomousSelfLocation |
transferToThirdParty |

## Details

SS_Code

    SS-Code ::= OCTET STRING (SIZE (1))
         -- This type is used to represent the code identifying a single
         -- supplementary service, a group of supplementary services, or
         -- all supplementary services. The services and abbreviations
         -- used are defined in TS 3GPP TS 22.004 [5]. The internal structure is
         -- defined as follows:
         --
         -- bits 87654321: group (bits 8765), and specific service
         -- (bits 4321)
    allSS

allSS

    const SS_Code allSS                                     SS-Code ::= '00000000'B
         -- reserved for possible future use
         -- all SS
    allLineIdentificationSS

allLineIdentificationSS

    const SS_Code allLineIdentificationSS                   SS-Code ::= '00010000'B
         -- reserved for possible future use
         -- all line identification SS
    clip

clip

    const SS_Code clip                                      SS-Code ::= '00010001'B
         -- calling line identification presentation
    clir

clir

    const SS_Code clir                                      SS-Code ::= '00010010'B
         -- calling line identification restriction
    colp

colp

    const SS_Code colp                                      SS-Code ::= '00010011'B
         -- connected line identification presentation
    colr

colr

    const SS_Code colr                                      SS-Code ::= '00010100'B
         -- connected line identification restriction
    mci

mci

    const SS_Code mci                                       SS-Code ::= '00010101'B
         -- reserved for possible future use
         -- malicious call identification
    allNameIdentificationSS

allNameIdentificationSS

    const SS_Code allNameIdentificationSS                   SS-Code ::= '00011000'B
         -- all name identification SS
    cnap

cnap

    const SS_Code cnap                                      SS-Code ::= '00011001'B
         -- calling name presentation
         -- SS-Codes '00011010'B to '00011111'B are reserved for future
         -- NameIdentification Supplementary Service use.
    allForwardingSS

allForwardingSS

    const SS_Code allForwardingSS                           SS-Code ::= '00100000'B
         -- all forwarding SS
    cfu

cfu

    const SS_Code cfu                                       SS-Code ::= '00100001'B
         -- call forwarding unconditional
    allCondForwardingSS

allCondForwardingSS

    const SS_Code allCondForwardingSS                       SS-Code ::= '00101000'B
         -- all conditional forwarding SS
    cfb

cfb

    const SS_Code cfb                                       SS-Code ::= '00101001'B
         -- call forwarding on mobile subscriber busy
    cfnry

cfnry

    const SS_Code cfnry                                     SS-Code ::= '00101010'B
         -- call forwarding on no reply
    cfnrc

cfnrc

    const SS_Code cfnrc                                     SS-Code ::= '00101011'B
         -- call forwarding on mobile subscriber not reachable
    cd

cd

    const SS_Code cd                                        SS-Code ::= '00100100'B
         -- call deflection
    allCallOfferingSS

allCallOfferingSS

    const SS_Code allCallOfferingSS                         SS-Code ::= '00110000'B
         -- reserved for possible future use
         -- all call offering SS includes also all forwarding SS
    ect

ect

    const SS_Code ect                                       SS-Code ::= '00110001'B
              -- explicit call transfer
    mah

mah

    const SS_Code mah                                       SS-Code ::= '00110010'B
         -- reserved for possible future use
         -- mobile access hunting
    allCallCompletionSS

allCallCompletionSS

    const SS_Code allCallCompletionSS                       SS-Code ::= '01000000'B
         -- reserved for possible future use
         -- all Call completion SS
    cw

cw

    const SS_Code cw                                        SS-Code ::= '01000001'B
         -- call waiting
    hold

hold

    const SS_Code hold                                      SS-Code ::= '01000010'B
         -- call hold
    ccbs-A

ccbs_A

    const SS_Code ccbs-A                                    SS-Code ::= '01000011'B
         -- completion of call to busy subscribers, originating side
         -- this SS-Code is used only in InsertSubscriberData, DeleteSubscriberData
         -- and InterrogateSS
    ccbs-B

ccbs_B

    const SS_Code ccbs-B                                    SS-Code ::= '01000100'B
         -- completion of call to busy subscribers, destination side
         -- this SS-Code is used only in InsertSubscriberData and DeleteSubscriberData
    mc

mc

    const SS_Code mc                                        SS-Code ::= '01000101'B
         -- multicall
    allMultiPartySS

allMultiPartySS

    const SS_Code allMultiPartySS                           SS-Code ::= '01010000'B
         -- reserved for possible future use
         -- all multiparty SS
    multiPTY

multiPTY

    const SS_Code multiPTY                                  SS-Code ::= '01010001'B
         -- multiparty
    allCommunityOfInterest-SS

allCommunityOfInterest_SS

    const SS_Code allCommunityOfInterest-SS                 SS-Code ::= '01100000'B
         -- reserved for possible future use
         -- all community of interest SS
    cug

cug

    const SS_Code cug                                       SS-Code ::= '01100001'B
         -- closed user group
    allChargingSS

allChargingSS

    const SS_Code allChargingSS                             SS-Code ::= '01110000'B
         -- reserved for possible future use
         -- all charging SS
    aoci

aoci

    const SS_Code aoci                                      SS-Code ::= '01110001'B
         -- advice of charge information
    aocc

aocc

    const SS_Code aocc                                      SS-Code ::= '01110010'B
         -- advice of charge charging
    allAdditionalInfoTransferSS

allAdditionalInfoTransferSS

    const SS_Code allAdditionalInfoTransferSS               SS-Code  ::= '10000000'B
         -- reserved for possible future use
         -- all additional information transfer SS
    uus1

uus1

    const SS_Code uus1                                      SS-Code  ::= '10000001'B
         -- UUS1 user-to-user signalling
    uus2

uus2

    const SS_Code uus2                                      SS-Code  ::= '10000010'B
         -- UUS2 user-to-user signalling
    uus3

uus3

    const SS_Code uus3                                      SS-Code  ::= '10000011'B
         -- UUS3 user-to-user signalling
    allBarringSS

allBarringSS

    const SS_Code allBarringSS                              SS-Code ::= '10010000'B
         -- all barring SS
    barringOfOutgoingCalls

barringOfOutgoingCalls

    const SS_Code barringOfOutgoingCalls                    SS-Code ::= '10010001'B
         -- barring of outgoing calls
    baoc

baoc

    const SS_Code baoc                                      SS-Code ::= '10010010'B
         -- barring of all outgoing calls
    boic

boic

    const SS_Code boic                                      SS-Code ::= '10010011'B
         -- barring of outgoing international calls
    boicExHC

boicExHC

    const SS_Code boicExHC                                  SS-Code ::= '10010100'B
         -- barring of outgoing international calls except those directed
         -- to the home PLMN Country
    barringOfIncomingCalls

barringOfIncomingCalls

    const SS_Code barringOfIncomingCalls                    SS-Code ::= '10011001'B
         -- barring of incoming calls
    baic

baic

    const SS_Code baic                                      SS-Code ::= '10011010'B
         -- barring of all incoming calls
    bicRoam

bicRoam

    const SS_Code bicRoam                                   SS-Code ::= '10011011'B
         -- barring of incoming calls when roaming outside home PLMN
         -- Country
    allPLMN-specificSS

allPLMN_specificSS

    const SS_Code allPLMN-specificSS                        SS-Code  ::= '11110000'B
    plmn-specificSS-1

plmn_specificSS_1

    const SS_Code plmn-specificSS-1                         SS-Code  ::= '11110001'B
    plmn-specificSS-2

plmn_specificSS_2

    const SS_Code plmn-specificSS-2                         SS-Code  ::= '11110010'B
    plmn-specificSS-3

plmn_specificSS_3

    const SS_Code plmn-specificSS-3                         SS-Code  ::= '11110011'B
    plmn-specificSS-4

plmn_specificSS_4

    const SS_Code plmn-specificSS-4                         SS-Code  ::= '11110100'B
    plmn-specificSS-5

plmn_specificSS_5

    const SS_Code plmn-specificSS-5                         SS-Code  ::= '11110101'B
    plmn-specificSS-6

plmn_specificSS_6

    const SS_Code plmn-specificSS-6                         SS-Code  ::= '11110110'B
    plmn-specificSS-7

plmn_specificSS_7

    const SS_Code plmn-specificSS-7                         SS-Code  ::= '11110111'B
    plmn-specificSS-8

plmn_specificSS_8

    const SS_Code plmn-specificSS-8                         SS-Code  ::= '11111000'B
    plmn-specificSS-9

plmn_specificSS_9

    const SS_Code plmn-specificSS-9                         SS-Code  ::= '11111001'B
    plmn-specificSS-A

plmn_specificSS_A

    const SS_Code plmn-specificSS-A                         SS-Code  ::= '11111010'B
    plmn-specificSS-B

plmn_specificSS_B

    const SS_Code plmn-specificSS-B                         SS-Code  ::= '11111011'B
    plmn-specificSS-C

plmn_specificSS_C

    const SS_Code plmn-specificSS-C                         SS-Code  ::= '11111100'B
    plmn-specificSS-D

plmn_specificSS_D

    const SS_Code plmn-specificSS-D                         SS-Code  ::= '11111101'B
    plmn-specificSS-E

plmn_specificSS_E

    const SS_Code plmn-specificSS-E                         SS-Code  ::= '11111110'B
    plmn-specificSS-F

plmn_specificSS_F

    const SS_Code plmn-specificSS-F                         SS-Code  ::= '11111111'B
    allCallPrioritySS

allCallPrioritySS

    const SS_Code allCallPrioritySS                         SS-Code ::= '10100000'B
         -- reserved for possible future use
         -- all call priority SS
    emlpp

emlpp

    const SS_Code emlpp                                     SS-Code ::= '10100001'B
         -- enhanced Multilevel Precedence Pre-emption (EMLPP) service
    allLCSPrivacyException

allLCSPrivacyException

    const SS_Code allLCSPrivacyException                    SS-Code ::= '10110000'B
         -- all LCS Privacy Exception Classes
    universal

universal_

    const SS_Code universal                                 SS-Code ::= '10110001'B
         -- allow location by any LCS client
    callSessionRelated

callSessionRelated

    const SS_Code callSessionRelated                        SS-Code ::= '10110010'B
         -- allow location by any value added LCS client to which a call/session
         -- is established from the target MS
    callSessionUnrelated

callSessionUnrelated

    const SS_Code callSessionUnrelated                      SS-Code ::= '10110011'B
         -- allow location by designated external value added LCS clients
    plmnoperator

plmnoperator

    const SS_Code plmnoperator                              SS-Code ::= '10110100'B
         -- allow location by designated PLMN operator LCS clients
    serviceType

serviceType

    const SS_Code serviceType                               SS-Code ::= '10110101'B
         -- allow location by LCS clients of a designated LCS service type
    allMOLR-SS

allMOLR_SS

    const SS_Code allMOLR-SS                                SS-Code ::= '11000000'B
         -- all Mobile Originating Location Request Classes
    basicSelfLocation

basicSelfLocation

    const SS_Code basicSelfLocation                         SS-Code ::= '11000001'B
         -- allow an MS to request its own location
    autonomousSelfLocation

autonomousSelfLocation

    const SS_Code autonomousSelfLocation                    SS-Code ::= '11000010'B
         -- allow an MS to perform self location without interaction
         -- with the PLMN for a predetermined period of time
    transferToThirdParty

transferToThirdParty

    const SS_Code transferToThirdParty                      SS-Code ::= '11000011'B
         -- allow an MS to request transfer of its location to another LCS client
    END

© Copyright Testing Technologies IST GmbH 2012