OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Group suplIxitItemsGroup.SET

Declared in module SUPL_V2_Parameters

Modulepars Summary
ixit_timer_UT7 | (integer) value of Timer UT7, default = 10s
ixit_timer_UT8 | (integer) value of Timer UT8, default = 10s
ixit_SUPL_MAJ_VERSION | (integer 0-255) Current SUPL major version supported by this test suite
ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX | (integer 0-255) SUPL servind version number higher than maximally supported by SET
ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX | (integer 0-255) SUPL min version number higher than maximally supported by SET
ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX | (integer 0-255) SUPL servind version lower than the maximum value supported by the SET
ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX | (integer 0-255) SUPL min version lower than the maximum value supported by the SET
ixit_SET_MAJ_VERSION | (integer 0-255) The maj version number supported by the SET
ixit_SET_SERVIND_VERSION | (integer 0-255) A server ind version number higher than the one supported by the SUT
ixit_SET_SERVIND_VERSION_V1 | (integer 0-255) A server ind version number higher than the one supported by the SUT (if SUPL V1 selected)
ixit_SET_MIN_VERSION | (integer 0-255) SUPL min version number supported by the SET
ixit_SET_MIN_VERSION_V1 | (integer 0-255) SUPL min version number supported by the SET (if SUPL V1 selected)
ixit_SET_REPORTING_CAP | (ReportingCap) Reporting Capabilities supported by the SET
ixit_SET_SERVICE_SUPPORTED | (serviceSupported) service supported by the SET
ixit_SET_EVENTTRIGGER_CAP | (EventTriggerCap)Event Trigger Capabilities supported by the SET

## Details

ixit_timer_UT7

    integer ixit_timer_UT7 := 10

Declared in group suplIxitItemsGroup.SET
(integer) value of Timer UT7, default = 10s

ixit_timer_UT8

    integer ixit_timer_UT8 := 10

Declared in group suplIxitItemsGroup.SET
(integer) value of Timer UT8, default = 10s

ixit_SUPL_MAJ_VERSION

    _0Version ixit_SUPL_MAJ_VERSION := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) Current SUPL major version supported by this test suite

ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX

    _0Version1 ixit_SET_SERVIND_VERSION_HIGHER_THAN_SET_MAX := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL servind version number higher than maximally supported by SET

ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX

    _0Version0 ixit_SET_MIN_VERSION_HIGHER_THAN_SET_MAX := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number higher than maximally supported by SET

ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX

    _0Version1 ixit_SET_SERVIND_VERSION_LOWER_THAN_SET_MAX := 1

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL servind version lower than the maximum value supported by the SET

ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX

    _0Version0 ixit_SET_MIN_VERSION_LOWER_THAN_SET_MAX := 1

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version lower than the maximum value supported by the SET

ixit_SET_MAJ_VERSION

    _0Version ixit_SET_MAJ_VERSION := 2

Declared in group suplIxitItemsGroup.SET
(integer 0-255) The maj version number supported by the SET

ixit_SET_SERVIND_VERSION

    _0Version1 ixit_SET_SERVIND_VERSION := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) A server ind version number higher than the one supported by the SUT

ixit_SET_SERVIND_VERSION_V1

    _0Version1 ixit_SET_SERVIND_VERSION_V1 := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) A server ind version number higher than the one supported by the SUT (if SUPL V1 selected)

ixit_SET_MIN_VERSION

    _0Version1 ixit_SET_MIN_VERSION := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number supported by the SET

ixit_SET_MIN_VERSION_V1

    _0Version1 ixit_SET_MIN_VERSION_V1 := 0

Declared in group suplIxitItemsGroup.SET
(integer 0-255) SUPL min version number supported by the SET (if SUPL V1 selected)

ixit_SET_REPORTING_CAP

    ReportingCap ixit_SET_REPORTING_CAP := {
    minInt := 1,
    maxInt := 1,
    repMode := {
    realtime := true,
    quasirealtime := true,
    batch := true
    },
    batchRepCap := {
    report_position := true,
    report_measurements := true,
    max_num_positions := 1,
    max_num_measurements := 1
    }
    }

Declared in group suplIxitItemsGroup.SET
(ReportingCap) Reporting Capabilities supported by the SET

ixit_SET_SERVICE_SUPPORTED

    ServicesSupported ixit_SET_SERVICE_SUPPORTED := {
    periodicTrigger := true,
    areaEventTrigger := true
    }

Declared in group suplIxitItemsGroup.SET
(serviceSupported) service supported by the SET

ixit_SET_EVENTTRIGGER_CAP

    EventTriggerCapabilities ixit_SET_EVENTTRIGGER_CAP := {
       geoAreaShapesSupported := {
       ellipticalArea := false,
       polygonArea := false
       },
       maxNumGeoAreaSupported := 3,
       maxAreaIdListSupported := 6,
       maxAreaIdSupportedPerList := 256
       }

Declared in group suplIxitItemsGroup.SET
(EventTriggerCap)Event Trigger Capabilities supported by the SET

© Copyright Testing Technologies IST GmbH 2012