OVERVIEW INDEX DEPRECATED HELP CORRESPONDENCES | provided by TTworkbench

Modulepars Data Types Component Types Port Types Constants Templates Signatures Functions Altsteps Test cases

# Module MAP_BS_Code_V10

Import Declarations:

- ASNAUX
  all

Data Types Summary
BearerServiceCode |
Ext_BearerServiceCode |

Constants Summary
allBearerServices |
allDataCDA_Services |
dataCDA_300bps |
dataCDA_1200bps |
dataCDA_1200_75bps |
dataCDA_2400bps |
dataCDA_4800bps |
dataCDA_9600bps |
general_dataCDA |
allDataCDS_Services |
dataCDS_1200bps |
dataCDS_2400bps |
dataCDS_4800bps |
dataCDS_9600bps |
general_dataCDS |
allPadAccessCA_Services |
padAccessCA_300bps |
padAccessCA_1200bps |
padAccessCA_1200_75bps |
padAccessCA_2400bps |
padAccessCA_4800bps |
padAccessCA_9600bps |
general_padAccessCA |
allDataPDS_Services |
dataPDS_2400bps |
dataPDS_4800bps |
dataPDS_9600bps |
general_dataPDS |
allAlternateSpeech_DataCDA |
allAlternateSpeech_DataCDS |
allSpeechFollowedByDataCDA |
allSpeechFollowedByDataCDS |
allDataCircuitAsynchronous |
allAsynchronousServices |
allDataCircuitSynchronous |
allSynchronousServices |
allPLMN_specificBS |
plmn_specificBS_1 |
plmn_specificBS_2 |
plmn_specificBS_3 |
plmn_specificBS_4 |
plmn_specificBS_5 |
plmn_specificBS_6 |
plmn_specificBS_7 |
plmn_specificBS_8 |
plmn_specificBS_9 |
plmn_specificBS_A |
plmn_specificBS_B |
plmn_specificBS_C |
plmn_specificBS_D |
plmn_specificBS_E |
plmn_specificBS_F |

## Details

BearerServiceCode

    BearerServiceCode ::= OCTET STRING (SIZE (1))
          -- This type is used to represent the code identifying a single
          -- bearer service, a group of bearer services, or all bearer
          -- services. The services are defined in TS 3GPP TS 22.002 [3].
          -- The internal structure is defined as follows:
          --
          -- plmn-specific bearer services:
          -- bits 87654321: defined by the HPLMN operator
          -- rest of bearer services:
          -- bit 8: 0 (unused)
          -- bits 7654321: group (bits 7654), and rate, if applicable
          -- (bits 321)
    Ext-BearerServiceCode

Ext_BearerServiceCode

    Ext-BearerServiceCode ::= OCTET STRING (SIZE (1..5))
         -- This type is used to represent the code identifying a single
         -- bearer service, a group of bearer services, or all bearer
         -- services. The services are defined in TS 3GPP TS 22.002 [3].
         -- The internal structure is defined as follows:
         --
         -- OCTET 1:
         -- plmn-specific bearer services:
         -- bits 87654321: defined by the HPLMN operator
         --
         -- rest of bearer services:
         -- bit 8: 0 (unused)
         -- bits 7654321: group (bits 7654), and rate, if applicable
         -- (bits 321)
         -- OCTETS 2-5: reserved for future use. If received the
        -- Ext-TeleserviceCode shall be
         -- treated according to the exception handling defined for the
         -- operation that uses this type.
         -- Ext-BearerServiceCode includes all values defined for BearerServiceCode.
    allBearerServices

allBearerServices

    const BearerServiceCode allBearerServices                         BearerServiceCode ::= '00000000'B
    allDataCDA-Services

allDataCDA_Services

    const BearerServiceCode allDataCDA-Services                       BearerServiceCode ::= '00010000'B
    dataCDA-300bps

dataCDA_300bps

    const BearerServiceCode dataCDA-300bps                            BearerServiceCode ::= '00010001'B
    dataCDA-1200bps

dataCDA_1200bps

    const BearerServiceCode dataCDA-1200bps                           BearerServiceCode ::= '00010010'B
    dataCDA-1200-75bps

dataCDA_1200_75bps

    const BearerServiceCode dataCDA-1200-75bps                        BearerServiceCode ::= '00010011'B
    dataCDA-2400bps

dataCDA_2400bps

    const BearerServiceCode dataCDA-2400bps                           BearerServiceCode ::= '00010100'B
    dataCDA-4800bps

dataCDA_4800bps

    const BearerServiceCode dataCDA-4800bps                           BearerServiceCode ::= '00010101'B
    dataCDA-9600bps

dataCDA_9600bps

    const BearerServiceCode dataCDA-9600bps                           BearerServiceCode ::= '00010110'B
    general-dataCDA

general_dataCDA

    const BearerServiceCode general-dataCDA                           BearerServiceCode ::= '00010111'B
    allDataCDS-Services

allDataCDS_Services

    const BearerServiceCode allDataCDS-Services                       BearerServiceCode ::= '00011000'B
    dataCDS-1200bps

dataCDS_1200bps

    const BearerServiceCode dataCDS-1200bps                           BearerServiceCode ::= '00011010'B
    dataCDS-2400bps

dataCDS_2400bps

    const BearerServiceCode dataCDS-2400bps                           BearerServiceCode ::= '00011100'B
    dataCDS-4800bps

dataCDS_4800bps

    const BearerServiceCode dataCDS-4800bps                           BearerServiceCode ::= '00011101'B
    dataCDS-9600bps

dataCDS_9600bps

    const BearerServiceCode dataCDS-9600bps                           BearerServiceCode ::= '00011110'B
    general-dataCDS

general_dataCDS

    const BearerServiceCode general-dataCDS                           BearerServiceCode ::= '00011111'B
    allPadAccessCA-Services

allPadAccessCA_Services

    const BearerServiceCode allPadAccessCA-Services                   BearerServiceCode ::= '00100000'B
    padAccessCA-300bps

padAccessCA_300bps

    const BearerServiceCode padAccessCA-300bps                        BearerServiceCode ::= '00100001'B
    padAccessCA-1200bps

padAccessCA_1200bps

    const BearerServiceCode padAccessCA-1200bps                       BearerServiceCode ::= '00100010'B
    padAccessCA-1200-75bps

padAccessCA_1200_75bps

    const BearerServiceCode padAccessCA-1200-75bps                    BearerServiceCode ::= '00100011'B
    padAccessCA-2400bps

padAccessCA_2400bps

    const BearerServiceCode padAccessCA-2400bps                       BearerServiceCode ::= '00100100'B
    padAccessCA-4800bps

padAccessCA_4800bps

    const BearerServiceCode padAccessCA-4800bps                       BearerServiceCode ::= '00100101'B
    padAccessCA-9600bps

padAccessCA_9600bps

    const BearerServiceCode padAccessCA-9600bps                       BearerServiceCode ::= '00100110'B
    general-padAccessCA

general_padAccessCA

    const BearerServiceCode general-padAccessCA                       BearerServiceCode ::= '00100111'B
    allDataPDS-Services

allDataPDS_Services

    const BearerServiceCode allDataPDS-Services                       BearerServiceCode ::= '00101000'B
    dataPDS-2400bps

dataPDS_2400bps

    const BearerServiceCode dataPDS-2400bps                           BearerServiceCode ::= '00101100'B
    dataPDS-4800bps

dataPDS_4800bps

    const BearerServiceCode dataPDS-4800bps                           BearerServiceCode ::= '00101101'B
    dataPDS-9600bps

dataPDS_9600bps

    const BearerServiceCode dataPDS-9600bps                           BearerServiceCode ::= '00101110'B
    general-dataPDS

general_dataPDS

    const BearerServiceCode general-dataPDS                           BearerServiceCode ::= '00101111'B
    allAlternateSpeech-DataCDA

allAlternateSpeech_DataCDA

    const BearerServiceCode allAlternateSpeech-DataCDA                BearerServiceCode ::= '00110000'B
    allAlternateSpeech-DataCDS

allAlternateSpeech_DataCDS

    const BearerServiceCode allAlternateSpeech-DataCDS                BearerServiceCode ::= '00111000'B
    allSpeechFollowedByDataCDA

allSpeechFollowedByDataCDA

    const BearerServiceCode allSpeechFollowedByDataCDA                BearerServiceCode ::= '01000000'B
    allSpeechFollowedByDataCDS

allSpeechFollowedByDataCDS

    const BearerServiceCode allSpeechFollowedByDataCDS                BearerServiceCode ::= '01001000'B
    -- The following non-hierarchical Compound Bearer Service
    -- Groups are defined in TS 3GPP TS 22.030:
    allDataCircuitAsynchronous

allDataCircuitAsynchronous

    const BearerServiceCode allDataCircuitAsynchronous                BearerServiceCode ::= '01010000'B
         -- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA" and
         -- "allSpeechFollowedByDataCDA"
    allAsynchronousServices

allAsynchronousServices

    const BearerServiceCode allAsynchronousServices                   BearerServiceCode ::= '01100000'B
         -- covers "allDataCDA-Services", "allAlternateSpeech-DataCDA",
         -- "allSpeechFollowedByDataCDA" and "allPadAccessCDA-Services"
    allDataCircuitSynchronous

allDataCircuitSynchronous

    const BearerServiceCode allDataCircuitSynchronous                 BearerServiceCode ::= '01011000'B
         -- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS" and
         -- "allSpeechFollowedByDataCDS"
    allSynchronousServices

allSynchronousServices

    const BearerServiceCode allSynchronousServices                    BearerServiceCode ::= '01101000'B
         -- covers "allDataCDS-Services", "allAlternateSpeech-DataCDS",
         -- "allSpeechFollowedByDataCDS" and "allDataPDS-Services"
    --
    -- Compound Bearer Service Group Codes are only used in call
    -- independent supplementary service operations, i.e. they
    -- are not used in InsertSubscriberData or in
    -- DeleteSubscriberData messages.
    allPLMN-specificBS

allPLMN_specificBS

    const BearerServiceCode allPLMN-specificBS                        BearerServiceCode ::= '11010000'B
    plmn-specificBS-1

plmn_specificBS_1

    const BearerServiceCode plmn-specificBS-1                         BearerServiceCode ::= '11010001'B
    plmn-specificBS-2

plmn_specificBS_2

    const BearerServiceCode plmn-specificBS-2                         BearerServiceCode ::= '11010010'B
    plmn-specificBS-3

plmn_specificBS_3

    const BearerServiceCode plmn-specificBS-3                         BearerServiceCode ::= '11010011'B
    plmn-specificBS-4

plmn_specificBS_4

    const BearerServiceCode plmn-specificBS-4                         BearerServiceCode ::= '11010100'B
    plmn-specificBS-5

plmn_specificBS_5

    const BearerServiceCode plmn-specificBS-5                         BearerServiceCode ::= '11010101'B
    plmn-specificBS-6

plmn_specificBS_6

    const BearerServiceCode plmn-specificBS-6                         BearerServiceCode ::= '11010110'B
    plmn-specificBS-7

plmn_specificBS_7

    const BearerServiceCode plmn-specificBS-7                         BearerServiceCode ::= '11010111'B
    plmn-specificBS-8

plmn_specificBS_8

    const BearerServiceCode plmn-specificBS-8                         BearerServiceCode ::= '11011000'B
    plmn-specificBS-9

plmn_specificBS_9

    const BearerServiceCode plmn-specificBS-9                         BearerServiceCode ::= '11011001'B
    plmn-specificBS-A

plmn_specificBS_A

    const BearerServiceCode plmn-specificBS-A                         BearerServiceCode ::= '11011010'B
    plmn-specificBS-B

plmn_specificBS_B

    const BearerServiceCode plmn-specificBS-B                         BearerServiceCode ::= '11011011'B
    plmn-specificBS-C

plmn_specificBS_C

    const BearerServiceCode plmn-specificBS-C                         BearerServiceCode ::= '11011100'B
    plmn-specificBS-D

plmn_specificBS_D

    const BearerServiceCode plmn-specificBS-D                         BearerServiceCode ::= '11011101'B
    plmn-specificBS-E

plmn_specificBS_E

    const BearerServiceCode plmn-specificBS-E                         BearerServiceCode ::= '11011110'B
    plmn-specificBS-F

plmn_specificBS_F

    const BearerServiceCode plmn-specificBS-F                         BearerServiceCode ::= '11011111'B
    END

© Copyright Testing Technologies IST GmbH 2012